#!/bin/sh
#
# mRo x21 specific board defaults
#------------------------------------------------------------------------------


if [ $AUTOCNF = yes ]
then

	# to minimize cpu usage on older boards limit inner loop to 400 Hz
	param set IMU_GYRO_RATEMAX 400

fi
