#!/bin/sh
#
# Omnibus F4SD specific board sensors init
#------------------------------------------------------------------------------

adc start

if ! mpu6000 -R 12 -s start
then
	# some boards such as the Hobbywing XRotor F4 G2 use the ICM-20602
	icm20602 -R 6 start
	#mpu6000 -R 12 -T 20602 -s start
fi

# Possible external compasses
hmc5883 -X start

bmp280 start

