#!/bin/sh
#
# @name Plane SITL with camera
#

sh /etc/init.d-posix/1030_plane

if [ $AUTOCNF = yes ]
then
	# Camera trigger interface is MAVLink
	param set TRIG_INTERFACE 3
	# Distance trigger mode enabled
	param set TRIG_MODE 4
fi
