uint64 timestamp                   # time since system start (microseconds)
uint64 timestamp_sample            # the timestamp the data this control response is based on was sampled

uint8 NUM_ACTUATOR_SETPOINT = 16

float32[16] actuator
