Multirotor mixer for PX4FMU
===========================

This file defines a single mixer for a quadrotor with a wide configuration.  All controls are mixed 100%.

R: 4w

Gimbal / payload mixer for last two channels
-----------------------------------------------------

M: 1
S: 3 5  10000  10000      0 -10000  10000

M: 1
S: 3 6  10000  10000      0 -10000  10000
