#
# support for buttons on UAVCAN
# while a button is being pressed this message should be sent at 10Hz

uint8 BUTTON_SAFETY      = 1

uint8 button

# number of 0.1s units the button has been pressed for. If over 255
# then send 255
uint8 press_time
