#
# The following command will be executed on reset
# - wait for target halt
# - erase memory
# - flash content of file nuttx.bin into target-memory
# - shutdown openocd
#
# Based on file originally created by Martin Thomas
#

arm7_9 dcc_downloads enable
wait_halt
sleep 10
poll
flash probe 0

# STR710 erase all banks:
#flash erase 0 0 9
# STR710 erase first 4 banks (32kB)
flash erase 0 0 4

flash write 0 nuttx.bin 0x0
reset run
sleep 10
shutdown

