(module USB_Micro-B_10103594-0001LF placed (layer F.Cu) (tedit 58371F44)
  (descr "Micro USB Type B 10103594-0001LF")
  (tags "USB USB_B USB_micro USB_OTG")
  (attr smd)
  (fp_text reference P1 (at 0 -4.625) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.2)))
  )
  (fp_text value USB_OTG (at 0 4.75) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 2.65 3.11) (end -2.65 3.11) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.02 -2.82) (end 3.75 -2.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.02 -2.82) (end -4.02 -2.82) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.75 2.8) (end -3.75 2.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.75 2.8) (end -3.75 -2.2) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.75 -2.2) (end 3.75 -2.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.75 -2.2) (end 3.75 2.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.02 -2.82) (end -3.75 -2.2) (layer F.SilkS) (width 0.15))
  (pad 6 smd rect (at -1 -0.25 180) (size 1.25 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1 -0.25 180) (size 1.25 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 6 thru_hole oval (at -2.7 0 180) (size 1.4 2.5) (drill 0.9 (offset 0 -0.5)) (layers *.Cu *.Mask F.Paste))
  (pad 6 thru_hole oval (at 2.7 0 180) (size 1.4 2.5) (drill 0.9 (offset 0 -0.5)) (layers *.Cu *.Mask F.Paste))
  (pad 6 thru_hole circle (at -2.425 3.11 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask F.Paste))
  (pad 6 thru_hole circle (at 2.425 3.11 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask F.Paste))
  (pad 5 smd rect (at -1.3 2.875 180) (size 0.4 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -0.65 2.875 180) (size 0.4 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0 2.875 180) (size 0.4 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.65 2.875 180) (size 0.4 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 1.3 2.875 180) (size 0.4 1.75) (layers F.Cu F.Paste F.Mask))
)
