(module Pin_Header_Straight_1x06 (layer F.Cu) (tedit 593CB068)
  (descr "Through hole pin header")
  (tags "pin header")
  (fp_text reference P5 (at 0 -8.25) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value CONN_01X06 (at 0 8.25) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.27 -7.62) (end 1.27 -7.62) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.27 -7.62) (end 1.27 7.62) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.27 7.62) (end -1.27 7.62) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.27 7.62) (end -1.27 -7.62) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.27 -5.08) (end 1.27 -5.08) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole roundrect (at 0 -6.35) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS)(roundrect_rratio 0.1))
  (pad 2 thru_hole roundrect (at 0 -3.81) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS)(roundrect_rratio 0.25))
  (pad 3 thru_hole roundrect (at 0 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS)(roundrect_rratio 0.25))
  (pad 4 thru_hole roundrect (at 0 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS)(roundrect_rratio 0.25))
  (pad 5 thru_hole roundrect (at 0 3.81) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS)(roundrect_rratio 0.25))
  (pad 6 thru_hole roundrect (at 0 6.35) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS)(roundrect_rratio 0.25))
  (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
    (at (xyz 0 -0.25 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
