(module C_Radial_D6.5_L11_P2.5 (layer F.Cu) (tedit 5897A0BA)
  (descr "Radial Electrolytic Capacitor, Diameter 6.3mm x Length 11.2mm, Pitch 2.5mm")
  (tags "Electrolytic Capacitor")
  (fp_text reference C143 (at -3.212 -2.332) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 22µ (at 1.25 4.4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.25 1.5) (end 4.25 1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.25 1.5) (end -2.25 12.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.75 1.5) (end 3.75 12.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 4 1.75) (end 4 12.25) (layer F.SilkS) (width 0.5))
  (fp_line (start 2.25 -0.25) (end 2.25 1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.75 -0.25) (end 2.25 -0.25) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.75 1.5) (end 1.75 -0.25) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.25 -0.25) (end 0.25 1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.25 -0.25) (end 0.25 -0.25) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.25 0) (end -0.25 -0.25) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.25 1.5) (end -0.25 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.25 12.5) (end 4.25 1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.25 12.5) (end 4.25 12.5) (layer F.SilkS) (width 0.15))
  (pad 2 thru_hole circle (at 2 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole roundrect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)(roundrect_rratio 0.25))
  (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.wrl
    (at (xyz 0 -0.03937007874015748 0.09842519685039371))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
