(module SOLDER_JUMPER (layer F.Cu) (tedit 5831C1B1)
  (fp_text reference JP4 (at 0 2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Jumper_NO_Small (at 0 -2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.75 0) (end -0.2 0) (layer F.Mask) (width 0.45))
  (fp_line (start 0.75 0) (end 0.2 0) (layer F.Cu) (width 0.15))
  (fp_line (start -0.75 0) (end -0.2 0) (layer F.Cu) (width 0.15))
  (fp_line (start 0.2 0) (end 0.75 0) (layer F.Mask) (width 0.45))
  (pad 1 smd rect (at -0.75 0) (size 1 1.5) (layers F.Cu F.Mask))
  (pad 2 smd rect (at 0.75 0) (size 1 1.5) (layers F.Cu F.Mask))
)
