(module C_0603 (layer F.Cu) (tedit 594E9747)
  (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
  (tags "capacitor 0603")
  (attr smd)
  (fp_text reference C22 (at -3.248 0.064) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.2)))
  )
  (fp_text value 100n (at 0 1.4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0.5 -0.4) (end 0.5 0.4) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.5 -0.4) (end -0.5 0.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.3 -0.6) (end 1.3 -0.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.3 0.6) (end 1.3 0.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.3 -0.6) (end -1.3 0.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.3 -0.6) (end 1.3 0.6) (layer F.CrtYd) (width 0.05))
  (pad 2 smd roundrect (at 0.75 0) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 1 smd roundrect (at -0.75 0) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (model Capacitors_SMD.3dshapes/C_0603.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
