(module LQFP-100_14x14mm_Pitch0.5mm (layer F.Cu) (tedit 57D5FC61)
  (descr "LQFP100: plastic low profile quad flat package; 100 leads; body 14 x 14 x 1.4 mm (see NXP sot407-1_po.pdf and sot407-1_fr.pdf)")
  (tags "QFP 0.5")
  (attr smd)
  (fp_text reference U26 (at 0 -9.65) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value STM32F405VG (at 0 9.65) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -8.9 -8.9) (end -8.9 8.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start 8.9 -8.9) (end 8.9 8.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8.9 -8.9) (end 8.9 -8.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8.9 8.9) (end 8.9 8.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start -7.125 -7.125) (end -7.125 -6.365) (layer F.SilkS) (width 0.15))
  (fp_line (start 7.125 -7.125) (end 7.125 -6.365) (layer F.SilkS) (width 0.15))
  (fp_line (start 7.125 7.125) (end 7.125 6.365) (layer F.SilkS) (width 0.15))
  (fp_line (start -7.125 7.125) (end -7.125 6.365) (layer F.SilkS) (width 0.15))
  (fp_line (start -7.125 -7.125) (end -6.365 -7.125) (layer F.SilkS) (width 0.15))
  (fp_line (start -7.125 7.125) (end -6.365 7.125) (layer F.SilkS) (width 0.15))
  (fp_line (start 7.125 7.125) (end 6.365 7.125) (layer F.SilkS) (width 0.15))
  (fp_line (start 7.125 -7.125) (end 6.365 -7.125) (layer F.SilkS) (width 0.15))
  (fp_line (start -7.125 -6.365) (end -8.65 -6.365) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -7.75 -6) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -7.75 -5.5) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -7.75 -5) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -7.75 -4.5) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -7.75 -4) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -7.75 -3.5) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -7.75 -3) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -7.75 -2.5) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -7.75 -2) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -7.75 -1.5) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -7.75 -1) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -7.75 -0.5) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -7.75 0) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at -7.75 0.5) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -7.75 1) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at -7.75 1.5) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at -7.75 2) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at -7.75 2.5) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at -7.75 3) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at -7.75 3.5) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at -7.75 4) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at -7.75 4.5) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at -7.75 5) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at -7.75 5.5) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at -7.75 6) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at -6 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at -5.5 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd rect (at -5 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at -4.5 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 30 smd rect (at -4 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 31 smd rect (at -3.5 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 32 smd rect (at -3 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 33 smd rect (at -2.5 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 34 smd rect (at -2 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 35 smd rect (at -1.5 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 36 smd rect (at -1 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 37 smd rect (at -0.5 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 38 smd rect (at 0 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 39 smd rect (at 0.5 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 40 smd rect (at 1 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 41 smd rect (at 1.5 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 42 smd rect (at 2 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 43 smd rect (at 2.5 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 44 smd rect (at 3 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 45 smd rect (at 3.5 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 46 smd rect (at 4 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 47 smd rect (at 4.5 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 48 smd rect (at 5 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 49 smd rect (at 5.5 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 50 smd rect (at 6 7.75 90) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 51 smd rect (at 7.75 6 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 52 smd rect (at 7.75 5.5 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 53 smd rect (at 7.75 5 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 54 smd rect (at 7.75 4.5 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 55 smd rect (at 7.75 4 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 56 smd rect (at 7.75 3.5 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 57 smd rect (at 7.75 3 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 58 smd rect (at 7.75 2.5 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 59 smd rect (at 7.75 2 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 60 smd rect (at 7.75 1.5 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 61 smd rect (at 7.75 1 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 62 smd rect (at 7.75 0.5 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 63 smd rect (at 7.75 0 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 64 smd rect (at 7.75 -0.5 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 65 smd rect (at 7.75 -1 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 66 smd rect (at 7.75 -1.5 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 67 smd rect (at 7.75 -2 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 68 smd rect (at 7.75 -2.5 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 69 smd rect (at 7.75 -3 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 70 smd rect (at 7.75 -3.5 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 71 smd rect (at 7.75 -4 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 72 smd rect (at 7.75 -4.5 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 73 smd rect (at 7.75 -5 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 74 smd rect (at 7.75 -5.5 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 75 smd rect (at 7.75 -6 180) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 76 smd rect (at 6 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 77 smd rect (at 5.5 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 78 smd rect (at 5 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 79 smd rect (at 4.5 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 80 smd rect (at 4 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 81 smd rect (at 3.5 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 82 smd rect (at 3 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 83 smd rect (at 2.5 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 84 smd rect (at 2 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 85 smd rect (at 1.5 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 86 smd rect (at 1 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 87 smd rect (at 0.5 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 88 smd rect (at 0 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 89 smd rect (at -0.5 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 90 smd rect (at -1 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 91 smd rect (at -1.5 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 92 smd rect (at -2 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 93 smd rect (at -2.5 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 94 smd rect (at -3 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 95 smd rect (at -3.5 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 96 smd rect (at -4 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 97 smd rect (at -4.5 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 98 smd rect (at -5 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 99 smd rect (at -5.5 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 100 smd rect (at -6 -7.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask))
  (model Housings_QFP.3dshapes/LQFP-100_14x14mm_Pitch0.5mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
