(module Pin_Header_Straight_1x04 (layer F.Cu) (tedit 59447BCF)
  (descr "Through hole pin header")
  (tags "pin header")
  (fp_text reference P2 (at 0 -5.1) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value CONN_01X04 (at 0 -3.1) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.27 -2.54) (end 1.27 -2.54) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.27 5.08) (end 1.27 5.08) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.27 -5.08) (end -1.27 5.08) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.27 -5.08) (end -1.27 -5.08) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.27 5.08) (end 1.27 -5.08) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole circle (at 0 -3.81) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (pad 2 smd roundrect (at 0 -1.27) (size 1.75 1.75) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 3 thru_hole circle (at 0 1.27) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0 3.81) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (pad 4 smd roundrect (at 0 3.81) (size 1.75 1.75) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 3 smd roundrect (at 0 1.27) (size 1.75 1.75) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 2 thru_hole circle (at 0 -1.27) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (pad 1 smd roundrect (at 0 -3.81) (size 1.75 1.75) (layers B.Cu B.Mask)(roundrect_rratio 0.1))
  (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
    (at (xyz 0 -0.15 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
