EESchema-DOCLIB  Version 2.0
#
$CMP ADM4857
D 10Mbps RS485/RS422 transceiver, full duplex, receiver/driver enable, low power shutdown
K RS485 RS422 transceiver full duplex
F http://www.intersil.com/content/dam/Intersil/documents/isl8/isl83483-85-88-90-91.pdf
$ENDCMP
#
#End Doc Library
