(module C_0805 (layer F.Cu) (tedit 5959AFD9)
  (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
  (tags "capacitor 0805")
  (attr smd)
  (fp_text reference C20 (at 0 -1.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 220n (at 0 1.6) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0.5 -0.65) (end 0.5 0.625) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.5 -0.625) (end -0.5 0.625) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 -0.625) (end -1 -0.625) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 0.625) (end 1 -0.625) (layer F.SilkS) (width 0.15))
  (fp_line (start -1 0.625) (end 1 0.625) (layer F.SilkS) (width 0.15))
  (fp_line (start -1 -0.625) (end -1 0.625) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.7 -0.8) (end 1.7 -0.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.7 0.8) (end 1.7 0.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.7 -0.8) (end -1.7 0.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.7 -0.8) (end 1.7 0.8) (layer F.CrtYd) (width 0.05))
  (pad 1 smd roundrect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 2 smd roundrect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (model Capacitors_SMD.3dshapes/C_0805.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
