(module c_elec_5x5.3 (layer F.Cu) (tedit 593CC022)
  (descr "SMT capacitor, aluminium electrolytic, 5x5.3")
  (attr smd)
  (fp_text reference C26 (at 0 -3.81) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 10u (at 0 3.81) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 0 0) (end -2.5 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.778 -0.381) (end 1.778 0.381) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.159 0) (end 1.397 0) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.75 2.75) (end -2.75 -2.75) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 2.75) (end -2.75 2.75) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.75 -2) (end 2.75 2) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.75 -2.75) (end 2 -2.75) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 -2.75) (end 2.75 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 2.75) (end 2.75 2) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 -1.25) (end -2 1.25) (layer F.SilkS) (width 0.4))
  (pad 2 smd roundrect (at -2.2 0) (size 2.5 1.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 1 smd roundrect (at 2.2 0) (size 2.5 1.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (model ../lib/stmbl.pretty/ALU-C.WRL
    (at (xyz 0 0 0))
    (scale (xyz 390 390 390))
    (rotate (xyz 0 0 0))
  )
)
