(kicad_pcb (version 20160815) (host pcbnew "(2016-09-11 revision 6dfe58f)-master")

  (general
    (links 751)
    (no_connects 687)
    (area 172.924999 34.924999 273.075001 135.075001)
    (thickness 1.6)
    (drawings 21)
    (tracks 163)
    (zones 0)
    (modules 346)
    (nets 181)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 1)
    (zone_45_only no)
    (trace_min 0.15)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5 5)
    (pad_drill 5)
    (pad_to_mask_clearance 0.075)
    (pad_to_paste_clearance_ratio -0.1)
    (aux_axis_origin 273 135)
    (visible_elements FFFCFF7F)
    (pcbplotparams
      (layerselection 0x00030_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 +3.3VP)
  (net 4 GNDPWR)
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C4-Pad1)")
  (net 7 "Net-(C5-Pad1)")
  (net 8 "Net-(C6-Pad1)")
  (net 9 +5V)
  (net 10 /hv/f3/A_U)
  (net 11 +1V8)
  (net 12 "Net-(C15-Pad2)")
  (net 13 +3V3)
  (net 14 "Net-(C17-Pad1)")
  (net 15 /hv/f3/A_V)
  (net 16 VPP)
  (net 17 /hv/f3/A_W)
  (net 18 "Net-(C24-Pad1)")
  (net 19 "Net-(C24-Pad2)")
  (net 20 "Net-(C25-Pad1)")
  (net 21 "Net-(C25-Pad2)")
  (net 22 "Net-(C26-Pad1)")
  (net 23 "Net-(C26-Pad2)")
  (net 24 "Net-(C27-Pad1)")
  (net 25 "Net-(C27-Pad2)")
  (net 26 "Net-(C31-Pad1)")
  (net 27 "Net-(C32-Pad1)")
  (net 28 /hv/cur/A_IU)
  (net 29 /hv/f3/A_HV)
  (net 30 /hv/f3/BKIN)
  (net 31 "Net-(C41-Pad1)")
  (net 32 "Net-(C41-Pad2)")
  (net 33 /hv/back-emf/W)
  (net 34 "Net-(C42-Pad2)")
  (net 35 /hv/back-emf/V)
  (net 36 "Net-(C43-Pad2)")
  (net 37 /hv/back-emf/U)
  (net 38 "Net-(C44-Pad2)")
  (net 39 /hv/cur/A_IV)
  (net 40 /ctrl/FB1/A12)
  (net 41 /ctrl/FB0/A12)
  (net 42 /ctrl/FB0/A35)
  (net 43 /ctrl/FB1/A35)
  (net 44 "Net-(C51-Pad1)")
  (net 45 /hv/cur/A_IW)
  (net 46 +15V)
  (net 47 /ctrl/f4/A_24V_)
  (net 48 /ctrl/f4/A_5V_)
  (net 49 "Net-(C88-Pad1)")
  (net 50 "Net-(C90-Pad1)")
  (net 51 "Net-(D1-Pad2)")
  (net 52 "Net-(D1-Pad1)")
  (net 53 +24V)
  (net 54 "Net-(D2-Pad2)")
  (net 55 "Net-(D3-Pad2)")
  (net 56 "Net-(D5-Pad2)")
  (net 57 "Net-(D7-Pad2)")
  (net 58 "Net-(D8-Pad2)")
  (net 59 /ctrl/RX)
  (net 60 "Net-(Q1-Pad1)")
  (net 61 "Net-(Q2-Pad1)")
  (net 62 "Net-(Q3-Pad1)")
  (net 63 "Net-(Q4-Pad1)")
  (net 64 "Net-(JP1-Pad2)")
  (net 65 "Net-(R27-Pad2)")
  (net 66 "Net-(R32-Pad2)")
  (net 67 "Net-(J2-Pad3)")
  (net 68 "Net-(J1-Pad3)")
  (net 69 "Net-(J1-Pad6)")
  (net 70 "Net-(J2-Pad6)")
  (net 71 "Net-(J1-Pad1)")
  (net 72 "Net-(J2-Pad1)")
  (net 73 "Net-(J1-Pad2)")
  (net 74 "Net-(J2-Pad2)")
  (net 75 /hv/driver/CUH)
  (net 76 "Net-(R51-Pad2)")
  (net 77 "Net-(R54-Pad1)")
  (net 78 "Net-(R55-Pad1)")
  (net 79 "Net-(R56-Pad1)")
  (net 80 "Net-(R57-Pad1)")
  (net 81 "Net-(JP9-Pad2)")
  (net 82 "Net-(J3-Pad1)")
  (net 83 "Net-(J3-Pad2)")
  (net 84 "Net-(J3-Pad3)")
  (net 85 "Net-(J3-Pad6)")
  (net 86 "Net-(J3-Pad5)")
  (net 87 "Net-(J3-Pad4)")
  (net 88 "Net-(J3-Pad7)")
  (net 89 "Net-(J3-Pad8)")
  (net 90 /hv/f3/HV_RX)
  (net 91 "Net-(R77-Pad2)")
  (net 92 /hv/driver/CVH)
  (net 93 /hv/driver/CWH)
  (net 94 "Net-(R91-Pad2)")
  (net 95 /ctrl/f4/CMD_12E)
  (net 96 /ctrl/f4/CMD_36E)
  (net 97 /ctrl/f4/CMD_45E)
  (net 98 /ctrl/f4/CMD_78E)
  (net 99 "Net-(J1-Pad5)")
  (net 100 "Net-(J1-Pad4)")
  (net 101 "Net-(J2-Pad5)")
  (net 102 "Net-(J2-Pad4)")
  (net 103 /hv/f3/A_T_HV)
  (net 104 /ctrl/FB0/E12)
  (net 105 /ctrl/FB1/E12)
  (net 106 /ctrl/FB0/E36)
  (net 107 /ctrl/FB1/E36)
  (net 108 /ctrl/FB1/E45)
  (net 109 /ctrl/FB0/E45)
  (net 110 /hv/f3/HV_EN)
  (net 111 "Net-(T1-Pad1)")
  (net 112 /hv/f3/HV_TX)
  (net 113 /ctrl/f4/CMD_12)
  (net 114 /ctrl/f4/CMD_36)
  (net 115 /ctrl/f4/CMD_45)
  (net 116 /ctrl/f4/CMD_78)
  (net 117 /ctrl/FB1/D12)
  (net 118 /ctrl/FB0/D12)
  (net 119 /ctrl/FB1/D36)
  (net 120 /ctrl/FB0/D36)
  (net 121 /ctrl/FB0/D45)
  (net 122 /ctrl/FB1/D45)
  (net 123 "Net-(T44-Pad1)")
  (net 124 "Net-(T45-Pad1)")
  (net 125 "Net-(T46-Pad1)")
  (net 126 "Net-(P1-Pad3)")
  (net 127 "Net-(P1-Pad2)")
  (net 128 /hv/f3/CH1N)
  (net 129 /hv/f3/CH2N)
  (net 130 /hv/f3/CH1)
  (net 131 /hv/f3/CH3)
  (net 132 /hv/f3/CH3N)
  (net 133 /hv/f3/CH2)
  (net 134 "Net-(J2-Pad12)")
  (net 135 "Net-(J1-Pad12)")
  (net 136 "Net-(J1-Pad10)")
  (net 137 "Net-(J2-Pad10)")
  (net 138 "Net-(J3-Pad12)")
  (net 139 "Net-(J3-Pad10)")
  (net 140 "Net-(R129-Pad2)")
  (net 141 "Net-(C15-Pad1)")
  (net 142 "Net-(C53-Pad1)")
  (net 143 "Net-(C119-Pad2)")
  (net 144 "Net-(C71-Pad1)")
  (net 145 "Net-(C72-Pad1)")
  (net 146 "Net-(C83-Pad2)")
  (net 147 "Net-(C105-Pad1)")
  (net 148 "Net-(C105-Pad2)")
  (net 149 "Net-(C106-Pad1)")
  (net 150 "Net-(C106-Pad2)")
  (net 151 +12V)
  (net 152 "Net-(D7-Pad1)")
  (net 153 "Net-(R19-Pad1)")
  (net 154 "Net-(R19-Pad2)")
  (net 155 "Net-(R131-Pad2)")
  (net 156 "Net-(R130-Pad2)")
  (net 157 "Net-(R30-Pad2)")
  (net 158 "Net-(R35-Pad1)")
  (net 159 "Net-(R120-Pad2)")
  (net 160 /ctrl/TX)
  (net 161 /ctrl/IO/NRST)
  (net 162 +5F)
  (net 163 "Net-(C114-Pad1)")
  (net 164 "Net-(C117-Pad1)")
  (net 165 "Net-(C121-Pad1)")
  (net 166 "Net-(C121-Pad2)")
  (net 167 "Net-(R132-Pad1)")
  (net 168 /ctrl/FB0/A78)
  (net 169 /ctrl/FB1/A78)
  (net 170 /ctrl/f4/IO_AIN0)
  (net 171 /ctrl/f4/IO_AIN1)
  (net 172 "Net-(P9-Pad5)")
  (net 173 "Net-(P9-Pad2)")
  (net 174 /hv/f3/NRST)
  (net 175 "Net-(C36-Pad2)")
  (net 176 "Net-(C37-Pad2)")
  (net 177 /hv/f3/A_T_MOT)
  (net 178 "Net-(P2-Pad1)")
  (net 179 /hv/f3/SWCLK)
  (net 180 /hv/f3/SWDIO)

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net +12V)
    (add_net +15V)
    (add_net +1V8)
    (add_net +24V)
    (add_net +3.3VP)
    (add_net +3V3)
    (add_net +5F)
    (add_net +5V)
    (add_net /ctrl/FB0/A12)
    (add_net /ctrl/FB0/A35)
    (add_net /ctrl/FB0/A78)
    (add_net /ctrl/FB0/D12)
    (add_net /ctrl/FB0/D36)
    (add_net /ctrl/FB0/D45)
    (add_net /ctrl/FB0/E12)
    (add_net /ctrl/FB0/E36)
    (add_net /ctrl/FB0/E45)
    (add_net /ctrl/FB1/A12)
    (add_net /ctrl/FB1/A35)
    (add_net /ctrl/FB1/A78)
    (add_net /ctrl/FB1/D12)
    (add_net /ctrl/FB1/D36)
    (add_net /ctrl/FB1/D45)
    (add_net /ctrl/FB1/E12)
    (add_net /ctrl/FB1/E36)
    (add_net /ctrl/FB1/E45)
    (add_net /ctrl/IO/NRST)
    (add_net /ctrl/RX)
    (add_net /ctrl/TX)
    (add_net /ctrl/f4/A_24V_)
    (add_net /ctrl/f4/A_5V_)
    (add_net /ctrl/f4/CMD_12)
    (add_net /ctrl/f4/CMD_12E)
    (add_net /ctrl/f4/CMD_36)
    (add_net /ctrl/f4/CMD_36E)
    (add_net /ctrl/f4/CMD_45)
    (add_net /ctrl/f4/CMD_45E)
    (add_net /ctrl/f4/CMD_78)
    (add_net /ctrl/f4/CMD_78E)
    (add_net /ctrl/f4/IO_AIN0)
    (add_net /ctrl/f4/IO_AIN1)
    (add_net /hv/cur/A_IU)
    (add_net /hv/cur/A_IV)
    (add_net /hv/cur/A_IW)
    (add_net /hv/f3/A_HV)
    (add_net /hv/f3/A_T_HV)
    (add_net /hv/f3/A_T_MOT)
    (add_net /hv/f3/A_U)
    (add_net /hv/f3/A_V)
    (add_net /hv/f3/A_W)
    (add_net /hv/f3/BKIN)
    (add_net /hv/f3/CH1)
    (add_net /hv/f3/CH1N)
    (add_net /hv/f3/CH2)
    (add_net /hv/f3/CH2N)
    (add_net /hv/f3/CH3)
    (add_net /hv/f3/CH3N)
    (add_net /hv/f3/HV_EN)
    (add_net /hv/f3/HV_RX)
    (add_net /hv/f3/HV_TX)
    (add_net /hv/f3/NRST)
    (add_net /hv/f3/SWCLK)
    (add_net /hv/f3/SWDIO)
    (add_net GND)
    (add_net GNDPWR)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C105-Pad1)")
    (add_net "Net-(C105-Pad2)")
    (add_net "Net-(C106-Pad1)")
    (add_net "Net-(C106-Pad2)")
    (add_net "Net-(C114-Pad1)")
    (add_net "Net-(C117-Pad1)")
    (add_net "Net-(C119-Pad2)")
    (add_net "Net-(C121-Pad1)")
    (add_net "Net-(C121-Pad2)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C24-Pad1)")
    (add_net "Net-(C24-Pad2)")
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C25-Pad2)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C26-Pad2)")
    (add_net "Net-(C27-Pad1)")
    (add_net "Net-(C27-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C32-Pad1)")
    (add_net "Net-(C36-Pad2)")
    (add_net "Net-(C37-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C41-Pad1)")
    (add_net "Net-(C41-Pad2)")
    (add_net "Net-(C42-Pad2)")
    (add_net "Net-(C43-Pad2)")
    (add_net "Net-(C44-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C51-Pad1)")
    (add_net "Net-(C53-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C71-Pad1)")
    (add_net "Net-(C72-Pad1)")
    (add_net "Net-(C83-Pad2)")
    (add_net "Net-(C88-Pad1)")
    (add_net "Net-(C90-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J3-Pad12)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP9-Pad2)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P9-Pad2)")
    (add_net "Net-(P9-Pad5)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(R120-Pad2)")
    (add_net "Net-(R129-Pad2)")
    (add_net "Net-(R130-Pad2)")
    (add_net "Net-(R131-Pad2)")
    (add_net "Net-(R132-Pad1)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R27-Pad2)")
    (add_net "Net-(R30-Pad2)")
    (add_net "Net-(R32-Pad2)")
    (add_net "Net-(R35-Pad1)")
    (add_net "Net-(R51-Pad2)")
    (add_net "Net-(R54-Pad1)")
    (add_net "Net-(R55-Pad1)")
    (add_net "Net-(R56-Pad1)")
    (add_net "Net-(R57-Pad1)")
    (add_net "Net-(R77-Pad2)")
    (add_net "Net-(R91-Pad2)")
    (add_net "Net-(T1-Pad1)")
    (add_net "Net-(T44-Pad1)")
    (add_net "Net-(T45-Pad1)")
    (add_net "Net-(T46-Pad1)")
  )

  (net_class UVW ""
    (clearance 0.5)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net /hv/back-emf/U)
    (add_net /hv/back-emf/V)
    (add_net /hv/back-emf/W)
  )

  (net_class UVW_L ""
    (clearance 0.2)
    (trace_width 2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net /hv/driver/CUH)
    (add_net /hv/driver/CVH)
    (add_net /hv/driver/CWH)
  )

  (net_class VPP ""
    (clearance 1.5)
    (trace_width 4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net VPP)
  )

  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5415CFA7) (tstamp 57756C70)
    (at 210.25 106.5 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (path /5659094D/56590A3E/5669628D)
    (attr smd)
    (fp_text reference R32 (at 0 -2.3 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 250k (at 0 2.3 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 -1.2) (end 2.2 -1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -1.2) (end -2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.2 -1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 1.075) (end -1 1.075) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 -1.075) (end 1 -1.075) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 35 /hv/back-emf/V))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R32-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5415CFA7) (tstamp 57756C6B)
    (at 214.5 111 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (path /5659094D/56590A3E/56696104)
    (attr smd)
    (fp_text reference R28 (at 0 -2.3 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 250k (at 0 2.3 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 -1.2) (end 2.2 -1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -1.2) (end -2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.2 -1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 1.075) (end -1 1.075) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 -1.075) (end 1 -1.075) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R27-Pad2)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /hv/f3/A_U))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757646)
    (at 475.844577 24.626361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/56602D8C)
    (attr smd)
    (fp_text reference C1 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775764C)
    (at 425.286717 95.806361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D0/566317E6)
    (attr smd)
    (fp_text reference C2 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757652)
    (at 322.906717 57.696361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/5659191C/565DFF8B)
    (attr smd)
    (fp_text reference C3 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757658)
    (at 493.396717 98.706361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/565F7162/565DFF8B)
    (attr smd)
    (fp_text reference C4 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775765E)
    (at 421.090527 97.086361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D0/56631605)
    (attr smd)
    (fp_text reference C5 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 18p (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757664)
    (at 438.050527 82.726361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D0/566316C7)
    (attr smd)
    (fp_text reference C6 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 18p (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775766A)
    (at 418.196717 102.986361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D0/56631C3B)
    (attr smd)
    (fp_text reference C7 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 174 /hv/f3/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA) (tstamp 57757670)
    (at 448.485766 127.666361)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (path /56590966/56591916/566076FA)
    (attr smd)
    (fp_text reference C8 (at 0 -2.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7µ (at 0 2.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.8 -1) (end 1.8 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1) (end 1.8 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1) (end -1.8 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1) (end 1.8 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757676)
    (at 320.385766 51.796361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D0/57B30D45)
    (attr smd)
    (fp_text reference C9 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775767C)
    (at 479.168146 98.706361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D0/57B2E6B6)
    (attr smd)
    (fp_text reference C10 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757682)
    (at 513.488146 65.926361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/56590A3E/5682FF8E)
    (attr smd)
    (fp_text reference C11 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 18p (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 /hv/f3/A_U))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757688)
    (at 491.356717 86.906361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/565F7162/565E3C38)
    (attr smd)
    (fp_text reference C12 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 +1V8))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775768E)
    (at 239.25 58 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/5659191C/565E3C38)
    (attr smd)
    (fp_text reference C13 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 +1V8))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757694)
    (at 483.596717 86.906361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D4/57B2A93C)
    (attr smd)
    (fp_text reference C14 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 46 +15V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775769A)
    (at 328.616717 51.796361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D4/578281AC)
    (attr smd)
    (fp_text reference C15 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C15-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577576A0)
    (at 473.125791 12.826361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/5666869C)
    (attr smd)
    (fp_text reference C16 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577576A6)
    (at 264.076717 11.276361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591919/565DE6AE)
    (attr smd)
    (fp_text reference C17 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA) (tstamp 577576AC)
    (at 452.535766 127.666361)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (path /56590966/56591916/566075DC)
    (attr smd)
    (fp_text reference C18 (at 0 -2.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7µ (at 0 2.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.8 -1) (end 1.8 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1) (end 1.8 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1) (end -1.8 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1) (end 1.8 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577576B2)
    (at 332.496717 131.506361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/566A3B64)
    (attr smd)
    (fp_text reference C19 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577576B8)
    (at 528.198146 52.846361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/56590A3E/5683022A)
    (attr smd)
    (fp_text reference C20 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 18p (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 /hv/f3/A_V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577576CA)
    (at 539.598146 52.846361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/56590A3E/568302B9)
    (attr smd)
    (fp_text reference C23 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 18p (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /hv/f3/A_W))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577576D0)
    (at 458.698146 108.726361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/565F7162/565E18D1)
    (attr smd)
    (fp_text reference C24 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 18p (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C24-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C24-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577576D6)
    (at 245.5 55.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/5659191C/565E18D1)
    (attr smd)
    (fp_text reference C25 (at 0 -1.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 18p (at 0 1.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C25-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C25-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577576DC)
    (at 470.458146 94.086361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/565F7162/565FB16C)
    (attr smd)
    (fp_text reference C26 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 18p (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C26-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C26-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577576E2)
    (at 244.25 65.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/5659191C/565FB16C)
    (attr smd)
    (fp_text reference C27 (at 0 -1.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 18p (at 0 1.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C27-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C27-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577576EE)
    (at 469.047612 12.826361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/565FFAD0)
    (attr smd)
    (fp_text reference C29 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 161 /ctrl/IO/NRST))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577576F4)
    (at 326.496717 132.786361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/566A4471)
    (attr smd)
    (fp_text reference C30 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577576FA)
    (at 451.375503 29.726361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/565FDF4E)
    (attr smd)
    (fp_text reference C31 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 18p (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C31-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757700)
    (at 450.01611 35.626361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/565FDFAD)
    (attr smd)
    (fp_text reference C32 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 18p (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C32-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757706)
    (at 484.888146 120.286361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/57745B52/57747194)
    (attr smd)
    (fp_text reference C33 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 18p (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 28 /hv/cur/A_IU))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757718)
    (at 240.75 58 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/5659191C/565E1292)
    (attr smd)
    (fp_text reference C36 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(C36-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775771E)
    (at 493.756717 92.806361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/565F7162/565E1292)
    (attr smd)
    (fp_text reference C37 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(C37-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775772A)
    (at 513.488146 60.026361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/56590A3E/56830430)
    (attr smd)
    (fp_text reference C39 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 18p (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 29 /hv/f3/A_HV))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757730)
    (at 335.946717 125.606361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/566A5119)
    (attr smd)
    (fp_text reference C40 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 30 /hv/f3/BKIN))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757736)
    (at 411.896717 124.176361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D4/5774B2A5)
    (attr smd)
    (fp_text reference C41 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C41-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C41-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775773C)
    (at 204.25 100.5 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/56590A75/5659119D)
    (attr smd)
    (fp_text reference C42 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2.2µ (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 /hv/back-emf/W))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C42-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757742)
    (at 209.25 100.5 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/56590A75/5668E03D)
    (attr smd)
    (fp_text reference C43 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2.2µ (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 35 /hv/back-emf/V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C43-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757748)
    (at 214.25 100.5 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/56590A75/5668E1AC)
    (attr smd)
    (fp_text reference C44 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2.2µ (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 37 /hv/back-emf/U))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C44-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775774E)
    (at 478.938146 126.186361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/57745B52/57747518)
    (attr smd)
    (fp_text reference C45 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 18p (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 39 /hv/cur/A_IV))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757754)
    (at 486.428146 92.806361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/565F7162/565E24CA)
    (attr smd)
    (fp_text reference C46 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 /ctrl/FB1/A12))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775775A)
    (at 332.498146 51.796361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/5659191C/565E24CA)
    (attr smd)
    (fp_text reference C47 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 41 /ctrl/FB0/A12))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757760)
    (at 316.988146 51.796361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/5659191C/565E32D1)
    (attr smd)
    (fp_text reference C48 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 /ctrl/FB0/A35))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757766)
    (at 455.028146 109.006361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/565F7162/565E32D1)
    (attr smd)
    (fp_text reference C49 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 43 /ctrl/FB1/A35))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757778)
    (at 471.766398 24.626361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591923/5777ECBE)
    (attr smd)
    (fp_text reference C52 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 170 /ctrl/f4/IO_AIN0))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775777E)
    (at 249.966717 -0.523639)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591919/565DD843)
    (attr smd)
    (fp_text reference C53 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(C53-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757784)
    (at 241.656717 8.216361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591919/565DDCA7)
    (attr smd)
    (fp_text reference C54 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(C53-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775778A)
    (at 248.776717 5.376361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591919/565DDF12)
    (attr smd)
    (fp_text reference C55 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(C53-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757790)
    (at 259.766717 11.276361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591919/565DDF48)
    (attr smd)
    (fp_text reference C56 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(C53-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757796)
    (at 474.538146 120.286361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/57745B52/5774768D)
    (attr smd)
    (fp_text reference C57 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 18p (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 45 /hv/cur/A_IW))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775779C)
    (at 419.706717 128.796361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D4/56657F29)
    (attr smd)
    (fp_text reference C58 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 46 +15V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577577A2)
    (at 484.000935 18.726361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591923/5777ECC5)
    (attr smd)
    (fp_text reference C59 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 171 /ctrl/f4/IO_AIN1))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577577AE)
    (at 432.856717 88.626361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D0/566A7777)
    (attr smd)
    (fp_text reference C61 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577577BA)
    (at 239.75 100.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/56590A75/56690594)
    (attr smd)
    (fp_text reference C63 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 46 +15V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577577C0)
    (at 490.7979 12.826361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/56693D94)
    (attr smd)
    (fp_text reference C64 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 47 /ctrl/f4/A_24V_))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577577C6)
    (at 467.688219 33.086361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/565FE80F)
    (attr smd)
    (fp_text reference C65 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2.2µ (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(C119-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577577CC)
    (at 363.588146 109.376361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591923/56819E35)
    (attr smd)
    (fp_text reference C66 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value C (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577577D2)
    (at 366.828146 103.476361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591923/56819EA9)
    (attr smd)
    (fp_text reference C67 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value C (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577577D8)
    (at 358.448146 110.476361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591923/56819EF3)
    (attr smd)
    (fp_text reference C68 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value C (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577577DE)
    (at 421.92005 116.996361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D4/57B295B0)
    (attr smd)
    (fp_text reference C69 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 46 +15V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577577EA)
    (at 471.836717 99.986361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/565F7162/565DFE96)
    (attr smd)
    (fp_text reference C71 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(C71-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577577F0)
    (at 317.326717 45.896361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/5659191C/565DFE96)
    (attr smd)
    (fp_text reference C72 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(C72-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577577F6)
    (at 466.246717 105.886361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/565F7162/565DFEBA)
    (attr smd)
    (fp_text reference C73 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(C71-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 577577FC)
    (at 319.146717 34.096361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/5659191C/565DFEBA)
    (attr smd)
    (fp_text reference C74 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(C72-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757802)
    (at 309.566717 41.276361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/5659191C/565DFEDE)
    (attr smd)
    (fp_text reference C75 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(C72-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757808)
    (at 482.546717 92.806361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/565F7162/565DFEDE)
    (attr smd)
    (fp_text reference C76 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(C71-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775780E)
    (at 482.641542 24.626361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/565FE7DB)
    (attr smd)
    (fp_text reference C77 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757814)
    (at 413.886717 104.426361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D0/5663136E)
    (attr smd)
    (fp_text reference C78 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775781A)
    (at 434.216717 82.726361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D0/56631543)
    (attr smd)
    (fp_text reference C79 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757820)
    (at 492.157293 18.726361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/565FE7A9)
    (attr smd)
    (fp_text reference C80 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757826)
    (at 479.922756 30.526361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/56692CBC)
    (attr smd)
    (fp_text reference C81 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 48 /ctrl/f4/A_5V_))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775782C)
    (at 425.286717 89.906361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D0/5663155A)
    (attr smd)
    (fp_text reference C82 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757832)
    (at 429.906717 82.726361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D0/56631574)
    (attr smd)
    (fp_text reference C83 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(C83-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757838)
    (at 477.20397 36.426361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/565FE77A)
    (attr smd)
    (fp_text reference C84 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775783E)
    (at 488.079114 24.626361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/565FE74C)
    (attr smd)
    (fp_text reference C85 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757844)
    (at 470.407005 36.426361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/565FE720)
    (attr smd)
    (fp_text reference C86 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775784A)
    (at 493.516686 12.826361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/565FE6F4)
    (attr smd)
    (fp_text reference C87 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757850)
    (at 466.328826 38.986361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/565FE20A)
    (attr smd)
    (fp_text reference C88 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2.2µ (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(C88-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757856)
    (at 474.485184 30.526361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/565FE528)
    (attr smd)
    (fp_text reference C89 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 5775785C)
    (at 489.438507 18.726361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/565FE1E0)
    (attr smd)
    (fp_text reference C90 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2.2µ (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(C90-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57757862)
    (at 448.656717 41.526361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/565FF416)
    (attr smd)
    (fp_text reference C91 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED-0603 (layer F.Cu) (tedit 55BDE255) (tstamp 57757868)
    (at 398.412908 107.896361)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5659094D/565909D0/5776010E)
    (attr smd)
    (fp_text reference D1 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 0.55) (end 0.8 0.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.1 -0.55) (end 0.8 -0.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.2 0) (end 0.25 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 -0.25) (end -0.25 0.25) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 0) (end 0 -0.25) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -0.25) (end 0 0.25) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 0.25) (end -0.25 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.4 -0.75) (end 1.4 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.75) (end -1.4 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.75) (end -1.4 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.75) (end 1.4 -0.75) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D1-Pad1)"))
  )

  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5530FCB9) (tstamp 5775786E)
    (at 377.325766 82.826361)
    (descr SOD-123)
    (tags SOD-123)
    (path /56590966/56591923/5700FF9B)
    (attr smd)
    (fp_text reference D2 (at 0 -2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 0 2.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.3175 0) (end 0.6985 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.6985 0) (end -0.3175 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.3175 0) (end 0.3175 -0.381) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.3175 -0.381) (end 0.3175 0.381) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.3175 0.381) (end -0.3175 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.3175 -0.508) (end -0.3175 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.25 -1.05) (end 2.25 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 -1.05) (end 2.25 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.05) (end -2.25 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -1.05) (end -2.25 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2 0.9) (end 1.54 0.9) (layer F.SilkS) (width 0.15))
    (fp_line (start -2 -0.9) (end 1.54 -0.9) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 53 +24V))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D2-Pad2)"))
  )

  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5530FCB9) (tstamp 57757874)
    (at 355.935766 104.376361)
    (descr SOD-123)
    (tags SOD-123)
    (path /56590966/56591923/57011965)
    (attr smd)
    (fp_text reference D3 (at 0 -2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 0 2.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.3175 0) (end 0.6985 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.6985 0) (end -0.3175 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.3175 0) (end 0.3175 -0.381) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.3175 -0.381) (end 0.3175 0.381) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.3175 0.381) (end -0.3175 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.3175 -0.508) (end -0.3175 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.25 -1.05) (end 2.25 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 -1.05) (end 2.25 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.05) (end -2.25 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -1.05) (end -2.25 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2 0.9) (end 1.54 0.9) (layer F.SilkS) (width 0.15))
    (fp_line (start -2 -0.9) (end 1.54 -0.9) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 53 +24V))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(D3-Pad2)"))
  )

  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5530FCB9) (tstamp 57757880)
    (at 365.925766 97.376361)
    (descr SOD-123)
    (tags SOD-123)
    (path /56590966/56591923/570122EB)
    (attr smd)
    (fp_text reference D5 (at 0 -2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 0 2.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.3175 0) (end 0.6985 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.6985 0) (end -0.3175 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.3175 0) (end 0.3175 -0.381) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.3175 -0.381) (end 0.3175 0.381) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.3175 0.381) (end -0.3175 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.3175 -0.508) (end -0.3175 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.25 -1.05) (end 2.25 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 -1.05) (end 2.25 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.05) (end -2.25 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -1.05) (end -2.25 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2 0.9) (end 1.54 0.9) (layer F.SilkS) (width 0.15))
    (fp_line (start -2 -0.9) (end 1.54 -0.9) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 53 +24V))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(D5-Pad2)"))
  )

  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5530FCB9) (tstamp 57757886)
    (at 347.345766 111.026361)
    (descr SOD-123)
    (tags SOD-123)
    (path /56590966/56591923/57014DB3)
    (attr smd)
    (fp_text reference D7 (at 0 -2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 0 2.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.3175 0) (end 0.6985 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.6985 0) (end -0.3175 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.3175 0) (end 0.3175 -0.381) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.3175 -0.381) (end 0.3175 0.381) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.3175 0.381) (end -0.3175 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.3175 -0.508) (end -0.3175 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.25 -1.05) (end 2.25 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 -1.05) (end 2.25 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.05) (end -2.25 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -1.05) (end -2.25 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2 0.9) (end 1.54 0.9) (layer F.SilkS) (width 0.15))
    (fp_line (start -2 -0.9) (end 1.54 -0.9) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(D7-Pad2)"))
  )

  (module LEDs:LED-0603 (layer F.Cu) (tedit 55BDE255) (tstamp 5775788C)
    (at 396.932908 134.526361)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5659094D/565909D4/57752985)
    (attr smd)
    (fp_text reference D8 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 0.55) (end 0.8 0.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.1 -0.55) (end 0.8 -0.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.2 0) (end 0.25 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 -0.25) (end -0.25 0.25) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 0) (end 0 -0.25) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -0.25) (end 0 0.25) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 0.25) (end -0.25 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.4 -0.75) (end 1.4 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.75) (end -1.4 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.75) (end -1.4 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.75) (end 1.4 -0.75) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(D8-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
  )

  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C) (tstamp 577578D4)
    (at 400.589098 120.196361)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5659094D/565909D4/566D36EA)
    (fp_text reference P11 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.27 1.27) (end 1.27 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.75 -1.75) (end -1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 4.3) (end 1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 1.27) (end -1.27 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 3.81) (end 1.27 3.81) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 +15V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 0) (tstamp 577578DC)
    (at 399.509098 85.926361)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5659094D/565909D0/5663248E)
    (fp_text reference P12 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X04 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 9.4) (end 1.75 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 8.89) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end 1.27 8.89) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 8.89) (end 1.27 8.89) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 179 /hv/f3/SWCLK))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 180 /hv/f3/SWDIO))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 174 /hv/f3/NRST))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8) (tstamp 577578F3)
    (at 349.169574 97.976361)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /56590966/56591923/5700EA19)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IRLML6344 (at 0 2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.65 -1.6) (end 1.65 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.6) (end 1.65 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 1.6) (end -1.65 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.65 1.6) (end -1.65 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.29916 -0.65024) (end 1.2509 -0.65024) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.49982 0.0508) (end -1.49982 -0.65024) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.49982 -0.65024) (end -1.2509 -0.65024) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.29916 -0.65024) (end 1.49982 -0.65024) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.49982 -0.65024) (end 1.49982 0.0508) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D2-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8) (tstamp 577578FA)
    (at 367.749574 90.976361)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /56590966/56591923/57011943)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IRLML6344 (at 0 2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.65 -1.6) (end 1.65 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.6) (end 1.65 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 1.6) (end -1.65 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.65 1.6) (end -1.65 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.29916 -0.65024) (end 1.2509 -0.65024) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.49982 0.0508) (end -1.49982 -0.65024) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.49982 -0.65024) (end -1.2509 -0.65024) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.29916 -0.65024) (end 1.49982 -0.65024) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.49982 -0.65024) (end 1.49982 0.0508) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(D3-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8) (tstamp 57757901)
    (at 357.759574 97.976361)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /56590966/56591923/570122C9)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IRLML6344 (at 0 2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.65 -1.6) (end 1.65 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.6) (end 1.65 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 1.6) (end -1.65 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.65 1.6) (end -1.65 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.29916 -0.65024) (end 1.2509 -0.65024) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.49982 0.0508) (end -1.49982 -0.65024) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.49982 -0.65024) (end -1.2509 -0.65024) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.29916 -0.65024) (end 1.49982 -0.65024) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.49982 -0.65024) (end 1.49982 0.0508) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(D5-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8) (tstamp 57757908)
    (at 349.169574 104.626361)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /56590966/56591923/57014D91)
    (attr smd)
    (fp_text reference Q4 (at 0 -2.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IRLML6344 (at 0 2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.65 -1.6) (end 1.65 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.6) (end 1.65 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 1.6) (end -1.65 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.65 1.6) (end -1.65 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.29916 -0.65024) (end 1.2509 -0.65024) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.49982 0.0508) (end -1.49982 -0.65024) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.49982 -0.65024) (end -1.2509 -0.65024) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.29916 -0.65024) (end 1.49982 -0.65024) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.49982 -0.65024) (end 1.49982 0.0508) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(D7-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 5775790E)
    (at 456.813075 27.186361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591913/56602DEB)
    (attr smd)
    (fp_text reference R1 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757914)
    (at 429.072908 89.906361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/565909D0/566A7D18)
    (attr smd)
    (fp_text reference R2 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(JP1-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 5775791A)
    (at 307.704336 58.976361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565DFFA4)
    (attr smd)
    (fp_text reference R3 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 560 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(J2-Pad12)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757920)
    (at 475.294336 92.806361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565DFFA4)
    (attr smd)
    (fp_text reference R4 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 560 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(J1-Pad12)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757926)
    (at 478.694336 92.806361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565DFFAB)
    (attr smd)
    (fp_text reference R5 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 560 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(J1-Pad10)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 5775792C)
    (at 328.084336 39.996361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565DFFAB)
    (attr smd)
    (fp_text reference R6 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 560 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(J2-Pad10)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757932)
    (at 413.434336 98.526361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/57DD2315)
    (attr smd)
    (fp_text reference R7 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 177 /hv/f3/A_T_MOT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757938)
    (at 417.714336 97.086361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/565909D0/57760220)
    (attr smd)
    (fp_text reference R8 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 560 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 5775793E)
    (at 363.575766 103.476361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591923/5700ECBA)
    (attr smd)
    (fp_text reference R9 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757944)
    (at 354.998146 110.926361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591923/5701194A)
    (attr smd)
    (fp_text reference R10 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 5775794A)
    (at 373.768146 90.626361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591923/570122D0)
    (attr smd)
    (fp_text reference R11 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757950)
    (at 377.218146 88.926361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591923/5700F279)
    (attr smd)
    (fp_text reference R12 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757956)
    (at 370.128146 97.276361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591923/57011951)
    (attr smd)
    (fp_text reference R13 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 5775795C)
    (at 373.768146 96.526361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591923/570122D7)
    (attr smd)
    (fp_text reference R14 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757962)
    (at 493.918146 104.606361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565DFF84)
    (attr smd)
    (fp_text reference R15 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757968)
    (at 304.278146 54.356361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565DFF84)
    (attr smd)
    (fp_text reference R16 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 5775796E)
    (at 255.888146 11.276361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/565DE7AD)
    (attr smd)
    (fp_text reference R17 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(J3-Pad12)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757974)
    (at 249.538146 -6.423639)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/565DE83B)
    (attr smd)
    (fp_text reference R18 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(J3-Pad10)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 5775797A)
    (at 486.068146 104.606361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/565909D4/5782819E)
    (attr smd)
    (fp_text reference R19 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 15k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(R19-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(R19-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757980)
    (at 313.448146 39.996361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/565909D4/5782DC21)
    (attr smd)
    (fp_text reference R20 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(R19-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757986)
    (at 482.618146 104.606361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/565909D4/57828197)
    (attr smd)
    (fp_text reference R21 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(R19-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 5775798C)
    (at 315.578146 57.696361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/565909D4/578281E1)
    (attr smd)
    (fp_text reference R22 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(R19-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757992)
    (at 475.318146 86.906361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565E3AE9)
    (attr smd)
    (fp_text reference R23 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(R131-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 +1V8))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757998)
    (at 238 62.75 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565E3AE9)
    (attr smd)
    (fp_text reference R24 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(R130-Pad2)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 +1V8))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 5775799E)
    (at 237.5 58 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565E3BA8)
    (attr smd)
    (fp_text reference R25 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 +1V8))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 577579A4)
    (at 462.148146 108.726361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565E3BA8)
    (attr smd)
    (fp_text reference R26 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 +1V8))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 577579B6)
    (at 216.5 113.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/56590A3E/56696127)
    (attr smd)
    (fp_text reference R29 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3.9k (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 /hv/f3/A_U))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 577579BC)
    (at 509.891003 60.026361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/565909D4/57B00182)
    (attr smd)
    (fp_text reference R30 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 +15V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(R30-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 577579C2)
    (at 252.988146 -6.423639)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/565DE65E)
    (attr smd)
    (fp_text reference R31 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 577579D4)
    (at 212.25 113.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/56590A3E/56696299)
    (attr smd)
    (fp_text reference R34 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3.9k (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /hv/f3/A_V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 577579DA)
    (at 536.5 63)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591916/57AD3DAE)
    (attr smd)
    (fp_text reference R35 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(R35-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 577579E0)
    (at 246.5 53.25 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565E2D07)
    (attr smd)
    (fp_text reference R36 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C25-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(J2-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 577579E6)
    (at 486.778146 110.506361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565E2D07)
    (attr smd)
    (fp_text reference R37 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C24-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(J1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 577579EC)
    (at 489.518146 98.706361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565E2D0D)
    (attr smd)
    (fp_text reference R38 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C24-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(J1-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 577579F2)
    (at 244.75 53.25 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565E2D0D)
    (attr smd)
    (fp_text reference R39 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C25-Pad2)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(J2-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 577579F8)
    (at 351.548146 110.926361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591923/57014D98)
    (attr smd)
    (fp_text reference R40 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 577579FE)
    (at 489.878146 92.806361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565E07F5)
    (attr smd)
    (fp_text reference R41 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C26-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(J1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A04)
    (at 246.75 66 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565E07F5)
    (attr smd)
    (fp_text reference R42 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C27-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(J2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A0A)
    (at 479.168146 104.606361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565E0878)
    (attr smd)
    (fp_text reference R43 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C26-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(J1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A10)
    (at 244.25 67)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565E0878)
    (attr smd)
    (fp_text reference R44 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C27-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(J2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A16)
    (at 360.138146 104.276361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591923/57014D9F)
    (attr smd)
    (fp_text reference R45 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A1C)
    (at 481.438146 120.286361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/57745B52/5774716E)
    (attr smd)
    (fp_text reference R46 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 560 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 /hv/cur/A_IU))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 75 /hv/driver/CUH))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A22)
    (at 240.25 62)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565E0919)
    (attr smd)
    (fp_text reference R47 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 15k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 +1V8))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C27-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A28)
    (at 475.718146 104.606361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565E0919)
    (attr smd)
    (fp_text reference R48 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 15k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 +1V8))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C26-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A2E)
    (at 470.128146 105.886361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565E2D13)
    (attr smd)
    (fp_text reference R49 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 15k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 +1V8))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C24-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A34)
    (at 240.25 60.25)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565E2D13)
    (attr smd)
    (fp_text reference R50 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 15k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 +1V8))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C25-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A46)
    (at 208 113.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/56590A3E/56696344)
    (attr smd)
    (fp_text reference R53 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3.9k (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /hv/f3/A_W))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A4C)
    (at 487.478146 86.906361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565E098D)
    (attr smd)
    (fp_text reference R54 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 15k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(R54-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C26-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A52)
    (at 241.75 66 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565E098D)
    (attr smd)
    (fp_text reference R55 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 15k (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(R55-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C27-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A58)
    (at 243 54.75 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565E2D19)
    (attr smd)
    (fp_text reference R56 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 15k (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(R56-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C25-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A5E)
    (at 475.718146 98.706361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565E2D19)
    (attr smd)
    (fp_text reference R57 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 15k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(R57-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C24-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A64)
    (at 471.088146 120.286361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/57745B52/57747224)
    (attr smd)
    (fp_text reference R58 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 15k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 /hv/cur/A_IU))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A6A)
    (at 525.501003 64.646361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591916/57AD27A6)
    (attr smd)
    (fp_text reference R59 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3.9k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(R120-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A70)
    (at 451.148146 133.766361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591916/57AD3DA8)
    (attr smd)
    (fp_text reference R60 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(R35-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A76)
    (at 486.719721 18.726361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591913/566A9C27)
    (attr smd)
    (fp_text reference R61 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(JP9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A7C)
    (at 261.25 47.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/56F9D4F8)
    (attr smd)
    (fp_text reference R62 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(C53-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(J3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A82)
    (at 263.25 47.25 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/565DD7F2)
    (attr smd)
    (fp_text reference R63 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(J3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A88)
    (at 270.75 46)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/56F9D5CB)
    (attr smd)
    (fp_text reference R64 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(J3-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A8E)
    (at 260.5 44 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/56F9E212)
    (attr smd)
    (fp_text reference R65 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(C53-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(J3-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A94)
    (at 268.5 44.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/565DDCA1)
    (attr smd)
    (fp_text reference R66 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(J3-Pad3)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(J3-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757A9A)
    (at 270.75 42.5)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/56F9E5E6)
    (attr smd)
    (fp_text reference R67 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(J3-Pad6)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757AA0)
    (at 261.25 40.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/56F9EA0F)
    (attr smd)
    (fp_text reference R68 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(C53-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(J3-Pad5)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757AA6)
    (at 263.25 44 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/565DDF0C)
    (attr smd)
    (fp_text reference R69 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(J3-Pad5)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(J3-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757AAC)
    (at 270.75 44.25)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/56F9EFAF)
    (attr smd)
    (fp_text reference R70 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(J3-Pad4)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757AB2)
    (at 256.108146 5.376361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/56F9FEE2)
    (attr smd)
    (fp_text reference R71 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(C53-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(J3-Pad7)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757AB8)
    (at 263.25 40.75 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/565DDF42)
    (attr smd)
    (fp_text reference R72 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(J3-Pad7)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(J3-Pad8)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757ABE)
    (at 270.75 40.75)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/56F9FFE7)
    (attr smd)
    (fp_text reference R73 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(J3-Pad8)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757AC4)
    (at 462.571003 120.286361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591916/57AD3DEC)
    (attr smd)
    (fp_text reference R74 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(R35-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757ACA)
    (at 404.471003 130.476361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/565909D4/57752B29)
    (attr smd)
    (fp_text reference R75 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(R30-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(D8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757AD0)
    (at 319.168146 132.786361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/566A39B6)
    (attr smd)
    (fp_text reference R76 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 /hv/f3/BKIN))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 90 /hv/f3/HV_RX))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757AE2)
    (at 239.5 118.75 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/56590A3E/566963E3)
    (attr smd)
    (fp_text reference R79 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3.9k (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /hv/f3/A_HV))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757AFA)
    (at 322.618146 132.786361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/566A56D0)
    (attr smd)
    (fp_text reference R83 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 /hv/f3/BKIN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B00)
    (at 471.088146 126.186361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/57745B52/57747512)
    (attr smd)
    (fp_text reference R84 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 560 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 /hv/cur/A_IV))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 92 /hv/driver/CVH))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B06)
    (at 332.068146 125.606361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/566A5921)
    (attr smd)
    (fp_text reference R85 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 /hv/f3/BKIN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B0C)
    (at 329.928146 34.096361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565E236D)
    (attr smd)
    (fp_text reference R86 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 /ctrl/FB0/A12))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(R55-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B12)
    (at 451.578146 109.006361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565E236D)
    (attr smd)
    (fp_text reference R87 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 /ctrl/FB1/A12))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(R54-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B18)
    (at 467.008146 94.086361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565E32C5)
    (attr smd)
    (fp_text reference R88 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 /ctrl/FB1/A35))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(R57-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B1E)
    (at 321.208146 39.996361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565E32C5)
    (attr smd)
    (fp_text reference R89 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 /ctrl/FB0/A35))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(R56-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B24)
    (at 477.988146 120.286361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/57745B52/5774751E)
    (attr smd)
    (fp_text reference R90 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 15k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 /hv/cur/A_IV))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B2A)
    (at 393.578146 130.096361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/565909D4/5774B784)
    (attr smd)
    (fp_text reference R91 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C41-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(R91-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B30)
    (at 412.468146 130.076361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/565909D4/5774BB53)
    (attr smd)
    (fp_text reference R92 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(R91-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C51-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B36)
    (at 311.818146 34.096361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565E23EB)
    (attr smd)
    (fp_text reference R93 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 /ctrl/FB0/A12))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B3C)
    (at 482.618146 98.706361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565E23EB)
    (attr smd)
    (fp_text reference R94 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 /ctrl/FB1/A12))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B42)
    (at 300.828146 48.736361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565E32CB)
    (attr smd)
    (fp_text reference R95 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 /ctrl/FB0/A35))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B48)
    (at 486.068146 98.706361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565E32CB)
    (attr smd)
    (fp_text reference R96 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 /ctrl/FB1/A35))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B4E)
    (at 460.891254 27.186361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591916/57AD27A0)
    (attr smd)
    (fp_text reference R97 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(R120-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B54)
    (at 462.250647 38.986361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591923/5777ECA3)
    (attr smd)
    (fp_text reference R98 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(P9-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 170 /ctrl/f4/IO_AIN0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B5A)
    (at 458.172468 38.986361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591923/5777ECAA)
    (attr smd)
    (fp_text reference R99 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 170 /ctrl/f4/IO_AIN0))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B60)
    (at 488.814336 120.286361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/57745B52/57747687)
    (attr smd)
    (fp_text reference R100 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 560 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 /hv/cur/A_IW))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 /hv/driver/CWH))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B66)
    (at 260.034336 5.376361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/57758B35)
    (attr smd)
    (fp_text reference R101 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 95 /ctrl/f4/CMD_12E))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B6C)
    (at 264.434336 5.376361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/57758F9B)
    (attr smd)
    (fp_text reference R102 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 96 /ctrl/f4/CMD_36E))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B72)
    (at 256.914336 -6.423639)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/577591B1)
    (attr smd)
    (fp_text reference R103 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 97 /ctrl/f4/CMD_45E))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B78)
    (at 268.124336 -0.523639)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/5775928B)
    (attr smd)
    (fp_text reference R104 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 98 /ctrl/f4/CMD_78E))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B7E)
    (at 478.563363 18.726361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591923/5777EC9C)
    (attr smd)
    (fp_text reference R105 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 170 /ctrl/f4/IO_AIN0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B84)
    (at 485.360328 12.826361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591923/5777EC80)
    (attr smd)
    (fp_text reference R106 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(P9-Pad5)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 171 /ctrl/f4/IO_AIN1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B8A)
    (at 475.014336 126.186361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/57745B52/57747693)
    (attr smd)
    (fp_text reference R107 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 15k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 /hv/cur/A_IW))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B90)
    (at 463.61004 33.086361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591923/5777EC87)
    (attr smd)
    (fp_text reference R108 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 171 /ctrl/f4/IO_AIN1))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B96)
    (at 263.25 63.75 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565DFE8F)
    (attr smd)
    (fp_text reference R109 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(J2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757B9C)
    (at 474.054336 110.506361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565DFE8F)
    (attr smd)
    (fp_text reference R110 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(J1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757BA2)
    (at 268.5 59.75 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565DFEB3)
    (attr smd)
    (fp_text reference R111 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(J2-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757BA8)
    (at 479.244336 86.906361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565DFEB3)
    (attr smd)
    (fp_text reference R112 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(J1-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757BAE)
    (at 467.484336 99.986361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/565DFED7)
    (attr smd)
    (fp_text reference R113 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(J1-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757BB4)
    (at 263.25 60.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/565DFED7)
    (attr smd)
    (fp_text reference R114 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(J2-Pad5)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(J2-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757BBA)
    (at 310.25 102.25)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/56590A75/566DE4EC)
    (attr smd)
    (fp_text reference R115 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 103 /hv/f3/A_T_HV))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757BC0)
    (at 454.094289 38.986361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591913/5668EA86)
    (attr smd)
    (fp_text reference R116 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 +24V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 /ctrl/f4/A_24V_))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757BC6)
    (at 481.282149 12.826361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591913/5668EAFB)
    (attr smd)
    (fp_text reference R117 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 /ctrl/f4/A_24V_))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757BCC)
    (at 408.544336 130.476361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/565909D4/56657FD1)
    (attr smd)
    (fp_text reference R118 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3.9k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 +15V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757BD2)
    (at 459.531861 33.086361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591923/5777EC79)
    (attr smd)
    (fp_text reference R119 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 171 /ctrl/f4/IO_AIN1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757BDE)
    (at 455.453682 33.086361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591913/5668F2EF)
    (attr smd)
    (fp_text reference R121 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 /ctrl/f4/A_5V_))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757BE4)
    (at 464.969433 27.186361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591913/5668F395)
    (attr smd)
    (fp_text reference R122 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 /ctrl/f4/A_5V_))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757BEA)
    (at 324.264336 51.796361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/57756B74)
    (attr smd)
    (fp_text reference R123 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 104 /ctrl/FB0/E12))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757BF0)
    (at 478.454336 110.506361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/57756B74)
    (attr smd)
    (fp_text reference R124 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 105 /ctrl/FB1/E12))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757BF6)
    (at 330.394336 45.896361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/57757310)
    (attr smd)
    (fp_text reference R125 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 106 /ctrl/FB0/E36))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757BFC)
    (at 482.854336 110.506361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/57757310)
    (attr smd)
    (fp_text reference R126 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 107 /ctrl/FB1/E36))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757C02)
    (at 489.994336 104.606361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/57757D9E)
    (attr smd)
    (fp_text reference R127 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 108 /ctrl/FB1/E45))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57757C08)
    (at 327.264336 57.696361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/57757D9E)
    (attr smd)
    (fp_text reference R128 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 109 /ctrl/FB0/E45))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 0) (tstamp 57757C12)
    (at 405.67148 106.346361)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (path /5659094D/565909D0/57751F4A)
    (fp_text reference T1 (at 0 -2.54) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value testpoint (at 1.27 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(T1-Pad1)"))
  )

  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 0) (tstamp 57757C6C)
    (at 510.31148 53.486361)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (path /5659094D/56590A3E/568301A4)
    (fp_text reference T19 (at 0 -2.54) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value testpoint (at 1.27 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
  )

  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 0) (tstamp 57757C8F)
    (at 234.67148 1.676361)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (path /56590966/56591919/5681B104)
    (fp_text reference T26 (at 0 -2.54) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value testpoint (at 1.27 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 113 /ctrl/f4/CMD_12))
  )

  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 0) (tstamp 57757C94)
    (at 241.79148 1.676361)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (path /56590966/56591919/5681AEA1)
    (fp_text reference T27 (at 0 -2.54) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value testpoint (at 1.27 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 114 /ctrl/f4/CMD_36))
  )

  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 0) (tstamp 57757C99)
    (at 234.67148 8.856361)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (path /56590966/56591919/5681AC45)
    (fp_text reference T28 (at 0 -2.54) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value testpoint (at 1.27 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 115 /ctrl/f4/CMD_45))
  )

  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 0) (tstamp 57757C9E)
    (at 242.98148 -5.783639)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (path /56590966/56591919/5681A9CE)
    (fp_text reference T29 (at 0 -2.54) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value testpoint (at 1.27 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 116 /ctrl/f4/CMD_78))
  )

  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 0) (tstamp 57757CE9)
    (at 418.30148 90.546361)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (path /5659094D/565909D0/57751000)
    (fp_text reference T44 (at 0 -2.54) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value testpoint (at 1.27 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(T44-Pad1)"))
  )

  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 0) (tstamp 57757CEE)
    (at 406.90148 99.166361)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (path /5659094D/565909D0/57750CEC)
    (fp_text reference T45 (at 0 -2.54) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value testpoint (at 1.27 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(T45-Pad1)"))
  )

  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 0) (tstamp 57757CF3)
    (at 418.30148 83.366361)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (path /5659094D/565909D0/5775117B)
    (fp_text reference T46 (at 0 -2.54) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value testpoint (at 1.27 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(T46-Pad1)"))
  )

  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 53DE8DE3) (tstamp 57757CFD)
    (at 437.964336 35.226361)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (path /56590966/56591913/5667D8FF)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USBLC6-4SC6 (at 0 2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center -0.4 -1.7) (end -0.3 -1.7) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 -1.45) (end -0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 1.45) (end 0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 1.45) (end 0.25 1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 -1.45) (end -0.25 1.45) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(P1-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 169 /ctrl/FB1/A78))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 168 /ctrl/FB0/A78))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stmbl:SOT-223 (layer F.Cu) (tedit 56D705E3) (tstamp 57757D05)
    (at 442.631766 122.108362)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (path /56590966/56591916/566074A9)
    (attr smd)
    (fp_text reference U2 (at 0 -0.762) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value zldo1117 (at 0 0.762) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.556 1.524) (end -3.556 4.572) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.556 4.572) (end 3.556 4.572) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.556 4.572) (end 3.556 1.524) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.556 -1.524) (end -3.556 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.556 -2.286) (end -2.032 -4.572) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 -4.572) (end 2.032 -4.572) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.032 -4.572) (end 3.556 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.556 -2.286) (end 3.556 -1.524) (layer F.SilkS) (width 0.15))
    (pad 2 smd rect (at 0 -3.302) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 2 smd rect (at 0 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 3 smd rect (at 2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 1 smd rect (at -2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 53DE8DE3) (tstamp 57757DEB)
    (at 410.314336 83.726361)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (path /5659094D/565909D0/566A7439)
    (attr smd)
    (fp_text reference U20 (at 0 -2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USBLC6-4SC6 (at 0 2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center -0.4 -1.7) (end -0.3 -1.7) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 -1.45) (end -0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 1.45) (end 0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 1.45) (end 0.25 1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 -1.45) (end -0.25 1.45) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 /hv/f3/A_U))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 /hv/f3/A_V))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 29 /hv/f3/A_HV))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 17 /hv/f3/A_W))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 53DE8DE3) (tstamp 57757DF5)
    (at 410.314336 91.626361)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (path /5659094D/565909D0/56820F0C)
    (attr smd)
    (fp_text reference U21 (at 0 -2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USBLC6-4SC6 (at 0 2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center -0.4 -1.7) (end -0.3 -1.7) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 -1.45) (end -0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 1.45) (end 0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 1.45) (end 0.25 1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 -1.45) (end -0.25 1.45) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 177 /hv/f3/A_T_MOT))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 53DE8DE3) (tstamp 57757DFF)
    (at 339.174336 110.726361)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (path /56590966/56591923/56819D62)
    (attr smd)
    (fp_text reference U22 (at 0 -2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USBLC6-4SC6 (at 0 2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center -0.4 -1.7) (end -0.3 -1.7) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 -1.45) (end -0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 1.45) (end 0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 1.45) (end 0.25 1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 -1.45) (end -0.25 1.45) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 53DE8DE3) (tstamp 57757E09)
    (at 369.154336 83.726361)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (path /56590966/56591923/56819DA2)
    (attr smd)
    (fp_text reference U23 (at 0 -2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USBLC6-4SC6 (at 0 2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center -0.4 -1.7) (end -0.3 -1.7) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 -1.45) (end -0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 1.45) (end 0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 1.45) (end 0.25 1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 -1.45) (end -0.25 1.45) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 53DE8DE3) (tstamp 57757E13)
    (at 339.174336 102.826361)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (path /56590966/56591923/56819DFD)
    (attr smd)
    (fp_text reference U24 (at 0 -2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USBLC6-4SC6 (at 0 2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center -0.4 -1.7) (end -0.3 -1.7) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 -1.45) (end -0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 1.45) (end 0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 1.45) (end 0.25 1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 -1.45) (end -0.25 1.45) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77) (tstamp 57757E47)
    (at 249 109.5 90)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (path /5659094D/565909D0/570DA682)
    (attr smd)
    (fp_text reference U25 (at 0 -6 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value STM32F303CBTx (at 0 6 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -5.25 -5.25) (end -5.25 5.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.25 -5.25) (end 5.25 5.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.25 -5.25) (end 5.25 -5.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.25 5.25) (end 5.25 5.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.625 -3.625) (end -3.625 -3.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.625 -3.625) (end 3.625 -3.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.625 3.625) (end 3.625 3.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.625 3.625) (end -3.625 3.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.625 -3.625) (end -3.1 -3.625) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.625 3.625) (end -3.1 3.625) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.625 3.625) (end 3.1 3.625) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.625 -3.625) (end 3.1 -3.625) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.625 -3.1) (end -5 -3.1) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.35 -2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (pad 2 smd rect (at -4.35 -2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -4.35 -1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (pad 6 smd rect (at -4.35 -0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (pad 7 smd rect (at -4.35 0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 174 /hv/f3/NRST))
    (pad 8 smd rect (at -4.35 0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (pad 9 smd rect (at -4.35 1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(C83-Pad2)"))
    (pad 10 smd rect (at -4.35 1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -4.35 2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -4.35 2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(T44-Pad1)"))
    (pad 13 smd rect (at -2.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(T45-Pad1)"))
    (pad 15 smd rect (at -1.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(T46-Pad1)"))
    (pad 17 smd rect (at -0.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(T1-Pad1)"))
    (pad 20 smd rect (at 0.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 112 /hv/f3/HV_TX))
    (pad 22 smd rect (at 1.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 90 /hv/f3/HV_RX))
    (pad 23 smd rect (at 2.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (pad 24 smd rect (at 2.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (pad 25 smd rect (at 4.35 2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 4.35 2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 4.35 1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 4.35 1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at 4.35 0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(D1-Pad2)"))
    (pad 30 smd rect (at 4.35 0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 31 smd rect (at 4.35 -0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 32 smd rect (at 4.35 -0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 33 smd rect (at 4.35 -1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd rect (at 4.35 -1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 180 /hv/f3/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (pad 36 smd rect (at 4.35 -2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (pad 37 smd rect (at 2.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 179 /hv/f3/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(R129-Pad2)"))
    (pad 39 smd rect (at 1.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 128 /hv/f3/CH1N))
    (pad 40 smd rect (at 1.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 129 /hv/f3/CH2N))
    (pad 41 smd rect (at 0.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 132 /hv/f3/CH3N))
    (pad 42 smd rect (at 0.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 130 /hv/f3/CH1))
    (pad 43 smd rect (at -0.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 110 /hv/f3/HV_EN))
    (pad 44 smd rect (at -0.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(JP1-Pad2)"))
    (pad 45 smd rect (at -1.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 133 /hv/f3/CH2))
    (pad 46 smd rect (at -1.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 131 /hv/f3/CH3))
    (pad 47 smd rect (at -2.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (pad 48 smd rect (at -2.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stmbl:Crystal_SMD_0603_4Pads (layer F.Cu) (tedit 56D33537) (tstamp 57757EB7)
    (at 400.080835 100.486361)
    (descr "Crystal, Quarz, SMD, 0603, 4 Pads,")
    (tags "Crystal, Quarz, SMD, 0603, 4 Pads,")
    (path /5659094D/565909D0/56631593)
    (attr smd)
    (fp_text reference Y1 (at 0 -3.81) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 8M (at 0 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.50038 0) (layer F.Adhes) (width 0.381))
    (fp_circle (center 0 0) (end 0.14986 0) (layer F.Adhes) (width 0.381))
    (fp_circle (center -0.50038 0.94996) (end -0.39878 1.04902) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.70104 1.84912) (end -0.70104 1.84912) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.70104 -1.84912) (end 0.70104 -1.84912) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.19964 1.19888) (size 1.80086 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (pad 3 smd rect (at 2.19964 1.19888) (size 1.80086 1.39954) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 2.19964 -1.19888) (size 1.80086 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (pad 3 smd rect (at -2.19964 -1.19888) (size 1.80086 1.39954) (layers F.Cu F.Paste F.Mask))
  )

  (module stmbl:Crystal_SMD_0603_4Pads (layer F.Cu) (tedit 56D33537) (tstamp 57757EBF)
    (at 452.734896 14.736361)
    (descr "Crystal, Quarz, SMD, 0603, 4 Pads,")
    (tags "Crystal, Quarz, SMD, 0603, 4 Pads,")
    (path /56590966/56591913/565FDF0A)
    (attr smd)
    (fp_text reference Y2 (at 0 -3.81) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 8M (at 0 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.50038 0) (layer F.Adhes) (width 0.381))
    (fp_circle (center 0 0) (end 0.14986 0) (layer F.Adhes) (width 0.381))
    (fp_circle (center -0.50038 0.94996) (end -0.39878 1.04902) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.70104 1.84912) (end -0.70104 1.84912) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.70104 -1.84912) (end 0.70104 -1.84912) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.19964 1.19888) (size 1.80086 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C31-Pad1)"))
    (pad 3 smd rect (at 2.19964 1.19888) (size 1.80086 1.39954) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 2.19964 -1.19888) (size 1.80086 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C32-Pad1)"))
    (pad 3 smd rect (at -2.19964 -1.19888) (size 1.80086 1.39954) (layers F.Cu F.Paste F.Mask))
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 5415D3E2) (tstamp 57755E0E)
    (at 223 109.5 270)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5659094D/56590A75/5668E2F9)
    (attr smd)
    (fp_text reference R80 (at 0 -3.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.002 (at 0 3.1 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.9 -1.95) (end 3.9 -1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.9 1.95) (end 3.9 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.9 -1.95) (end -3.9 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.9 -1.95) (end 3.9 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.6 1.825) (end -2.6 1.825) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.6 -1.825) (end 2.6 -1.825) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -3.1 0 270) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 75 /hv/driver/CUH))
    (pad 2 smd rect (at 3.1 0 270) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 5415D3E2) (tstamp 57755E13)
    (at 227 109.5 270)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5659094D/56590A75/5668E493)
    (attr smd)
    (fp_text reference R81 (at 0 -3.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.002 (at 0 3.1 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.9 -1.95) (end 3.9 -1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.9 1.95) (end 3.9 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.9 -1.95) (end -3.9 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.9 -1.95) (end 3.9 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.6 1.825) (end -2.6 1.825) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.6 -1.825) (end 2.6 -1.825) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -3.1 0 270) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 92 /hv/driver/CVH))
    (pad 2 smd rect (at 3.1 0 270) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 5415D3E2) (tstamp 57755E18)
    (at 231 109.5 270)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5659094D/56590A75/5668E4D6)
    (attr smd)
    (fp_text reference R82 (at 0 -3.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.002 (at 0 3.1 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.9 -1.95) (end 3.9 -1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.9 1.95) (end 3.9 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.9 -1.95) (end -3.9 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.9 -1.95) (end 3.9 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.6 1.825) (end -2.6 1.825) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.6 -1.825) (end 2.6 -1.825) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -3.1 0 270) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 93 /hv/driver/CWH))
    (pad 2 smd rect (at 3.1 0 270) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5415CFA7) (tstamp 57756C66)
    (at 214.5 106.5 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (path /5659094D/56590A3E/566960D3)
    (attr smd)
    (fp_text reference R27 (at 0 -2.3 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 250k (at 0 2.3 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 -1.2) (end 2.2 -1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -1.2) (end -2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.2 -1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 1.075) (end -1 1.075) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 -1.075) (end 1 -1.075) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 37 /hv/back-emf/U))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R27-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5415CFA7) (tstamp 57756C75)
    (at 210.25 111 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (path /5659094D/56590A3E/56696293)
    (attr smd)
    (fp_text reference R33 (at 0 -2.3 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 250k (at 0 2.3 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 -1.2) (end 2.2 -1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -1.2) (end -2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.2 -1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 1.075) (end -1 1.075) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 -1.075) (end 1 -1.075) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R32-Pad2)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 /hv/f3/A_V))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5415CFA7) (tstamp 57756C7A)
    (at 206 106.5 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (path /5659094D/56590A3E/56696338)
    (attr smd)
    (fp_text reference R51 (at 0 -2.3 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 250k (at 0 2.3 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 -1.2) (end 2.2 -1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -1.2) (end -2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.2 -1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 1.075) (end -1 1.075) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 -1.075) (end 1 -1.075) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 33 /hv/back-emf/W))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(R51-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5415CFA7) (tstamp 57756C7F)
    (at 206 111 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (path /5659094D/56590A3E/5669633E)
    (attr smd)
    (fp_text reference R52 (at 0 -2.3 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 250k (at 0 2.3 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 -1.2) (end 2.2 -1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -1.2) (end -2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.2 -1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 1.075) (end -1 1.075) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 -1.075) (end 1 -1.075) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(R51-Pad2)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /hv/f3/A_W))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5415CFA7) (tstamp 57756C84)
    (at 235.5 124.5)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (path /5659094D/56590A3E/566963D7)
    (attr smd)
    (fp_text reference R77 (at 0 -2.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 250k (at 0 2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 -1.2) (end 2.2 -1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -1.2) (end -2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.2 -1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 1.075) (end -1 1.075) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 -1.075) (end 1 -1.075) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 VPP))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(R77-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5415CFA7) (tstamp 57756C89)
    (at 237.5 121.25 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (path /5659094D/56590A3E/566963DD)
    (attr smd)
    (fp_text reference R78 (at 0 -2.3 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 250k (at 0 2.3 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 -1.2) (end 2.2 -1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -1.2) (end -2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.2 -1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 1.075) (end -1 1.075) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 -1.075) (end 1 -1.075) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(R77-Pad2)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 /hv/f3/A_HV))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stmbl:C_Radial_D26_L45_P10 (layer B.Cu) (tedit 5775699A) (tstamp 577576C4)
    (at 208.5 119.5 135)
    (descr "Radial Electrolytic Capacitor Diameter 26mm x Length 45mm, Pitch 10mm")
    (tags "Electrolytic Capacitor")
    (path /5659094D/56590A75/56590CD1)
    (fp_text reference C22 (at 0 14.3 135) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 270µ (at 0 -14.3 135) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 0.075 13) (end 0.075 -13) (layer B.SilkS) (width 0.15))
    (fp_line (start 0.215 12.998) (end 0.215 -12.998) (layer B.SilkS) (width 0.15))
    (fp_line (start 0.355 12.995) (end 0.355 -12.995) (layer B.SilkS) (width 0.15))
    (fp_line (start 0.495 12.991) (end 0.495 -12.991) (layer B.SilkS) (width 0.15))
    (fp_line (start 0.635 12.984) (end 0.635 -12.984) (layer B.SilkS) (width 0.15))
    (fp_line (start 0.775 12.977) (end 0.775 -12.977) (layer B.SilkS) (width 0.15))
    (fp_line (start 0.915 12.968) (end 0.915 -12.968) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.055 12.957) (end 1.055 -12.957) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.195 12.945) (end 1.195 -12.945) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.335 12.931) (end 1.335 -12.931) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.475 12.916) (end 1.475 -12.916) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.615 12.899) (end 1.615 -12.899) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.755 12.881) (end 1.755 -12.881) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.895 12.861) (end 1.895 -12.861) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.035 12.84) (end 2.035 -12.84) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.175 12.817) (end 2.175 -12.817) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.315 12.792) (end 2.315 -12.792) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.455 12.766) (end 2.455 -12.766) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.595 12.738) (end 2.595 -12.738) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.735 12.709) (end 2.735 -12.709) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.875 12.678) (end 2.875 -12.678) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.015 12.646) (end 3.015 -12.646) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.155 12.611) (end 3.155 -12.611) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.295 12.575) (end 3.295 -12.575) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.435 12.538) (end 3.435 -12.538) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.575 12.499) (end 3.575 -12.499) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.715 12.458) (end 3.715 -12.458) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.855 12.415) (end 3.855 0.107) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.855 -0.107) (end 3.855 -12.415) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.995 12.371) (end 3.995 0.559) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.995 -0.559) (end 3.995 -12.371) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.135 12.325) (end 4.135 0.758) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.135 -0.758) (end 4.135 -12.325) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.275 12.277) (end 4.275 0.893) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.275 -0.893) (end 4.275 -12.277) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.415 12.227) (end 4.415 0.99) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.415 -0.99) (end 4.415 -12.227) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.555 12.176) (end 4.555 1.06) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.555 -1.06) (end 4.555 -12.176) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.695 12.123) (end 4.695 1.109) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.695 -1.109) (end 4.695 -12.123) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.835 12.067) (end 4.835 1.138) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.835 -1.138) (end 4.835 -12.067) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.975 12.01) (end 4.975 1.15) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.975 -1.15) (end 4.975 -12.01) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.115 11.951) (end 5.115 1.144) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.115 -1.144) (end 5.115 -11.951) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.255 11.891) (end 5.255 1.121) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.255 -1.121) (end 5.255 -11.891) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.395 11.828) (end 5.395 1.08) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.395 -1.08) (end 5.395 -11.828) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.535 11.763) (end 5.535 1.018) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.535 -1.018) (end 5.535 -11.763) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.675 11.696) (end 5.675 0.931) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.675 -0.931) (end 5.675 -11.696) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.815 11.627) (end 5.815 0.811) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.815 -0.811) (end 5.815 -11.627) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.955 11.556) (end 5.955 0.641) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.955 -0.641) (end 5.955 -11.556) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.095 11.483) (end 6.095 0.351) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.095 -0.351) (end 6.095 -11.483) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.235 11.407) (end 6.235 -11.407) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.375 11.33) (end 6.375 -11.33) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.515 11.25) (end 6.515 -11.25) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.655 11.167) (end 6.655 -11.167) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.795 11.083) (end 6.795 -11.083) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.935 10.996) (end 6.935 -10.996) (layer B.SilkS) (width 0.15))
    (fp_line (start 7.075 10.906) (end 7.075 -10.906) (layer B.SilkS) (width 0.15))
    (fp_line (start 7.215 10.814) (end 7.215 -10.814) (layer B.SilkS) (width 0.15))
    (fp_line (start 7.355 10.719) (end 7.355 -10.719) (layer B.SilkS) (width 0.15))
    (fp_line (start 7.495 10.622) (end 7.495 -10.622) (layer B.SilkS) (width 0.15))
    (fp_line (start 7.635 10.522) (end 7.635 -10.522) (layer B.SilkS) (width 0.15))
    (fp_line (start 7.775 10.419) (end 7.775 -10.419) (layer B.SilkS) (width 0.15))
    (fp_line (start 7.915 10.313) (end 7.915 -10.313) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.055 10.204) (end 8.055 -10.204) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.195 10.092) (end 8.195 -10.092) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.335 9.976) (end 8.335 -9.976) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.475 9.858) (end 8.475 -9.858) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.615 9.736) (end 8.615 -9.736) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.755 9.61) (end 8.755 -9.61) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.895 9.48) (end 8.895 -9.48) (layer B.SilkS) (width 0.15))
    (fp_line (start 9.035 9.347) (end 9.035 -9.347) (layer B.SilkS) (width 0.15))
    (fp_line (start 9.175 9.21) (end 9.175 -9.21) (layer B.SilkS) (width 0.15))
    (fp_line (start 9.315 9.068) (end 9.315 -9.068) (layer B.SilkS) (width 0.15))
    (fp_line (start 9.455 8.922) (end 9.455 -8.922) (layer B.SilkS) (width 0.15))
    (fp_line (start 9.595 8.771) (end 9.595 -8.771) (layer B.SilkS) (width 0.15))
    (fp_line (start 9.735 8.616) (end 9.735 -8.616) (layer B.SilkS) (width 0.15))
    (fp_line (start 9.875 8.455) (end 9.875 -8.455) (layer B.SilkS) (width 0.15))
    (fp_line (start 10.015 8.289) (end 10.015 -8.289) (layer B.SilkS) (width 0.15))
    (fp_line (start 10.155 8.116) (end 10.155 -8.116) (layer B.SilkS) (width 0.15))
    (fp_line (start 10.295 7.938) (end 10.295 -7.938) (layer B.SilkS) (width 0.15))
    (fp_line (start 10.435 7.753) (end 10.435 -7.753) (layer B.SilkS) (width 0.15))
    (fp_line (start 10.575 7.561) (end 10.575 -7.561) (layer B.SilkS) (width 0.15))
    (fp_line (start 10.715 7.361) (end 10.715 -7.361) (layer B.SilkS) (width 0.15))
    (fp_line (start 10.855 7.153) (end 10.855 -7.153) (layer B.SilkS) (width 0.15))
    (fp_line (start 10.995 6.936) (end 10.995 -6.936) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.135 6.709) (end 11.135 -6.709) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.275 6.471) (end 11.275 -6.471) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.415 6.221) (end 11.415 -6.221) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.555 5.957) (end 11.555 -5.957) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.695 5.677) (end 11.695 -5.677) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.835 5.379) (end 11.835 -5.379) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.975 5.06) (end 11.975 -5.06) (layer B.SilkS) (width 0.15))
    (fp_line (start 12.115 4.715) (end 12.115 -4.715) (layer B.SilkS) (width 0.15))
    (fp_line (start 12.255 4.338) (end 12.255 -4.338) (layer B.SilkS) (width 0.15))
    (fp_line (start 12.395 3.92) (end 12.395 -3.92) (layer B.SilkS) (width 0.15))
    (fp_line (start 12.535 3.446) (end 12.535 -3.446) (layer B.SilkS) (width 0.15))
    (fp_line (start 12.675 2.889) (end 12.675 -2.889) (layer B.SilkS) (width 0.15))
    (fp_line (start 12.815 2.185) (end 12.815 -2.185) (layer B.SilkS) (width 0.15))
    (fp_line (start 12.955 1.081) (end 12.955 -1.081) (layer B.SilkS) (width 0.15))
    (fp_circle (center 5 0) (end 5 1.15) (layer B.SilkS) (width 0.15))
    (fp_circle (center 0 0) (end 0 13.0375) (layer B.SilkS) (width 0.15))
    (fp_circle (center 0 0) (end 0 13.3) (layer B.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at -5 0 135) (size 2 2) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 16 VPP))
    (pad 2 thru_hole circle (at 5 0 135) (size 2 2) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 4 GNDPWR))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D26_L45_P10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module stmbl:C_Radial_D26_L45_P10 (layer B.Cu) (tedit 5775699A) (tstamp 577576BE)
    (at 235.5 119.5 45)
    (descr "Radial Electrolytic Capacitor Diameter 26mm x Length 45mm, Pitch 10mm")
    (tags "Electrolytic Capacitor")
    (path /5659094D/56590A75/56590C91)
    (fp_text reference C21 (at 0 14.3 45) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 270µ (at 0 -14.3 45) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 0.075 13) (end 0.075 -13) (layer B.SilkS) (width 0.15))
    (fp_line (start 0.215 12.998) (end 0.215 -12.998) (layer B.SilkS) (width 0.15))
    (fp_line (start 0.355 12.995) (end 0.355 -12.995) (layer B.SilkS) (width 0.15))
    (fp_line (start 0.495 12.991) (end 0.495 -12.991) (layer B.SilkS) (width 0.15))
    (fp_line (start 0.635 12.984) (end 0.635 -12.984) (layer B.SilkS) (width 0.15))
    (fp_line (start 0.775 12.977) (end 0.775 -12.977) (layer B.SilkS) (width 0.15))
    (fp_line (start 0.915 12.968) (end 0.915 -12.968) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.055 12.957) (end 1.055 -12.957) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.195 12.945) (end 1.195 -12.945) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.335 12.931) (end 1.335 -12.931) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.475 12.916) (end 1.475 -12.916) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.615 12.899) (end 1.615 -12.899) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.755 12.881) (end 1.755 -12.881) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.895 12.861) (end 1.895 -12.861) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.035 12.84) (end 2.035 -12.84) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.175 12.817) (end 2.175 -12.817) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.315 12.792) (end 2.315 -12.792) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.455 12.766) (end 2.455 -12.766) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.595 12.738) (end 2.595 -12.738) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.735 12.709) (end 2.735 -12.709) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.875 12.678) (end 2.875 -12.678) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.015 12.646) (end 3.015 -12.646) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.155 12.611) (end 3.155 -12.611) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.295 12.575) (end 3.295 -12.575) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.435 12.538) (end 3.435 -12.538) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.575 12.499) (end 3.575 -12.499) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.715 12.458) (end 3.715 -12.458) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.855 12.415) (end 3.855 0.107) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.855 -0.107) (end 3.855 -12.415) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.995 12.371) (end 3.995 0.559) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.995 -0.559) (end 3.995 -12.371) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.135 12.325) (end 4.135 0.758) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.135 -0.758) (end 4.135 -12.325) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.275 12.277) (end 4.275 0.893) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.275 -0.893) (end 4.275 -12.277) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.415 12.227) (end 4.415 0.99) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.415 -0.99) (end 4.415 -12.227) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.555 12.176) (end 4.555 1.06) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.555 -1.06) (end 4.555 -12.176) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.695 12.123) (end 4.695 1.109) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.695 -1.109) (end 4.695 -12.123) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.835 12.067) (end 4.835 1.138) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.835 -1.138) (end 4.835 -12.067) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.975 12.01) (end 4.975 1.15) (layer B.SilkS) (width 0.15))
    (fp_line (start 4.975 -1.15) (end 4.975 -12.01) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.115 11.951) (end 5.115 1.144) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.115 -1.144) (end 5.115 -11.951) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.255 11.891) (end 5.255 1.121) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.255 -1.121) (end 5.255 -11.891) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.395 11.828) (end 5.395 1.08) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.395 -1.08) (end 5.395 -11.828) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.535 11.763) (end 5.535 1.018) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.535 -1.018) (end 5.535 -11.763) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.675 11.696) (end 5.675 0.931) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.675 -0.931) (end 5.675 -11.696) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.815 11.627) (end 5.815 0.811) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.815 -0.811) (end 5.815 -11.627) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.955 11.556) (end 5.955 0.641) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.955 -0.641) (end 5.955 -11.556) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.095 11.483) (end 6.095 0.351) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.095 -0.351) (end 6.095 -11.483) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.235 11.407) (end 6.235 -11.407) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.375 11.33) (end 6.375 -11.33) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.515 11.25) (end 6.515 -11.25) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.655 11.167) (end 6.655 -11.167) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.795 11.083) (end 6.795 -11.083) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.935 10.996) (end 6.935 -10.996) (layer B.SilkS) (width 0.15))
    (fp_line (start 7.075 10.906) (end 7.075 -10.906) (layer B.SilkS) (width 0.15))
    (fp_line (start 7.215 10.814) (end 7.215 -10.814) (layer B.SilkS) (width 0.15))
    (fp_line (start 7.355 10.719) (end 7.355 -10.719) (layer B.SilkS) (width 0.15))
    (fp_line (start 7.495 10.622) (end 7.495 -10.622) (layer B.SilkS) (width 0.15))
    (fp_line (start 7.635 10.522) (end 7.635 -10.522) (layer B.SilkS) (width 0.15))
    (fp_line (start 7.775 10.419) (end 7.775 -10.419) (layer B.SilkS) (width 0.15))
    (fp_line (start 7.915 10.313) (end 7.915 -10.313) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.055 10.204) (end 8.055 -10.204) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.195 10.092) (end 8.195 -10.092) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.335 9.976) (end 8.335 -9.976) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.475 9.858) (end 8.475 -9.858) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.615 9.736) (end 8.615 -9.736) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.755 9.61) (end 8.755 -9.61) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.895 9.48) (end 8.895 -9.48) (layer B.SilkS) (width 0.15))
    (fp_line (start 9.035 9.347) (end 9.035 -9.347) (layer B.SilkS) (width 0.15))
    (fp_line (start 9.175 9.21) (end 9.175 -9.21) (layer B.SilkS) (width 0.15))
    (fp_line (start 9.315 9.068) (end 9.315 -9.068) (layer B.SilkS) (width 0.15))
    (fp_line (start 9.455 8.922) (end 9.455 -8.922) (layer B.SilkS) (width 0.15))
    (fp_line (start 9.595 8.771) (end 9.595 -8.771) (layer B.SilkS) (width 0.15))
    (fp_line (start 9.735 8.616) (end 9.735 -8.616) (layer B.SilkS) (width 0.15))
    (fp_line (start 9.875 8.455) (end 9.875 -8.455) (layer B.SilkS) (width 0.15))
    (fp_line (start 10.015 8.289) (end 10.015 -8.289) (layer B.SilkS) (width 0.15))
    (fp_line (start 10.155 8.116) (end 10.155 -8.116) (layer B.SilkS) (width 0.15))
    (fp_line (start 10.295 7.938) (end 10.295 -7.938) (layer B.SilkS) (width 0.15))
    (fp_line (start 10.435 7.753) (end 10.435 -7.753) (layer B.SilkS) (width 0.15))
    (fp_line (start 10.575 7.561) (end 10.575 -7.561) (layer B.SilkS) (width 0.15))
    (fp_line (start 10.715 7.361) (end 10.715 -7.361) (layer B.SilkS) (width 0.15))
    (fp_line (start 10.855 7.153) (end 10.855 -7.153) (layer B.SilkS) (width 0.15))
    (fp_line (start 10.995 6.936) (end 10.995 -6.936) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.135 6.709) (end 11.135 -6.709) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.275 6.471) (end 11.275 -6.471) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.415 6.221) (end 11.415 -6.221) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.555 5.957) (end 11.555 -5.957) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.695 5.677) (end 11.695 -5.677) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.835 5.379) (end 11.835 -5.379) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.975 5.06) (end 11.975 -5.06) (layer B.SilkS) (width 0.15))
    (fp_line (start 12.115 4.715) (end 12.115 -4.715) (layer B.SilkS) (width 0.15))
    (fp_line (start 12.255 4.338) (end 12.255 -4.338) (layer B.SilkS) (width 0.15))
    (fp_line (start 12.395 3.92) (end 12.395 -3.92) (layer B.SilkS) (width 0.15))
    (fp_line (start 12.535 3.446) (end 12.535 -3.446) (layer B.SilkS) (width 0.15))
    (fp_line (start 12.675 2.889) (end 12.675 -2.889) (layer B.SilkS) (width 0.15))
    (fp_line (start 12.815 2.185) (end 12.815 -2.185) (layer B.SilkS) (width 0.15))
    (fp_line (start 12.955 1.081) (end 12.955 -1.081) (layer B.SilkS) (width 0.15))
    (fp_circle (center 5 0) (end 5 1.15) (layer B.SilkS) (width 0.15))
    (fp_circle (center 0 0) (end 0 13.0375) (layer B.SilkS) (width 0.15))
    (fp_circle (center 0 0) (end 0 13.3) (layer B.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at -5 0 45) (size 2 2) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 16 VPP))
    (pad 2 thru_hole circle (at 5 0 45) (size 2 2) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 4 GNDPWR))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D26_L45_P10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 0) (tstamp 5775BD34)
    (at 304.25 78.5)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /56590966/56591923/5660223A)
    (fp_text reference P7 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 6.85) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 6.35) (end 1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 6.35) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 152 "Net-(D7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(D7-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Socket_Strips:Socket_Strip_Angled_2x07 (layer B.Cu) (tedit 0) (tstamp 5775BD35)
    (at 215 46.54)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (path /56590966/56591923/57771E76)
    (fp_text reference P10 (at 0 4.6) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value CONN_02X07 (at 0 2.6) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -1.75 1.35) (end -1.75 -13.15) (layer B.CrtYd) (width 0.05))
    (fp_line (start 17 1.35) (end 17 -13.15) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.75 1.35) (end 17 1.35) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.75 -13.15) (end 17 -13.15) (layer B.CrtYd) (width 0.05))
    (fp_line (start 16.51 -3.81) (end 16.51 -12.64) (layer B.SilkS) (width 0.15))
    (fp_line (start 13.97 -3.81) (end 16.51 -3.81) (layer B.SilkS) (width 0.15))
    (fp_line (start 13.97 -12.64) (end 16.51 -12.64) (layer B.SilkS) (width 0.15))
    (fp_line (start 16.51 -12.64) (end 16.51 -3.81) (layer B.SilkS) (width 0.15))
    (fp_line (start 13.97 -12.64) (end 13.97 -3.81) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.43 -12.64) (end 13.97 -12.64) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.43 -3.81) (end 13.97 -3.81) (layer B.SilkS) (width 0.15))
    (fp_line (start 13.97 -3.81) (end 13.97 -12.64) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.43 -3.81) (end 11.43 -12.64) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.89 -3.81) (end 11.43 -3.81) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.89 -12.64) (end 11.43 -12.64) (layer B.SilkS) (width 0.15))
    (fp_line (start 11.43 -12.64) (end 11.43 -3.81) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.89 -12.64) (end 8.89 -3.81) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.35 -12.64) (end 8.89 -12.64) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.35 -3.81) (end 8.89 -3.81) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.89 -3.81) (end 8.89 -12.64) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.35 -3.81) (end 6.35 -12.64) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.81 -3.81) (end 6.35 -3.81) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.81 -12.64) (end 6.35 -12.64) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.35 -12.64) (end 6.35 -3.81) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.81 -12.64) (end 3.81 -3.81) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.27 -12.64) (end 3.81 -12.64) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.27 -3.81) (end 3.81 -3.81) (layer B.SilkS) (width 0.15))
    (fp_line (start 3.81 -3.81) (end 3.81 -12.64) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.27 -3.81) (end 1.27 -12.64) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.27 -3.81) (end 1.27 -3.81) (layer B.SilkS) (width 0.15))
    (fp_line (start 0 1.15) (end -1.55 1.15) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.55 1.15) (end -1.55 0) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.27 -3.81) (end -1.27 -12.64) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.27 -12.64) (end 1.27 -12.64) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.27 -12.64) (end 1.27 -3.81) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 5 thru_hole oval (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 6 thru_hole oval (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 7 thru_hole oval (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 8 thru_hole oval (at 7.62 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 9 thru_hole oval (at 10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 10 thru_hole oval (at 10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 11 thru_hole oval (at 12.7 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 12 thru_hole oval (at 12.7 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 13 thru_hole oval (at 15.24 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 14 thru_hole oval (at 15.24 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (model Socket_Strips.3dshapes/Socket_Strip_Angled_2x07.wrl
      (at (xyz 0.3 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module stmbl:C_1808 (layer F.Cu) (tedit 5775A534) (tstamp 5775CB50)
    (at 226 119.25 90)
    (descr "Capacitor SMD 1808, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1808")
    (path /5659094D/56590A75/56590D2C)
    (attr smd)
    (fp_text reference C28 (at 0 -2 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 150n (at 0 2 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.1 -1.25) (end 3.1 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 1.25) (end 3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 -1.25) (end -3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.1 -1.25) (end 3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.2) (end -1.8 -1.2) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.8 1.2) (end 1.8 1.2) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.3 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 16 VPP))
    (pad 2 smd rect (at 2.3 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stmbl:C_1808 (layer F.Cu) (tedit 5775A534) (tstamp 5775CB5B)
    (at 222.5 119.25 90)
    (descr "Capacitor SMD 1808, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1808")
    (path /5659094D/56590A75/56590D5B)
    (attr smd)
    (fp_text reference C34 (at 0 -2 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 150n (at 0 2 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.1 -1.25) (end 3.1 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 1.25) (end 3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 -1.25) (end -3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.1 -1.25) (end 3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.2) (end -1.8 -1.2) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.8 1.2) (end 1.8 1.2) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.3 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 16 VPP))
    (pad 2 smd rect (at 2.3 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stmbl:C_1808 (layer F.Cu) (tedit 5775A534) (tstamp 5775D965)
    (at 219 119.25 90)
    (descr "Capacitor SMD 1808, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1808")
    (path /5659094D/56590A75/57779550)
    (attr smd)
    (fp_text reference C38 (at 0 -2 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 150n (at 0 2 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.1 -1.25) (end 3.1 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 1.25) (end 3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 -1.25) (end -3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.1 -1.25) (end 3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.2) (end -1.8 -1.2) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.8 1.2) (end 1.8 1.2) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.3 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 16 VPP))
    (pad 2 smd rect (at 2.3 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stmbl:C_1808 (layer F.Cu) (tedit 5775A534) (tstamp 5775EBFA)
    (at 215.5 119.25 90)
    (descr "Capacitor SMD 1808, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1808")
    (path /5659094D/56590A75/5777A5B0)
    (attr smd)
    (fp_text reference C92 (at 0 -2 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 150n (at 0 2 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.1 -1.25) (end 3.1 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 1.25) (end 3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 -1.25) (end -3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.1 -1.25) (end 3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.2) (end -1.8 -1.2) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.8 1.2) (end 1.8 1.2) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.3 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 16 VPP))
    (pad 2 smd rect (at 2.3 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stmbl:C_1808 (layer F.Cu) (tedit 5775A534) (tstamp 5775EC06)
    (at 229.5 119.25 90)
    (descr "Capacitor SMD 1808, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1808")
    (path /5659094D/56590A75/5777A039)
    (attr smd)
    (fp_text reference C93 (at 0 -2 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 150n (at 0 2 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.1 -1.25) (end 3.1 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 1.25) (end 3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 -1.25) (end -3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.1 -1.25) (end 3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.2) (end -1.8 -1.2) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.8 1.2) (end 1.8 1.2) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.3 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 16 VPP))
    (pad 2 smd rect (at 2.3 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stmbl:C_1808 (layer F.Cu) (tedit 5775A534) (tstamp 5775F9FE)
    (at 218.75 110.25 270)
    (descr "Capacitor SMD 1808, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1808")
    (path /5659094D/56590A75/5777B413)
    (attr smd)
    (fp_text reference C94 (at 0 -2 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 150n (at 0 2 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.1 -1.25) (end 3.1 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 1.25) (end 3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 -1.25) (end -3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.1 -1.25) (end 3.1 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.2) (end -1.8 -1.2) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.8 1.2) (end 1.8 1.2) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.3 0 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 16 VPP))
    (pad 2 smd rect (at 2.3 0 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:SMA_Standard (layer F.Cu) (tedit 552FF239) (tstamp 577AF731)
    (at 311.826596 68.735904)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (path /5659094D/565909D4/56657C30)
    (attr smd)
    (fp_text reference D10 (at 0 -3.81) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value STTH1L06A (at 0 4.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.5 -2) (end 3.5 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.5 -2) (end 3.5 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.5 2) (end -3.5 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.5 2) (end -3.5 -2) (layer F.CrtYd) (width 0.05))
    (fp_text user K (at -2.9 2.95) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user A (at 2.9 2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.20066 -0.0508) (layer F.Adhes) (width 0.381))
    (fp_line (start -1.79914 1.75006) (end -1.79914 1.39954) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.79914 -1.75006) (end -1.79914 -1.39954) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.25044 1.75006) (end 2.25044 1.39954) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.25044 1.75006) (end -2.25044 1.39954) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.25044 -1.75006) (end -2.25044 -1.39954) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.25044 -1.75006) (end 2.25044 -1.39954) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.25044 1.75006) (end 2.25044 1.75006) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.25044 -1.75006) (end 2.25044 -1.75006) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.99898 0) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C41-Pad2)"))
    (pad 2 smd rect (at 1.99898 0) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Diodes_SMD.3dshapes/SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )

  (module Diodes_SMD:SMA_Standard (layer F.Cu) (tedit 552FF239) (tstamp 577AF746)
    (at 323.016596 68.735904)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (path /5659094D/565909D4/56657CAE)
    (attr smd)
    (fp_text reference D11 (at 0 -3.81) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value STTH1L06A (at 0 4.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.5 -2) (end 3.5 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.5 -2) (end 3.5 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.5 2) (end -3.5 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.5 2) (end -3.5 -2) (layer F.CrtYd) (width 0.05))
    (fp_text user K (at -2.9 2.95) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user A (at 2.9 2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.20066 -0.0508) (layer F.Adhes) (width 0.381))
    (fp_line (start -1.79914 1.75006) (end -1.79914 1.39954) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.79914 -1.75006) (end -1.79914 -1.39954) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.25044 1.75006) (end 2.25044 1.39954) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.25044 1.75006) (end -2.25044 1.39954) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.25044 -1.75006) (end -2.25044 -1.39954) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.25044 -1.75006) (end 2.25044 -1.39954) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.25044 1.75006) (end 2.25044 1.75006) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.25044 -1.75006) (end 2.25044 -1.75006) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.99898 0) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C51-Pad1)"))
    (pad 2 smd rect (at 1.99898 0) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 46 +15V))
    (model Diodes_SMD.3dshapes/SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 577B06E5)
    (at 425.334336 83.366361)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/565909D0/570E4A7D)
    (attr smd)
    (fp_text reference R129 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 110 /hv/f3/HV_EN))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(R129-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 53DE8DE3) (tstamp 577CC904)
    (at 437.6 137.45)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (path /5659094D/565909D4/578281C8)
    (attr smd)
    (fp_text reference U4 (at 0 -2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ACT4088 (at 0 2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center -0.4 -1.7) (end -0.3 -1.7) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 -1.45) (end -0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 1.45) (end 0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 1.45) (end 0.25 1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 -1.45) (end -0.25 1.45) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C15-Pad2)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 46 +15V))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(R19-Pad1)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(C15-Pad1)"))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5415D7BD) (tstamp 57AC0B2F)
    (at 432.818146 135.186361)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (path /5659094D/565909D4/57B2A7C0)
    (attr smd)
    (fp_text reference C35 (at 0 -2.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10µ (at 0 2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1.15) (end 2.3 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1.15) (end 2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1.15) (end -2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1.15) (end 2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -1.025) (end -1 -1.025) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 1.025) (end 1 1.025) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5415D7BD) (tstamp 57AC0B34)
    (at 447.671955 133.766361)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (path /5659094D/565909D4/57828190)
    (attr smd)
    (fp_text reference C50 (at 0 -2.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10µ (at 0 2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1.15) (end 2.3 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1.15) (end 2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1.15) (end -2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1.15) (end 2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -1.025) (end -1 -1.025) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 1.025) (end 1 1.025) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5415D7BD) (tstamp 57AC0B39)
    (at 421.92005 122.896361)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (path /5659094D/565909D4/5774AD7A)
    (attr smd)
    (fp_text reference C51 (at 0 -2.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10µ (at 0 2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1.15) (end 2.3 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1.15) (end 2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1.15) (end -2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1.15) (end 2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -1.025) (end -1 -1.025) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 1.025) (end 1 1.025) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C51-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C41-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0B3E)
    (at 407.715766 124.376361)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D4/57B2A8C5)
    (attr smd)
    (fp_text reference C60 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0B4D)
    (at 323.5 144)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D4/57B29613)
    (attr smd)
    (fp_text reference C70 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 46 +15V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0B59)
    (at 308 142.75)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591916/57AF3925)
    (attr smd)
    (fp_text reference C96 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0B5F)
    (at 315 144.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591916/57B215DE)
    (attr smd)
    (fp_text reference C97 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 53 +24V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0B65)
    (at 307.75 159.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591916/57B21B07)
    (attr smd)
    (fp_text reference C98 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 53 +24V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0B6B)
    (at 299.25 156)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591916/57AF53FF)
    (attr smd)
    (fp_text reference C99 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0B71)
    (at 297.75 149.25)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591916/57B21B6F)
    (attr smd)
    (fp_text reference C100 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 53 +24V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0B77)
    (at 303 136.25)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591916/57B21BDA)
    (attr smd)
    (fp_text reference C101 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 53 +24V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0B7D)
    (at 303.5 139.75)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591916/57B21C48)
    (attr smd)
    (fp_text reference C102 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 53 +24V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0B83)
    (at 312.75 141.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591916/57AF47AC)
    (attr smd)
    (fp_text reference C103 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 53 +24V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0B89)
    (at 303.25 142.75)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591916/57AF48FA)
    (attr smd)
    (fp_text reference C104 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 53 +24V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0B8F)
    (at 308 146.75)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591916/57AD3DBA)
    (attr smd)
    (fp_text reference C105 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(C105-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(C105-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0B95)
    (at 313 152.25)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591916/57AD27B2)
    (attr smd)
    (fp_text reference C106 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(C106-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(C106-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0B9B)
    (at 298.75 151.25)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591916/57AF42AD)
    (attr smd)
    (fp_text reference C107 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0BA1)
    (at 298.25 146)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591916/57AF3EB7)
    (attr smd)
    (fp_text reference C108 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5415D7BD) (tstamp 57AC0BA7)
    (at 313.25 149)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (path /56590966/56591916/57AD3DA2)
    (attr smd)
    (fp_text reference C109 (at 0 -2.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10µ (at 0 2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1.15) (end 2.3 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1.15) (end 2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1.15) (end -2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1.15) (end 2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -1.025) (end -1 -1.025) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 1.025) (end 1 1.025) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5415D7BD) (tstamp 57AC0BAD)
    (at 303 145.75)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (path /56590966/56591916/57AD279A)
    (attr smd)
    (fp_text reference C110 (at 0 -2.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10µ (at 0 2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1.15) (end 2.3 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1.15) (end 2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1.15) (end -2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1.15) (end 2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -1.025) (end -1 -1.025) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 1.025) (end 1 1.025) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5415D7BD) (tstamp 57AC0BB3)
    (at 315.75 160)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (path /56590966/56591916/57AF630D)
    (attr smd)
    (fp_text reference C111 (at 0 -2.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10µ (at 0 2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1.15) (end 2.3 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1.15) (end 2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1.15) (end -2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1.15) (end 2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -1.025) (end -1 -1.025) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 1.025) (end 1 1.025) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0BB9)
    (at 302.25 148.25)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591919/57AD80BE)
    (attr smd)
    (fp_text reference C112 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 162 +5F))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0BBF)
    (at 299.25 142)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/5659191C/57ADFEE4)
    (attr smd)
    (fp_text reference C113 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0BC5)
    (at 301 153.75)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/5659191C/57B0D6F6)
    (attr smd)
    (fp_text reference C114 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(C114-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0BCB)
    (at 313.5 154.25)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/5659191C/57AE2C9D)
    (attr smd)
    (fp_text reference C115 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 162 +5F))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0BD1)
    (at 307.5 149.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/565F7162/57ADFEE4)
    (attr smd)
    (fp_text reference C116 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0BD7)
    (at 302.5 150.25)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/565F7162/57B0D6F6)
    (attr smd)
    (fp_text reference C117 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(C117-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0BDD)
    (at 316.75 151.575001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/565F7162/57AE2C9D)
    (attr smd)
    (fp_text reference C118 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 162 +5F))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0BE3)
    (at 316.5 154.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591913/57B075E7)
    (attr smd)
    (fp_text reference C119 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(C119-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57AC0BEF)
    (at 313.25 157.75)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591916/57D63C1E)
    (attr smd)
    (fp_text reference C121 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(C121-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(C121-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Socket_Strips:Socket_Strip_Straight_1x04 (layer B.Cu) (tedit 0) (tstamp 57AC0BF0)
    (at 231 92 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (path /5659094D/57AEC939)
    (fp_text reference P13 (at 0 5.1 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value CONN_01X04 (at 0 3.1 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -1.75 1.75) (end -1.75 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 9.4 1.75) (end 9.4 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.75 1.75) (end 9.4 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 9.4 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end 8.89 1.27) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.27 -1.27) (end 8.89 -1.27) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 0 -1.55) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.89 1.27) (end 8.89 -1.27) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer B.SilkS) (width 0.15))
    (fp_line (start 0 1.55) (end -1.55 1.55) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.55 1.55) (end -1.55 -1.55) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 160 /ctrl/TX))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 59 /ctrl/RX))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 13 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x04.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Pin_Headers:Pin_Header_Angled_1x04 (layer F.Cu) (tedit 0) (tstamp 57AC0BF7)
    (at 214 76 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /56590966/57AEB2FC)
    (fp_text reference P14 (at 0 -5.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X04 (at 0 -3.1 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.5 -1.75) (end -1.5 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.65 -1.75) (end 10.65 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 -1.75) (end 10.65 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 9.4) (end 10.65 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -1.55) (end -1.3 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -1.55) (end -1.3 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.191 -0.127) (end 10.033 -0.127) (layer F.SilkS) (width 0.15))
    (fp_line (start 10.033 -0.127) (end 10.033 0.127) (layer F.SilkS) (width 0.15))
    (fp_line (start 10.033 0.127) (end 4.191 0.127) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.191 0.127) (end 4.191 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.191 0) (end 10.033 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 -0.254) (end 1.143 -0.254) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 0.254) (end 1.143 0.254) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 2.286) (end 1.143 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 2.794) (end 1.143 2.794) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 4.826) (end 1.143 4.826) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 5.334) (end 1.143 5.334) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 7.874) (end 1.143 7.874) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 7.366) (end 1.143 7.366) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 -1.27) (end 4.064 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 1.27) (end 4.064 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 1.27) (end 1.524 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 3.81) (end 4.064 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.286) (end 10.16 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 10.16 2.286) (end 10.16 2.794) (layer F.SilkS) (width 0.15))
    (fp_line (start 10.16 2.794) (end 4.064 2.794) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 3.81) (end 4.064 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 1.27) (end 4.064 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 10.16 0.254) (end 4.064 0.254) (layer F.SilkS) (width 0.15))
    (fp_line (start 10.16 -0.254) (end 10.16 0.254) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 -0.254) (end 10.16 -0.254) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 1.27) (end 4.064 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 -1.27) (end 1.524 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 6.35) (end 4.064 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 6.35) (end 1.524 8.89) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 8.89) (end 4.064 8.89) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 7.366) (end 10.16 7.366) (layer F.SilkS) (width 0.15))
    (fp_line (start 10.16 7.366) (end 10.16 7.874) (layer F.SilkS) (width 0.15))
    (fp_line (start 10.16 7.874) (end 4.064 7.874) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 8.89) (end 4.064 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 6.35) (end 4.064 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 10.16 5.334) (end 4.064 5.334) (layer F.SilkS) (width 0.15))
    (fp_line (start 10.16 4.826) (end 10.16 5.334) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 4.826) (end 10.16 4.826) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 6.35) (end 4.064 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 3.81) (end 1.524 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 3.81) (end 4.064 3.81) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 160 /ctrl/TX))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 /ctrl/RX))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57AC0C03)
    (at 302.75 156.5)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591916/57AD27E4)
    (attr smd)
    (fp_text reference R120 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(R120-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57AC0C09)
    (at 309.25 156.75)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/57B0307F)
    (attr smd)
    (fp_text reference R130 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(C36-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(R130-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57AC0C0F)
    (at 299 158.75)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/57B0307F)
    (attr smd)
    (fp_text reference R131 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(C37-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(R131-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57AC0C15)
    (at 306.25 157.25)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591916/57D63C12)
    (attr smd)
    (fp_text reference R132 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(R132-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57AC0C1B)
    (at 305.5 154)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591916/57D63C0C)
    (attr smd)
    (fp_text reference R133 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 162 +5F))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(R132-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57AC0C21)
    (at 309.25 152.25)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591916/57D63C4F)
    (attr smd)
    (fp_text reference R134 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 162 +5F))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(R132-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 53DE8DE3) (tstamp 57AC0C22)
    (at 388.021766 131.918362)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (path /56590966/56591916/57AD3DD4)
    (attr smd)
    (fp_text reference U13 (at 0 -2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ACT4088 (at 0 2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center -0.4 -1.7) (end -0.3 -1.7) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 -1.45) (end -0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 1.45) (end 0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 1.45) (end 0.25 1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 -1.45) (end -0.25 1.45) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(C105-Pad2)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 53 +24V))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(R35-Pad1)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(C105-Pad1)"))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 53DE8DE3) (tstamp 57AC0C34)
    (at 301.65 164.8)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (path /56590966/56591916/57AD27CC)
    (attr smd)
    (fp_text reference U27 (at 0 -2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ACT4088 (at 0 2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center -0.4 -1.7) (end -0.3 -1.7) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 -1.45) (end -0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 1.45) (end 0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 1.45) (end 0.25 1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 -1.45) (end -0.25 1.45) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(C106-Pad2)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 53 +24V))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(R120-Pad2)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(C106-Pad1)"))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_ThroughHole:C_Radial_D6.3_L11.2_P2.5 (layer F.Cu) (tedit 0) (tstamp 57AC1057)
    (at 415.801955 124.176361)
    (descr "Radial Electrolytic Capacitor, Diameter 6.3mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (path /5659094D/565909D4/56657F5F)
    (fp_text reference C62 (at 1.25 -4.4) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 47µ (at 1.25 4.4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.325 -3.149) (end 1.325 3.149) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.465 -3.143) (end 1.465 3.143) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.605 -3.13) (end 1.605 -0.446) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.605 0.446) (end 1.605 3.13) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.745 -3.111) (end 1.745 -0.656) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.745 0.656) (end 1.745 3.111) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.885 -3.085) (end 1.885 -0.789) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.885 0.789) (end 1.885 3.085) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.025 -3.053) (end 2.025 -0.88) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.025 0.88) (end 2.025 3.053) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.165 -3.014) (end 2.165 -0.942) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.165 0.942) (end 2.165 3.014) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.305 -2.968) (end 2.305 -0.981) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.305 0.981) (end 2.305 2.968) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.445 -2.915) (end 2.445 -0.998) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.445 0.998) (end 2.445 2.915) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.585 -2.853) (end 2.585 -0.996) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.585 0.996) (end 2.585 2.853) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.725 -2.783) (end 2.725 -0.974) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.725 0.974) (end 2.725 2.783) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.865 -2.704) (end 2.865 -0.931) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.865 0.931) (end 2.865 2.704) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.005 -2.616) (end 3.005 -0.863) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.005 0.863) (end 3.005 2.616) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.145 -2.516) (end 3.145 -0.764) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.145 0.764) (end 3.145 2.516) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.285 -2.404) (end 3.285 -0.619) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.285 0.619) (end 3.285 2.404) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.425 -2.279) (end 3.425 -0.38) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.425 0.38) (end 3.425 2.279) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.565 -2.136) (end 3.565 2.136) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.705 -1.974) (end 3.705 1.974) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.845 -1.786) (end 3.845 1.786) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.985 -1.563) (end 3.985 1.563) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.125 -1.287) (end 4.125 1.287) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.265 -0.912) (end 4.265 0.912) (layer F.SilkS) (width 0.15))
    (fp_circle (center 2.5 0) (end 2.5 -1) (layer F.SilkS) (width 0.15))
    (fp_circle (center 1.25 0) (end 1.25 -3.1875) (layer F.SilkS) (width 0.15))
    (fp_circle (center 1.25 0) (end 1.25 -3.4) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 46 +15V))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D6.3_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_ThroughHole:C_Radial_D6.3_L11.2_P2.5 (layer F.Cu) (tedit 0) (tstamp 57AC105C)
    (at 323.94946 153.75)
    (descr "Radial Electrolytic Capacitor, Diameter 6.3mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (path /5659094D/565909D4/57B29455)
    (fp_text reference C95 (at 1.25 -4.4) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 47µ (at 1.25 4.4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.325 -3.149) (end 1.325 3.149) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.465 -3.143) (end 1.465 3.143) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.605 -3.13) (end 1.605 -0.446) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.605 0.446) (end 1.605 3.13) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.745 -3.111) (end 1.745 -0.656) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.745 0.656) (end 1.745 3.111) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.885 -3.085) (end 1.885 -0.789) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.885 0.789) (end 1.885 3.085) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.025 -3.053) (end 2.025 -0.88) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.025 0.88) (end 2.025 3.053) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.165 -3.014) (end 2.165 -0.942) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.165 0.942) (end 2.165 3.014) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.305 -2.968) (end 2.305 -0.981) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.305 0.981) (end 2.305 2.968) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.445 -2.915) (end 2.445 -0.998) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.445 0.998) (end 2.445 2.915) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.585 -2.853) (end 2.585 -0.996) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.585 0.996) (end 2.585 2.853) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.725 -2.783) (end 2.725 -0.974) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.725 0.974) (end 2.725 2.783) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.865 -2.704) (end 2.865 -0.931) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.865 0.931) (end 2.865 2.704) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.005 -2.616) (end 3.005 -0.863) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.005 0.863) (end 3.005 2.616) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.145 -2.516) (end 3.145 -0.764) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.145 0.764) (end 3.145 2.516) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.285 -2.404) (end 3.285 -0.619) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.285 0.619) (end 3.285 2.404) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.425 -2.279) (end 3.425 -0.38) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.425 0.38) (end 3.425 2.279) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.565 -2.136) (end 3.565 2.136) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.705 -1.974) (end 3.705 1.974) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.845 -1.786) (end 3.845 1.786) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.985 -1.563) (end 3.985 1.563) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.125 -1.287) (end 4.125 1.287) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.265 -0.912) (end 4.265 0.912) (layer F.SilkS) (width 0.15))
    (fp_circle (center 2.5 0) (end 2.5 -1) (layer F.SilkS) (width 0.15))
    (fp_circle (center 1.25 0) (end 1.25 -3.1875) (layer F.SilkS) (width 0.15))
    (fp_circle (center 1.25 0) (end 1.25 -3.4) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 46 +15V))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D6.3_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stmbl:USB_Micro-B_10103594-0001LF placed (layer F.Cu) (tedit 57AC0B38) (tstamp 57755E00)
    (at 234.5 38 180)
    (descr "Micro USB Type B 10103594-0001LF")
    (tags "USB USB_B USB_micro USB_OTG")
    (path /56590966/56591913/56602983)
    (attr smd)
    (fp_text reference P1 (at 0 -4.625 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USB_OTG (at 0 4.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.25 -3.94) (end 4.25 -3.94) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.25 -3.94) (end 4.25 3.91) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.25 3.91) (end -4.25 3.91) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.25 3.91) (end -4.25 -3.94) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4 3.655) (end 4 3.655) (layer F.SilkS) (width 0.15))
    (fp_line (start -4 -3.665) (end 4 -3.665) (layer F.SilkS) (width 0.15))
    (fp_line (start 4 -3.665) (end 4 3.655) (layer F.SilkS) (width 0.15))
    (fp_line (start 4 3.035) (end -4 3.035) (layer F.SilkS) (width 0.15))
    (fp_line (start -4 3.655) (end -4 -3.665) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.3 -2.04 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.65 -2.04 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(P1-Pad2)"))
    (pad 3 smd rect (at -0.0009 -2.04 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(P1-Pad3)"))
    (pad 4 smd rect (at 0.65 -2.04 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.3 -2.04 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -2.425 -2.165 270) (size 1.2 1) (drill 0.6) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 6 thru_hole oval (at 2.425 -2.165 270) (size 1.2 1) (drill 0.6) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 6 thru_hole oval (at -2.75 0.835 270) (size 1.7 1.4) (drill 0.9) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 6 thru_hole oval (at 2.75 0.835 270) (size 1.6 1.4) (drill 0.9) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 6 smd rect (at -0.9625 1.085 270) (size 2.5 1.425) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 6 smd rect (at 0.9625 1.085 270) (size 2.5 1.425) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57D4A251)
    (at 311.25 164)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591916/57D63C71)
    (attr smd)
    (fp_text reference C120 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 53 +24V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57D4A25B)
    (at 363.848746 8.906547)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/56591916/57D63C68)
    (attr smd)
    (fp_text reference C122 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 162 +5F))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5415D7BD) (tstamp 57D4A261)
    (at 373.740176 -1.143453)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (path /56590966/56591916/57D63C06)
    (attr smd)
    (fp_text reference C123 (at 0 -2.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10µ (at 0 2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1.15) (end 2.3 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1.15) (end 2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1.15) (end -2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1.15) (end 2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -1.025) (end -1 -1.025) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 1.025) (end 1 1.025) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 162 +5F))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5415D7BD) (tstamp 57D4A267)
    (at 373.740176 8.106547)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (path /56590966/56591916/57D63C7A)
    (attr smd)
    (fp_text reference C124 (at 0 -2.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10µ (at 0 2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.3 -1.15) (end 2.3 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 1.15) (end 2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.3 -1.15) (end -2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -1.15) (end 2.3 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -1.025) (end -1 -1.025) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 1.025) (end 1 1.025) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 162 +5F))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57D4A26D)
    (at 401.048746 -1.543453)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/57D5F156)
    (attr smd)
    (fp_text reference R135 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(C114-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 168 /ctrl/FB0/A78))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57D4A273)
    (at 408.048746 -1.543453)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/57D5F335)
    (attr smd)
    (fp_text reference R136 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 168 /ctrl/FB0/A78))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57D4A279)
    (at 415.048746 -1.543453)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/57D5E6AA)
    (attr smd)
    (fp_text reference R137 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(C114-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 162 +5F))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57D4A27F)
    (at 401.048746 14.086547)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/57D5F156)
    (attr smd)
    (fp_text reference R138 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(C117-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 169 /ctrl/FB1/A78))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57D4A285)
    (at 408.048746 14.086547)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/57D5F335)
    (attr smd)
    (fp_text reference R139 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 169 /ctrl/FB1/A78))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57D4A28B)
    (at 415.048746 14.086547)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/57D5E6AA)
    (attr smd)
    (fp_text reference R140 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(C117-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 162 +5F))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 53DE8DE3) (tstamp 57D4A295)
    (at 316.5 172.5)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (path /56590966/56591916/57D63C38)
    (attr smd)
    (fp_text reference U28 (at 0 -2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ACT4088 (at 0 2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center -0.4 -1.7) (end -0.3 -1.7) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 -1.45) (end -0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 1.45) (end 0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 1.45) (end 0.25 1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 -1.45) (end -0.25 1.45) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(C121-Pad2)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 53 +24V))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(R132-Pad1)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(C121-Pad1)"))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57D62ACE)
    (at 382.216218 44.884921)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/5659191C/57D74C8F)
    (attr smd)
    (fp_text reference C125 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 168 /ctrl/FB0/A78))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57D62ADA)
    (at 382.216218 64.884921)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /56590966/565F7162/57D74C8F)
    (attr smd)
    (fp_text reference C126 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 169 /ctrl/FB1/A78))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57D62AE0)
    (at 405.450504 44.884921)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/565909D0/57B2E566)
    (attr smd)
    (fp_text reference L1 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "220r 700mA" (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(C83-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57D62AE6)
    (at 405.450504 56.864921)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591913/565FF296)
    (attr smd)
    (fp_text reference L3 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "220r 700mA" (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(C119-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57D62AEC)
    (at 424.130504 44.884921)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/56591919/57AD7F96)
    (attr smd)
    (fp_text reference L7 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "220r 700mA" (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(C53-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 162 +5F))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57D62AF2)
    (at 372.500504 44.884921)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/57ADE969)
    (attr smd)
    (fp_text reference L8 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "220r 700mA" (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(C36-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57D62AF8)
    (at 372.500504 53.334921)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/5659191C/57AE2C95)
    (attr smd)
    (fp_text reference L9 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "220r 700mA" (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 162 +5F))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(C72-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57D62AFE)
    (at 372.500504 64.884921)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/57ADE969)
    (attr smd)
    (fp_text reference L10 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "220r 700mA" (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(C37-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57D62B04)
    (at 372.500504 73.334921)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /56590966/565F7162/57AE2C95)
    (attr smd)
    (fp_text reference L11 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "220r 700mA" (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 162 +5F))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(C71-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57D75BD8)
    (at 360.702318 153.600877)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/57DCE80A)
    (attr smd)
    (fp_text reference C127 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 177 /hv/f3/A_T_MOT))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57D75BE4)
    (at 361.892318 174.070877)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5659094D/565909D0/57DF402E)
    (attr smd)
    (fp_text reference C128 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57D75BFA)
    (at 360.702318 162.050877)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/57DD09BB)
    (attr smd)
    (fp_text reference R141 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 15k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(P2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 177 /hv/f3/A_T_MOT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62) (tstamp 57D75C00)
    (at 367.702318 153.600877)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5659094D/57DCE6B7)
    (attr smd)
    (fp_text reference R142 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 +15V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(P2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_QFP:LQFP-100_14x14mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77) (tstamp 57D75C01)
    (at 219.5 60)
    (descr "LQFP100: plastic low profile quad flat package; 100 leads; body 14 x 14 x 1.4 mm (see NXP sot407-1_po.pdf and sot407-1_fr.pdf)")
    (tags "QFP 0.5")
    (path /56590966/56591913/565FD974)
    (attr smd)
    (fp_text reference U26 (at 0 -9.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value STM32F405VG (at 0 9.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -8.9 -8.9) (end -8.9 8.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.9 -8.9) (end 8.9 8.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -8.9 -8.9) (end 8.9 -8.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -8.9 8.9) (end 8.9 8.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -7.125 -7.125) (end -7.125 -6.365) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.125 -7.125) (end 7.125 -6.365) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.125 7.125) (end 7.125 6.365) (layer F.SilkS) (width 0.15))
    (fp_line (start -7.125 7.125) (end -7.125 6.365) (layer F.SilkS) (width 0.15))
    (fp_line (start -7.125 -7.125) (end -6.365 -7.125) (layer F.SilkS) (width 0.15))
    (fp_line (start -7.125 7.125) (end -6.365 7.125) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.125 7.125) (end 6.365 7.125) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.125 -7.125) (end 6.365 -7.125) (layer F.SilkS) (width 0.15))
    (fp_line (start -7.125 -6.365) (end -8.65 -6.365) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -7.9 -6) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -7.9 -5.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -7.9 -5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -7.9 -4.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -7.9 -4) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -7.9 -3.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 7 smd rect (at -7.9 -3) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -7.9 -2.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -7.9 -2) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -7.9 -1.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at -7.9 -1) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 12 smd rect (at -7.9 -0.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C31-Pad1)"))
    (pad 13 smd rect (at -7.9 0) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C32-Pad1)"))
    (pad 14 smd rect (at -7.9 0.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 161 /ctrl/IO/NRST))
    (pad 15 smd rect (at -7.9 1) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -7.9 1.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -7.9 2) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -7.9 2.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at -7.9 3) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 20 smd rect (at -7.9 3.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 21 smd rect (at -7.9 4) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(C119-Pad2)"))
    (pad 22 smd rect (at -7.9 4.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(C119-Pad2)"))
    (pad 23 smd rect (at -7.9 5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 160 /ctrl/TX))
    (pad 24 smd rect (at -7.9 5.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 59 /ctrl/RX))
    (pad 25 smd rect (at -7.9 6) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at -6 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at -5.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 28 smd rect (at -5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 29 smd rect (at -4.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at -4 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 31 smd rect (at -3.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 32 smd rect (at -3 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 33 smd rect (at -2.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd rect (at -2 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 35 smd rect (at -1.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 36 smd rect (at -1 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 37 smd rect (at -0.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 38 smd rect (at 0 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 0.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 117 /ctrl/FB1/D12))
    (pad 41 smd rect (at 1.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 2 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 119 /ctrl/FB1/D36))
    (pad 43 smd rect (at 2.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 44 smd rect (at 3 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 122 /ctrl/FB1/D45))
    (pad 45 smd rect (at 3.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 108 /ctrl/FB1/E45))
    (pad 46 smd rect (at 4 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 47 smd rect (at 4.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 122 /ctrl/FB1/D45))
    (pad 48 smd rect (at 5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 117 /ctrl/FB1/D12))
    (pad 49 smd rect (at 5.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(C88-Pad1)"))
    (pad 50 smd rect (at 6 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 51 smd rect (at 7.9 6) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 119 /ctrl/FB1/D36))
    (pad 52 smd rect (at 7.9 5.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 119 /ctrl/FB1/D36))
    (pad 53 smd rect (at 7.9 5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 117 /ctrl/FB1/D12))
    (pad 54 smd rect (at 7.9 4.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 122 /ctrl/FB1/D45))
    (pad 55 smd rect (at 7.9 4) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 56 smd rect (at 7.9 3.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 57 smd rect (at 7.9 3) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 58 smd rect (at 7.9 2.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 59 smd rect (at 7.9 2) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 118 /ctrl/FB0/D12))
    (pad 60 smd rect (at 7.9 1.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 120 /ctrl/FB0/D36))
    (pad 61 smd rect (at 7.9 1) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 121 /ctrl/FB0/D45))
    (pad 62 smd rect (at 7.9 0.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 109 /ctrl/FB0/E45))
    (pad 63 smd rect (at 7.9 0) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 121 /ctrl/FB0/D45))
    (pad 64 smd rect (at 7.9 -0.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 118 /ctrl/FB0/D12))
    (pad 65 smd rect (at 7.9 -1) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 120 /ctrl/FB0/D36))
    (pad 66 smd rect (at 7.9 -1.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 67 smd rect (at 7.9 -2) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 114 /ctrl/f4/CMD_36))
    (pad 68 smd rect (at 7.9 -2.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 115 /ctrl/f4/CMD_45))
    (pad 69 smd rect (at 7.9 -3) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 113 /ctrl/f4/CMD_12))
    (pad 70 smd rect (at 7.9 -3.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(P1-Pad2)"))
    (pad 71 smd rect (at 7.9 -4) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(P1-Pad3)"))
    (pad 72 smd rect (at 7.9 -4.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 73 smd rect (at 7.9 -5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(C90-Pad1)"))
    (pad 74 smd rect (at 7.9 -5.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 75 smd rect (at 7.9 -6) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 76 smd rect (at 6 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 77 smd rect (at 5.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 113 /ctrl/f4/CMD_12))
    (pad 78 smd rect (at 5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 120 /ctrl/FB0/D36))
    (pad 79 smd rect (at 4.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 118 /ctrl/FB0/D12))
    (pad 80 smd rect (at 4 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 121 /ctrl/FB0/D45))
    (pad 81 smd rect (at 3.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 82 smd rect (at 3 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 83 smd rect (at 2.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 84 smd rect (at 2 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 85 smd rect (at 1.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 86 smd rect (at 1 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 87 smd rect (at 0.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 88 smd rect (at 0 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 89 smd rect (at -0.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 114 /ctrl/f4/CMD_36))
    (pad 90 smd rect (at -1 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 113 /ctrl/f4/CMD_12))
    (pad 91 smd rect (at -1.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 115 /ctrl/f4/CMD_45))
    (pad 92 smd rect (at -2 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 93 smd rect (at -2.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 94 smd rect (at -3 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(JP9-Pad2)"))
    (pad 95 smd rect (at -3.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 96 smd rect (at -4 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 97 smd rect (at -4.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 98 smd rect (at -5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 99 smd rect (at -5.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 100 smd rect (at -6 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (model Housings_QFP.3dshapes/LQFP-100_14x14mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 53DE8DE3) (tstamp 57D75C71)
    (at 351.392318 175.070877)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (path /5659094D/565909D0/57DEBE00)
    (attr smd)
    (fp_text reference U29 (at 0 -2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USBLC6-4SC6 (at 0 2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center -0.4 -1.7) (end -0.3 -1.7) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 -1.45) (end -0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 1.45) (end 0.25 -1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 1.45) (end 0.25 1.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 -1.45) (end -0.25 1.45) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stmbl:SOIC-8-N (layer F.Cu) (tedit 0) (tstamp 57D7782E)
    (at 244 93 180)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (path /5659094D/56590991)
    (attr smd)
    (fp_text reference U3 (at 0 -1.27 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SI8621 (at 0 1.27 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.54 -2.286) (end 2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 -2.286) (end 2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 2.286) (end -2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 2.286) (end -2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 -0.762) (end -2.032 -0.762) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 -0.762) (end -2.032 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 0.508) (end -2.54 0.508) (layer F.SilkS) (width 0.15))
    (pad 8 smd rect (at -1.905 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3VP))
    (pad 7 smd rect (at -0.635 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 90 /hv/f3/HV_RX))
    (pad 6 smd rect (at 0.635 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 112 /hv/f3/HV_TX))
    (pad 5 smd rect (at 1.905 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDPWR))
    (pad 4 smd rect (at 1.905 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.635 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 160 /ctrl/TX))
    (pad 2 smd rect (at -0.635 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 59 /ctrl/RX))
    (pad 1 smd rect (at -1.905 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (model ${KIPRJMOD}/stmbl.pretty/so8.wrl
      (at (xyz 0.09842519685039371 -0.1220472440944882 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stmbl:SOIC-8-N (layer F.Cu) (tedit 0) (tstamp 57D77839)
    (at 244.25 60.5)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (path /56590966/5659191C/5659192C)
    (attr smd)
    (fp_text reference U6 (at 0 -1.27) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LM358 (at 0 1.27) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.54 -2.286) (end 2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 -2.286) (end 2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 2.286) (end -2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 2.286) (end -2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 -0.762) (end -2.032 -0.762) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 -0.762) (end -2.032 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 0.508) (end -2.54 0.508) (layer F.SilkS) (width 0.15))
    (pad 8 smd rect (at -1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(C36-Pad2)"))
    (pad 7 smd rect (at -0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(R56-Pad1)"))
    (pad 6 smd rect (at 0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C25-Pad2)"))
    (pad 5 smd rect (at 1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C25-Pad1)"))
    (pad 4 smd rect (at 1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C27-Pad1)"))
    (pad 2 smd rect (at -0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C27-Pad2)"))
    (pad 1 smd rect (at -1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(R55-Pad1)"))
    (model ${KIPRJMOD}/stmbl.pretty/so8.wrl
      (at (xyz 0.09842519685039371 -0.1220472440944882 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stmbl:SOIC-8-N (layer F.Cu) (tedit 0) (tstamp 57D77844)
    (at 243.75 78.25)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (path /56590966/565F7162/5659192C)
    (attr smd)
    (fp_text reference U7 (at 0 -1.27) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LM358 (at 0 1.27) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.54 -2.286) (end 2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 -2.286) (end 2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 2.286) (end -2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 2.286) (end -2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 -0.762) (end -2.032 -0.762) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 -0.762) (end -2.032 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 0.508) (end -2.54 0.508) (layer F.SilkS) (width 0.15))
    (pad 8 smd rect (at -1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(C37-Pad2)"))
    (pad 7 smd rect (at -0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(R57-Pad1)"))
    (pad 6 smd rect (at 0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C24-Pad2)"))
    (pad 5 smd rect (at 1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C24-Pad1)"))
    (pad 4 smd rect (at 1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C26-Pad1)"))
    (pad 2 smd rect (at -0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C26-Pad2)"))
    (pad 1 smd rect (at -1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(R54-Pad1)"))
    (model ${KIPRJMOD}/stmbl.pretty/so8.wrl
      (at (xyz 0.09842519685039371 -0.1220472440944882 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stmbl:SOIC-8-N (layer F.Cu) (tedit 0) (tstamp 57D7784F)
    (at 253.5 49.5 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (path /56590966/56591919/565DD0E7)
    (attr smd)
    (fp_text reference U8 (at 0 -1.27 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SN65176B (at 0 1.27 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.54 -2.286) (end 2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 -2.286) (end 2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 2.286) (end -2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 2.286) (end -2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 -0.762) (end -2.032 -0.762) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 -0.762) (end -2.032 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 0.508) (end -2.54 0.508) (layer F.SilkS) (width 0.15))
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(C53-Pad1)"))
    (pad 7 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(J3-Pad2)"))
    (pad 6 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(J3-Pad1)"))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 113 /ctrl/f4/CMD_12))
    (pad 3 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 95 /ctrl/f4/CMD_12E))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 95 /ctrl/f4/CMD_12E))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 113 /ctrl/f4/CMD_12))
    (model ${KIPRJMOD}/stmbl.pretty/so8.wrl
      (at (xyz 0.09842519685039371 -0.1220472440944882 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stmbl:SOIC-8-N (layer F.Cu) (tedit 0) (tstamp 57D7785A)
    (at 253.5 44 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (path /56590966/56591919/565DDC9B)
    (attr smd)
    (fp_text reference U9 (at 0 -1.27 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SN65176B (at 0 1.27 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.54 -2.286) (end 2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 -2.286) (end 2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 2.286) (end -2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 2.286) (end -2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 -0.762) (end -2.032 -0.762) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 -0.762) (end -2.032 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 0.508) (end -2.54 0.508) (layer F.SilkS) (width 0.15))
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(C53-Pad1)"))
    (pad 7 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(J3-Pad6)"))
    (pad 6 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(J3-Pad3)"))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 114 /ctrl/f4/CMD_36))
    (pad 3 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 96 /ctrl/f4/CMD_36E))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 96 /ctrl/f4/CMD_36E))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 114 /ctrl/f4/CMD_36))
    (model ${KIPRJMOD}/stmbl.pretty/so8.wrl
      (at (xyz 0.09842519685039371 -0.1220472440944882 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stmbl:SOIC-8-N (layer F.Cu) (tedit 0) (tstamp 57D77865)
    (at 253.5 38.5 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (path /56590966/56591919/565DDF06)
    (attr smd)
    (fp_text reference U10 (at 0 -1.27 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SN65176B (at 0 1.27 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.54 -2.286) (end 2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 -2.286) (end 2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 2.286) (end -2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 2.286) (end -2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 -0.762) (end -2.032 -0.762) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 -0.762) (end -2.032 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 0.508) (end -2.54 0.508) (layer F.SilkS) (width 0.15))
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(C53-Pad1)"))
    (pad 7 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(J3-Pad4)"))
    (pad 6 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(J3-Pad5)"))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 115 /ctrl/f4/CMD_45))
    (pad 3 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 97 /ctrl/f4/CMD_45E))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 97 /ctrl/f4/CMD_45E))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 115 /ctrl/f4/CMD_45))
    (model ${KIPRJMOD}/stmbl.pretty/so8.wrl
      (at (xyz 0.09842519685039371 -0.1220472440944882 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stmbl:SOIC-8-N (layer F.Cu) (tedit 0) (tstamp 57D77870)
    (at 244.25 44 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (path /56590966/56591919/565DDF3C)
    (attr smd)
    (fp_text reference U11 (at 0 -1.27 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SN65176B (at 0 1.27 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.54 -2.286) (end 2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 -2.286) (end 2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 2.286) (end -2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 2.286) (end -2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 -0.762) (end -2.032 -0.762) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 -0.762) (end -2.032 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 0.508) (end -2.54 0.508) (layer F.SilkS) (width 0.15))
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(C53-Pad1)"))
    (pad 7 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(J3-Pad8)"))
    (pad 6 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(J3-Pad7)"))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 116 /ctrl/f4/CMD_78))
    (pad 3 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 98 /ctrl/f4/CMD_78E))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 98 /ctrl/f4/CMD_78E))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 116 /ctrl/f4/CMD_78))
    (model ${KIPRJMOD}/stmbl.pretty/so8.wrl
      (at (xyz 0.09842519685039371 -0.1220472440944882 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stmbl:SOIC-8-N (layer F.Cu) (tedit 0) (tstamp 57D7787B)
    (at 253.5 66 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (path /56590966/5659191C/565DFE81)
    (attr smd)
    (fp_text reference U14 (at 0 -1.27 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SN65176B (at 0 1.27 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.54 -2.286) (end 2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 -2.286) (end 2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 2.286) (end -2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 2.286) (end -2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 -0.762) (end -2.032 -0.762) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 -0.762) (end -2.032 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 0.508) (end -2.54 0.508) (layer F.SilkS) (width 0.15))
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(C72-Pad1)"))
    (pad 7 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(J2-Pad2)"))
    (pad 6 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(J2-Pad1)"))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 118 /ctrl/FB0/D12))
    (pad 3 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 104 /ctrl/FB0/E12))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 104 /ctrl/FB0/E12))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 118 /ctrl/FB0/D12))
    (model ${KIPRJMOD}/stmbl.pretty/so8.wrl
      (at (xyz 0.09842519685039371 -0.1220472440944882 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stmbl:SOIC-8-N (layer F.Cu) (tedit 0) (tstamp 57D77886)
    (at 253.5 82.5 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (path /56590966/565F7162/565DFE81)
    (attr smd)
    (fp_text reference U15 (at 0 -1.27 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SN65176B (at 0 1.27 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.54 -2.286) (end 2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 -2.286) (end 2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 2.286) (end -2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 2.286) (end -2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 -0.762) (end -2.032 -0.762) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 -0.762) (end -2.032 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 0.508) (end -2.54 0.508) (layer F.SilkS) (width 0.15))
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(C71-Pad1)"))
    (pad 7 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(J1-Pad2)"))
    (pad 6 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(J1-Pad1)"))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 117 /ctrl/FB1/D12))
    (pad 3 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 105 /ctrl/FB1/E12))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 105 /ctrl/FB1/E12))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 117 /ctrl/FB1/D12))
    (model ${KIPRJMOD}/stmbl.pretty/so8.wrl
      (at (xyz 0.09842519685039371 -0.1220472440944882 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stmbl:SOIC-8-N (layer F.Cu) (tedit 0) (tstamp 57D77891)
    (at 253.5 77 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (path /56590966/565F7162/565DFEAC)
    (attr smd)
    (fp_text reference U16 (at 0 -1.27 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SN65176B (at 0 1.27 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.54 -2.286) (end 2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 -2.286) (end 2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 2.286) (end -2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 2.286) (end -2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 -0.762) (end -2.032 -0.762) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 -0.762) (end -2.032 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 0.508) (end -2.54 0.508) (layer F.SilkS) (width 0.15))
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(C71-Pad1)"))
    (pad 7 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(J1-Pad3)"))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 119 /ctrl/FB1/D36))
    (pad 3 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 /ctrl/FB1/E36))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 /ctrl/FB1/E36))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 119 /ctrl/FB1/D36))
    (model ${KIPRJMOD}/stmbl.pretty/so8.wrl
      (at (xyz 0.09842519685039371 -0.1220472440944882 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stmbl:SOIC-8-N (layer F.Cu) (tedit 0) (tstamp 57D7789C)
    (at 253.5 60.5 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (path /56590966/5659191C/565DFEAC)
    (attr smd)
    (fp_text reference U17 (at 0 -1.27 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SN65176B (at 0 1.27 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.54 -2.286) (end 2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 -2.286) (end 2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 2.286) (end -2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 2.286) (end -2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 -0.762) (end -2.032 -0.762) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 -0.762) (end -2.032 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 0.508) (end -2.54 0.508) (layer F.SilkS) (width 0.15))
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(C72-Pad1)"))
    (pad 7 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(J2-Pad6)"))
    (pad 6 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(J2-Pad3)"))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 120 /ctrl/FB0/D36))
    (pad 3 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 106 /ctrl/FB0/E36))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 106 /ctrl/FB0/E36))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 120 /ctrl/FB0/D36))
    (model ${KIPRJMOD}/stmbl.pretty/so8.wrl
      (at (xyz 0.09842519685039371 -0.1220472440944882 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stmbl:SOIC-8-N (layer F.Cu) (tedit 0) (tstamp 57D778A7)
    (at 253.544 55 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (path /56590966/5659191C/565DFED0)
    (attr smd)
    (fp_text reference U18 (at 0 -1.27 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SN65176B (at 0 1.27 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.54 -2.286) (end 2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 -2.286) (end 2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 2.286) (end -2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 2.286) (end -2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 -0.762) (end -2.032 -0.762) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 -0.762) (end -2.032 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 0.508) (end -2.54 0.508) (layer F.SilkS) (width 0.15))
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(C72-Pad1)"))
    (pad 7 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(J2-Pad4)"))
    (pad 6 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(J2-Pad5)"))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 121 /ctrl/FB0/D45))
    (pad 3 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 109 /ctrl/FB0/E45))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 109 /ctrl/FB0/E45))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 121 /ctrl/FB0/D45))
    (model ${KIPRJMOD}/stmbl.pretty/so8.wrl
      (at (xyz 0.09842519685039371 -0.1220472440944882 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stmbl:SOIC-8-N (layer F.Cu) (tedit 0) (tstamp 57D778B2)
    (at 253.5 71.5 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (path /56590966/565F7162/565DFED0)
    (attr smd)
    (fp_text reference U19 (at 0 -1.27 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SN65176B (at 0 1.27 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.54 -2.286) (end 2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 -2.286) (end 2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 2.286) (end -2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 2.286) (end -2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 -0.762) (end -2.032 -0.762) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 -0.762) (end -2.032 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 0.508) (end -2.54 0.508) (layer F.SilkS) (width 0.15))
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(C71-Pad1)"))
    (pad 7 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(J1-Pad4)"))
    (pad 6 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(J1-Pad5)"))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 122 /ctrl/FB1/D45))
    (pad 3 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 108 /ctrl/FB1/E45))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 108 /ctrl/FB1/E45))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 122 /ctrl/FB1/D45))
    (model ${KIPRJMOD}/stmbl.pretty/so8.wrl
      (at (xyz 0.09842519685039371 -0.1220472440944882 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stmbl:SMD-8B (layer F.Cu) (tedit 57742D96) (tstamp 577CC905)
    (at 262 124)
    (path /5659094D/565909D4/57748D27)
    (fp_text reference U5 (at -1.25 -5.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value lnk304 (at 0 5.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.25 -4.75) (end 3.25 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.25 4.75) (end -3.25 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.25 4.75) (end -3.25 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.25 -4.75) (end 3.25 4.75) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.445 -3.81 270) (size 1.5 2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C41-Pad2)"))
    (pad 2 smd rect (at -4.445 -1.265883 270) (size 1.5 2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C41-Pad2)"))
    (pad 3 smd rect (at -4.445 1.274117 270) (size 1.5 2) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C41-Pad1)"))
    (pad 4 smd rect (at -4.445 3.814117 270) (size 1.5 2) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(R91-Pad2)"))
    (pad 5 smd rect (at 4.445 3.814117 270) (size 1.5 2) (layers F.Cu F.Paste F.Mask)
      (net 16 VPP))
    (pad 7 smd rect (at 4.445 -1.265883 270) (size 1.5 2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C41-Pad2)"))
    (pad 8 smd rect (at 4.445 -3.81 270) (size 1.5 2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C41-Pad2)"))
    (model ${KIPRJMOD}/stmbl.pretty/smd_8b.wrl
      (at (xyz -0.1929133858267717 -0.187007874015748 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )

  (module stmbl:IRAM256 (layer F.Cu) (tedit 5775AEC5) (tstamp 57757D91)
    (at 222 119.5 180)
    (path /5659094D/56590A75/5668DD3B)
    (fp_text reference U12 (at -27.5 -12 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IRAM256a (at 26.5 -12 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 25 -10) (end -25 -10) (layer F.SilkS) (width 0.15))
    (fp_line (start 25 10) (end 25 -10) (layer F.SilkS) (width 0.15))
    (fp_line (start -25 10) (end 25 10) (layer F.SilkS) (width 0.15))
    (fp_line (start -25 -10) (end -25 10) (layer F.SilkS) (width 0.15))
    (fp_line (start 31 1.5) (end 31 9.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 28 1.5) (end 31 1.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 28 -1.5) (end 31 -1.5) (layer F.SilkS) (width 0.15))
    (fp_arc (start 28 0) (end 28 1.5) (angle 180) (layer F.SilkS) (width 0.15))
    (fp_line (start -31 1.5) (end -31 9.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -28 1.5) (end -31 1.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -28 -1.5) (end -31 -1.5) (layer F.SilkS) (width 0.15))
    (fp_arc (start -28 0) (end -28 -1.5) (angle 180) (layer F.SilkS) (width 0.15))
    (fp_line (start -29.5 -11) (end -31 -9.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -29.5 11) (end -31 9.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 31 9.5) (end 29.5 11) (layer F.SilkS) (width 0.15))
    (fp_line (start 29.5 -11) (end 31 -9.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -31 -1.5) (end -31 -9.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 29.5 11) (end -29.5 11) (layer F.SilkS) (width 0.15))
    (fp_line (start 31 -9.5) (end 31 -1.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -29.5 -11) (end 29.5 -11) (layer F.SilkS) (width 0.15))
    (pad 13 thru_hole oval (at 2.54 16.5) (size 2 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 16 VPP))
    (pad 10 thru_hole oval (at 6.35 21.5) (size 2 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 37 /hv/back-emf/U))
    (pad 9 thru_hole oval (at 7.62 16.5) (size 1.5 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 38 "Net-(C44-Pad2)"))
    (pad 6 thru_hole oval (at 11.43 21.5) (size 2 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 35 /hv/back-emf/V))
    (pad 5 thru_hole oval (at 12.7 16.5) (size 1.5 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 36 "Net-(C43-Pad2)"))
    (pad 2 thru_hole oval (at 16.51 21.5) (size 2 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 33 /hv/back-emf/W))
    (pad 1 thru_hole oval (at 17.78 16.5) (size 1.5 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 34 "Net-(C42-Pad2)"))
    (pad 16 thru_hole oval (at -1.27 21.5) (size 1.5 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS))
    (pad 17 thru_hole oval (at -2.54 16.5) (size 1.5 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 75 /hv/driver/CUH))
    (pad 18 thru_hole oval (at -3.81 21.5) (size 1.5 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 110 /hv/f3/HV_EN))
    (pad 19 thru_hole oval (at -5.08 16.5) (size 1.5 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 92 /hv/driver/CVH))
    (pad 20 thru_hole oval (at -6.35 21.5) (size 1.5 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 128 /hv/f3/CH1N))
    (pad 21 thru_hole oval (at -7.62 16.5) (size 1.5 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 93 /hv/driver/CWH))
    (pad 22 thru_hole oval (at -8.89 21.5) (size 1.5 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 129 /hv/f3/CH2N))
    (pad 24 thru_hole oval (at -11.43 21.5) (size 1.5 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 130 /hv/f3/CH1))
    (pad 26 thru_hole oval (at -13.97 21.5) (size 1.5 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 131 /hv/f3/CH3))
    (pad 28 thru_hole oval (at -16.51 21.5) (size 1.5 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 46 +15V))
    (pad 23 thru_hole oval (at -10.16 16.5) (size 1.5 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 132 /hv/f3/CH3N))
    (pad 25 thru_hole oval (at -12.7 16.5) (size 1.5 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 133 /hv/f3/CH2))
    (pad 27 thru_hole oval (at -15.24 16.5) (size 1.5 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 103 /hv/f3/A_T_HV))
    (pad 29 thru_hole oval (at -17.78 16.5) (size 1.5 2) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 4 GNDPWR))
    (model ${KIPRJMOD}/stmbl.pretty/iram256.wrl
      (at (xyz -1.220472440944882 -0.4409448818897638 0.3149606299212598))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 180 90))
    )
  )

  (module stmbl:akl182-2 (layer B.Cu) (tedit 57D73CF8) (tstamp 57D75BF4)
    (at 192 131 90)
    (path /5659094D/57DC49A6)
    (fp_text reference P2 (at -0.6 3 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value CONN_01X02 (at 2.2 -9.8 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.55 -7.9) (end -2.55 2.3) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.55 2.3) (end 6.05 2.3) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.05 2.3) (end 6.05 -7.9) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.55 -7.9) (end 6.05 -7.9) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 178 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 3.5 0 90) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 4 GNDPWR))
    (model ${KIPRJMOD}/stmbl.pretty/akl182_2.wrl
      (at (xyz 0.2362204724409449 0.125984251968504 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 180))
    )
  )

  (module stmbl:akl182-2 (layer B.Cu) (tedit 57D73CF8) (tstamp 5775789A)
    (at 177 68.5 90)
    (path /56590966/56591916/566CDEAC)
    (fp_text reference P3 (at -0.6 3 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value CONN_01X02 (at 2.2 -9.8 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.55 -7.9) (end -2.55 2.3) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.55 2.3) (end 6.05 2.3) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.05 2.3) (end 6.05 -7.9) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.55 -7.9) (end 6.05 -7.9) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 3.5 0 90) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 53 +24V))
    (model ${KIPRJMOD}/stmbl.pretty/akl182_2.wrl
      (at (xyz 0.2362204724409449 0.125984251968504 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 180))
    )
  )

  (module stmbl:akl182-2 (layer B.Cu) (tedit 57D73CF8) (tstamp 57AC16AB)
    (at 207 42)
    (path /56590966/56591919/57B3D62F)
    (fp_text reference P15 (at -0.6 3) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value CONN_01X02 (at 2.2 -9.8) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.55 -7.9) (end -2.55 2.3) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.55 2.3) (end 6.05 2.3) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.05 2.3) (end 6.05 -7.9) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.55 -7.9) (end 6.05 -7.9) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole oval (at 0 0) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 87 "Net-(J3-Pad4)"))
    (pad 2 thru_hole oval (at 3.5 0) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 86 "Net-(J3-Pad5)"))
    (model ${KIPRJMOD}/stmbl.pretty/akl182_2.wrl
      (at (xyz 0.2362204724409449 0.125984251968504 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 180))
    )
  )

  (module stmbl:RM5.08_1x2 (layer B.Cu) (tedit 57755247) (tstamp 57755E06)
    (at 194 107.5 270)
    (path /5659094D/56590A75/566CF01F)
    (fp_text reference P6 (at -1.27 10.795 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value CONN_01X02 (at 5.715 -3.175 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -3.175 10.16) (end -3.175 -1.905) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.255 10.16) (end -3.175 10.16) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.255 -1.905) (end 8.255 10.16) (layer B.SilkS) (width 0.15))
    (fp_line (start -3.175 -1.905) (end 8.255 -1.905) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole oval (at 0 0 270) (size 2 3) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 4 GNDPWR))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2 3) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 16 VPP))
    (model ${KIPRJMOD}/stmbl.pretty/akl230_2.wrl
      (at (xyz -0.1240157480314961 -0.07874015748031496 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )

  (module stmbl:RM5.08_1x3 (layer B.Cu) (tedit 57755349) (tstamp 57755E0D)
    (at 194 90.5 270)
    (path /5659094D/56590A75/566CEA04)
    (fp_text reference P8 (at -1.27 10.795 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value CONN_01X03 (at 10.795 -3.175 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -3.175 10.16) (end -3.175 -1.905) (layer B.SilkS) (width 0.15))
    (fp_line (start 13.335 10.16) (end -3.175 10.16) (layer B.SilkS) (width 0.15))
    (fp_line (start 13.335 -1.905) (end 13.335 10.16) (layer B.SilkS) (width 0.15))
    (fp_line (start -3.175 -1.905) (end 13.335 -1.905) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole oval (at 0 0 270) (size 2 3) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 37 /hv/back-emf/U))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2 3) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 35 /hv/back-emf/V))
    (pad 3 thru_hole oval (at 10.16 0 270) (size 2 3) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 33 /hv/back-emf/W))
    (model ${KIPRJMOD}/stmbl.pretty/akl230_3.wrl
      (at (xyz -0.1240157480314961 -0.07874015748031496 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )

  (module stmbl:akl182-6 (layer B.Cu) (tedit 57D73CD8) (tstamp 577578B6)
    (at 177 59.5 90)
    (path /56590966/56591923/56684699)
    (fp_text reference P9 (at -0.6 3 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value CONN_01X06 (at 6 -9.8 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.55 -7.9) (end -2.55 2.3) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.55 2.3) (end 20.05 2.3) (layer B.SilkS) (width 0.15))
    (fp_line (start 20.05 2.3) (end 20.05 -7.9) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.55 -7.9) (end 20.05 -7.9) (layer B.SilkS) (width 0.15))
    (pad 6 thru_hole oval (at 17.5 0 90) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 14 0 90) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 172 "Net-(P9-Pad5)"))
    (pad 4 thru_hole oval (at 10.5 0 90) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 53 +24V))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 53 +24V))
    (pad 2 thru_hole oval (at 3.5 0 90) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 173 "Net-(P9-Pad2)"))
    (pad 3 thru_hole oval (at 7 0 90) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (model ${KIPRJMOD}/stmbl.pretty/akl182_6.wrl
      (at (xyz 0.7893700787401575 0.125984251968504 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 180))
    )
  )

  (module stmbl:akl182-6 (layer B.Cu) (tedit 57D73CD8) (tstamp 577578AC)
    (at 184 42)
    (path /56590966/56591923/56602281)
    (fp_text reference P5 (at -0.6 3) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value CONN_01X06 (at 6 -9.8) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.55 -7.9) (end -2.55 2.3) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.55 2.3) (end 20.05 2.3) (layer B.SilkS) (width 0.15))
    (fp_line (start 20.05 2.3) (end 20.05 -7.9) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.55 -7.9) (end 20.05 -7.9) (layer B.SilkS) (width 0.15))
    (pad 6 thru_hole oval (at 17.5 0) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 56 "Net-(D5-Pad2)"))
    (pad 5 thru_hole oval (at 14 0) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 53 +24V))
    (pad 4 thru_hole oval (at 10.5 0) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 55 "Net-(D3-Pad2)"))
    (pad 1 thru_hole oval (at 0 0) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 53 +24V))
    (pad 2 thru_hole oval (at 3.5 0) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 54 "Net-(D2-Pad2)"))
    (pad 3 thru_hole oval (at 7 0) (size 2.5 3.5) (drill 1.5 (offset 0 -0.5)) (layers *.Cu *.Mask B.SilkS)
      (net 53 +24V))
    (model ${KIPRJMOD}/stmbl.pretty/akl182_6.wrl
      (at (xyz 0.7893700787401575 0.125984251968504 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 180))
    )
  )

  (module stmbl:RJ45_LED (layer B.Cu) (tedit 57D70F56) (tstamp 577597F7)
    (at 274 44 90)
    (path /56590966/56591919/565DD759)
    (fp_text reference J3 (at 7 -16.5 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value RJ45_LED (at -5 1 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 8.25 -15.5) (end 8.25 0) (layer B.SilkS) (width 0.15))
    (fp_line (start -8.25 -15.5) (end 8.25 -15.5) (layer B.SilkS) (width 0.15))
    (fp_line (start -8.25 0) (end -8.25 -15.5) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.25 0) (end -8.25 0) (layer B.SilkS) (width 0.15))
    (pad "" np_thru_hole circle (at 6.35 -5.4 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 0.5))
    (pad "" np_thru_hole circle (at -6.35 -5.4 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 0.5))
    (pad 13 thru_hole circle (at 8.25 -8.83 90) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 "Net-(C17-Pad1)"))
    (pad 13 thru_hole circle (at -8.25 -8.83 90) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 "Net-(C17-Pad1)"))
    (pad 1 thru_hole circle (at -3.57 -7.94 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 82 "Net-(J3-Pad1)"))
    (pad 2 thru_hole circle (at -2.55 -9.72 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 83 "Net-(J3-Pad2)"))
    (pad 3 thru_hole circle (at -1.53 -7.94 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 84 "Net-(J3-Pad3)"))
    (pad 4 thru_hole circle (at -0.51 -9.72 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 87 "Net-(J3-Pad4)"))
    (pad 5 thru_hole circle (at 0.51 -7.94 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 86 "Net-(J3-Pad5)"))
    (pad 6 thru_hole circle (at 1.53 -9.72 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 85 "Net-(J3-Pad6)"))
    (pad 7 thru_hole circle (at 2.55 -7.94 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 88 "Net-(J3-Pad7)"))
    (pad 8 thru_hole circle (at 3.57 -9.72 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 89 "Net-(J3-Pad8)"))
    (pad 9 thru_hole circle (at 6.86 -14.58 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole circle (at 4.57 -14.58 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 139 "Net-(J3-Pad10)"))
    (pad 11 thru_hole circle (at -4.57 -14.58 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole circle (at -6.86 -14.58 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 138 "Net-(J3-Pad12)"))
    (model ${KIPRJMOD}/stmbl.pretty/rj45.wrl
      (at (xyz 0.3248031496062992 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 180))
    )
  )

  (module stmbl:RJ45_LED (layer B.Cu) (tedit 57D70F56) (tstamp 577597DD)
    (at 274 60.5 90)
    (path /56590966/5659191C/565DFE88)
    (fp_text reference J2 (at 7 -16.5 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value RJ45_LED (at -5 1 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 8.25 -15.5) (end 8.25 0) (layer B.SilkS) (width 0.15))
    (fp_line (start -8.25 -15.5) (end 8.25 -15.5) (layer B.SilkS) (width 0.15))
    (fp_line (start -8.25 0) (end -8.25 -15.5) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.25 0) (end -8.25 0) (layer B.SilkS) (width 0.15))
    (pad "" np_thru_hole circle (at 6.35 -5.4 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 0.5))
    (pad "" np_thru_hole circle (at -6.35 -5.4 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 0.5))
    (pad 13 thru_hole circle (at 8.25 -8.83 90) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 13 thru_hole circle (at -8.25 -8.83 90) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 1 thru_hole circle (at -3.57 -7.94 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 72 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at -2.55 -9.72 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 74 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at -1.53 -7.94 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 67 "Net-(J2-Pad3)"))
    (pad 4 thru_hole circle (at -0.51 -9.72 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 102 "Net-(J2-Pad4)"))
    (pad 5 thru_hole circle (at 0.51 -7.94 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 101 "Net-(J2-Pad5)"))
    (pad 6 thru_hole circle (at 1.53 -9.72 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 70 "Net-(J2-Pad6)"))
    (pad 7 thru_hole circle (at 2.55 -7.94 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 163 "Net-(C114-Pad1)"))
    (pad 8 thru_hole circle (at 3.57 -9.72 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole circle (at 6.86 -14.58 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole circle (at 4.57 -14.58 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 137 "Net-(J2-Pad10)"))
    (pad 11 thru_hole circle (at -4.57 -14.58 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole circle (at -6.86 -14.58 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 134 "Net-(J2-Pad12)"))
    (model ${KIPRJMOD}/stmbl.pretty/rj45.wrl
      (at (xyz 0.3248031496062992 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 180))
    )
  )

  (module stmbl:RJ45_LED (layer B.Cu) (tedit 57D70F56) (tstamp 577597C3)
    (at 274 77 90)
    (path /56590966/565F7162/565DFE88)
    (fp_text reference J1 (at 7 -16.5 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value RJ45_LED (at -5 1 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 8.25 -15.5) (end 8.25 0) (layer B.SilkS) (width 0.15))
    (fp_line (start -8.25 -15.5) (end 8.25 -15.5) (layer B.SilkS) (width 0.15))
    (fp_line (start -8.25 0) (end -8.25 -15.5) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.25 0) (end -8.25 0) (layer B.SilkS) (width 0.15))
    (pad "" np_thru_hole circle (at 6.35 -5.4 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 0.5))
    (pad "" np_thru_hole circle (at -6.35 -5.4 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 0.5))
    (pad 13 thru_hole circle (at 8.25 -8.83 90) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 13 thru_hole circle (at -8.25 -8.83 90) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 1 thru_hole circle (at -3.57 -7.94 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 71 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -2.55 -9.72 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 73 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -1.53 -7.94 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 68 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -0.51 -9.72 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 100 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at 0.51 -7.94 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 99 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at 1.53 -9.72 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 69 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at 2.55 -7.94 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 164 "Net-(C117-Pad1)"))
    (pad 8 thru_hole circle (at 3.57 -9.72 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole circle (at 6.86 -14.58 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole circle (at 4.57 -14.58 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 136 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at -4.57 -14.58 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole circle (at -6.86 -14.58 90) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 135 "Net-(J1-Pad12)"))
    (model ${KIPRJMOD}/stmbl.pretty/rj45.wrl
      (at (xyz 0.3248031496062992 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 180))
    )
  )

  (gr_circle (center 192.5 119.5) (end 192.5 122) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 251.5 119.5) (end 251.5 122) (layer Edge.Cuts) (width 0.15))
  (target plus (at 273 135) (size 5) (width 0.15) (layer Edge.Cuts))
  (target plus (at 273 135) (size 5) (width 0.15) (layer Edge.Cuts) (tstamp 577593C1))
  (target plus (at 273 135) (size 5) (width 0.15) (layer Edge.Cuts))
  (gr_line (start 185 87) (end 273 87) (layer F.SilkS) (width 0.15))
  (gr_arc (start 175 37) (end 173 37) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 176.5 77) (end 176.5 80.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 183 82.5) (end 183 80.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 187 133) (end 187 135) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 271 133) (end 273 133) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 271 37) (end 271 35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 185 86) (end 273 86) (layer F.SilkS) (width 0.15))
  (gr_line (start 185 82.5) (end 185 86.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.5 80.5) (end 183 80.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173 37) (end 173 77) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 271 35) (end 175 35) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 273 86) (end 273 37) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 273 133) (end 273 86) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187 135) (end 271 135) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 185 86.5) (end 185 133) (layer Edge.Cuts) (width 0.15))

  (segment (start 212.45 112.45) (end 212.5 112.5) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 241 60.25) (end 243.5475 60.25) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 243.5475 60.25) (end 246.155 57.6425) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 246.155 57.6425) (end 246.155 57.325) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 246.155 57.325) (end 246.155 55.595) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 246.155 55.595) (end 246.25 55.5) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 246.5 54) (end 246.5 55.25) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 246.5 55.25) (end 246.25 55.5) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 243 54) (end 244.75 54) (width 0.25) (layer F.Cu) (net 21))
  (segment (start 244.75 54) (end 244.75 55.5) (width 0.25) (layer F.Cu) (net 21))
  (segment (start 244.75 55.5) (end 244.75 57.19) (width 0.25) (layer F.Cu) (net 21))
  (segment (start 244.75 57.19) (end 244.885 57.325) (width 0.25) (layer F.Cu) (net 21))
  (segment (start 246.75 65.25) (end 245 65.25) (width 0.25) (layer F.Cu) (net 24))
  (segment (start 241 62) (end 243.5275 62) (width 0.25) (layer F.Cu) (net 24))
  (segment (start 243.5275 62) (end 244.885 63.3575) (width 0.25) (layer F.Cu) (net 24))
  (segment (start 244.885 63.3575) (end 244.885 63.675) (width 0.25) (layer F.Cu) (net 24))
  (segment (start 244.885 63.675) (end 244.885 65.135) (width 0.25) (layer F.Cu) (net 24))
  (segment (start 244.885 65.135) (end 245 65.25) (width 0.25) (layer F.Cu) (net 24))
  (segment (start 242 66.75) (end 243.25 66.75) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 243.25 66.75) (end 243.5 67) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 243.5 67) (end 243.5 65.25) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 243.615 63.675) (end 243.615 65.135) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 243.615 65.135) (end 243.5 65.25) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 206 98.51) (end 205.49 98) (width 0.25) (layer F.Cu) (net 33))
  (segment (start 211 98.43) (end 210.57 98) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 216 98.35) (end 215.65 98) (width 0.25) (layer F.Cu) (net 37))
  (segment (start 242 65.25) (end 242 64.02) (width 0.25) (layer F.Cu) (net 78))
  (segment (start 242 64.02) (end 242.345 63.675) (width 0.25) (layer F.Cu) (net 78))
  (segment (start 243.615 57.325) (end 243.615 56.115) (width 0.25) (layer F.Cu) (net 79))
  (segment (start 243.615 56.115) (end 243 55.5) (width 0.25) (layer F.Cu) (net 79))
  (segment (start 261.25 48) (end 263.25 48) (width 0.25) (layer F.Cu) (net 82))
  (segment (start 261.25 48) (end 261.25 48.5) (width 0.25) (layer F.Cu) (net 82))
  (segment (start 261.25 48.5) (end 259.865001 49.884999) (width 0.25) (layer F.Cu) (net 82))
  (segment (start 259.865001 49.884999) (end 257.530601 49.884999) (width 0.25) (layer F.Cu) (net 82))
  (segment (start 257.530601 49.884999) (end 257.2806 50.135) (width 0.25) (layer F.Cu) (net 82))
  (segment (start 257.2806 50.135) (end 256.294 50.135) (width 0.25) (layer F.Cu) (net 82))
  (segment (start 263.25 48) (end 266.39 48) (width 0.25) (layer F.Cu) (net 82))
  (segment (start 266.39 48) (end 266.82 47.57) (width 0.25) (layer F.Cu) (net 82))
  (segment (start 256.294 48.865) (end 256.7258 48.865) (width 0.25) (layer F.Cu) (net 83))
  (segment (start 256.7258 48.865) (end 258.3408 47.25) (width 0.25) (layer F.Cu) (net 83))
  (segment (start 258.3408 47.25) (end 262.3 47.25) (width 0.25) (layer F.Cu) (net 83))
  (segment (start 262.3 47.25) (end 263.05 46.5) (width 0.25) (layer F.Cu) (net 83))
  (segment (start 263.05 46.5) (end 263.25 46.5) (width 0.25) (layer F.Cu) (net 83))
  (segment (start 263.25 46.5) (end 264.99 46.5) (width 0.25) (layer F.Cu) (net 83))
  (segment (start 264.99 46.5) (end 265.04 46.55) (width 0.25) (layer F.Cu) (net 83))
  (segment (start 270 46) (end 267.883 46) (width 0.25) (layer F.Cu) (net 83))
  (segment (start 267.883 46) (end 267.333 46.55) (width 0.25) (layer F.Cu) (net 83))
  (segment (start 267.333 46.55) (end 265.959238 46.55) (width 0.25) (layer F.Cu) (net 83))
  (segment (start 265.959238 46.55) (end 265.04 46.55) (width 0.25) (layer F.Cu) (net 83))
  (segment (start 260.5 44.75) (end 256.409 44.75) (width 0.25) (layer F.Cu) (net 84))
  (segment (start 256.409 44.75) (end 256.294 44.635) (width 0.25) (layer F.Cu) (net 84))
  (segment (start 260.5 44.75) (end 261.2 44.75) (width 0.25) (layer F.Cu) (net 84))
  (segment (start 261.2 44.75) (end 261.98 45.53) (width 0.25) (layer F.Cu) (net 84))
  (segment (start 261.98 45.53) (end 265.900762 45.53) (width 0.25) (layer F.Cu) (net 84))
  (segment (start 265.900762 45.53) (end 266.82 45.53) (width 0.25) (layer F.Cu) (net 84))
  (segment (start 266.82 45.53) (end 268.22 45.53) (width 0.25) (layer F.Cu) (net 84))
  (segment (start 268.22 45.53) (end 268.5 45.25) (width 0.25) (layer F.Cu) (net 84))
  (segment (start 258.5 43.25) (end 259.28 42.47) (width 0.25) (layer B.Cu) (net 85))
  (segment (start 259.28 42.47) (end 265.04 42.47) (width 0.25) (layer B.Cu) (net 85))
  (segment (start 258.385 43.365) (end 258.5 43.25) (width 0.25) (layer F.Cu) (net 85))
  (via (at 258.5 43.25) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 85))
  (segment (start 256.294 43.365) (end 258.385 43.365) (width 0.25) (layer F.Cu) (net 85))
  (segment (start 265.04 42.47) (end 268.5 42.47) (width 0.25) (layer F.Cu) (net 85))
  (segment (start 268.5 42.47) (end 269.97 42.47) (width 0.25) (layer F.Cu) (net 85))
  (segment (start 268.5 43.75) (end 268.5 42.47) (width 0.25) (layer F.Cu) (net 85))
  (segment (start 269.97 42.47) (end 270 42.5) (width 0.25) (layer F.Cu) (net 85))
  (segment (start 256.294 39.135) (end 257.2806 39.135) (width 0.25) (layer F.Cu) (net 86))
  (segment (start 257.2806 39.135) (end 259.6456 41.5) (width 0.25) (layer F.Cu) (net 86))
  (segment (start 259.6456 41.5) (end 260.55 41.5) (width 0.25) (layer F.Cu) (net 86))
  (segment (start 260.55 41.5) (end 261.25 41.5) (width 0.25) (layer F.Cu) (net 86))
  (segment (start 263.25 43.25) (end 263.05 43.25) (width 0.25) (layer F.Cu) (net 86))
  (segment (start 263.05 43.25) (end 261.3 41.5) (width 0.25) (layer F.Cu) (net 86))
  (segment (start 261.3 41.5) (end 261.25 41.5) (width 0.25) (layer F.Cu) (net 86))
  (segment (start 263.25 43.25) (end 264.376998 43.25) (width 0.25) (layer F.Cu) (net 86))
  (segment (start 264.376998 43.25) (end 264.616998 43.49) (width 0.25) (layer F.Cu) (net 86))
  (segment (start 264.616998 43.49) (end 265.900762 43.49) (width 0.25) (layer F.Cu) (net 86))
  (segment (start 265.900762 43.49) (end 266.82 43.49) (width 0.25) (layer F.Cu) (net 86))
  (segment (start 256.294 37.865) (end 255.8622 37.865) (width 0.25) (layer F.Cu) (net 87))
  (segment (start 255.8622 37.865) (end 255.23239 38.49481) (width 0.25) (layer F.Cu) (net 87))
  (segment (start 255.23239 38.49481) (end 255.23239 39.395875) (width 0.25) (layer F.Cu) (net 87))
  (segment (start 255.23239 39.395875) (end 255.601325 39.76481) (width 0.25) (layer F.Cu) (net 87))
  (segment (start 255.601325 39.76481) (end 257.274 39.76481) (width 0.25) (layer F.Cu) (net 87))
  (segment (start 262.55 44.05) (end 262.55 44.25) (width 0.25) (layer F.Cu) (net 87))
  (segment (start 257.274 39.76481) (end 260.184189 42.674999) (width 0.25) (layer F.Cu) (net 87))
  (segment (start 260.184189 42.674999) (end 261.174999 42.674999) (width 0.25) (layer F.Cu) (net 87))
  (segment (start 261.174999 42.674999) (end 262.55 44.05) (width 0.25) (layer F.Cu) (net 87))
  (segment (start 262.55 44.25) (end 263.05 44.75) (width 0.25) (layer F.Cu) (net 87))
  (segment (start 263.05 44.75) (end 263.25 44.75) (width 0.25) (layer F.Cu) (net 87))
  (segment (start 263.25 44.75) (end 264.8 44.75) (width 0.25) (layer F.Cu) (net 87))
  (segment (start 264.8 44.75) (end 265.04 44.51) (width 0.25) (layer F.Cu) (net 87))
  (segment (start 270 44.25) (end 269.5 44.25) (width 0.25) (layer F.Cu) (net 87))
  (segment (start 269.5 44.25) (end 269.24 44.51) (width 0.25) (layer F.Cu) (net 87))
  (segment (start 265.959238 44.51) (end 265.04 44.51) (width 0.25) (layer F.Cu) (net 87))
  (segment (start 269.24 44.51) (end 265.959238 44.51) (width 0.25) (layer F.Cu) (net 87))
  (segment (start 263.25 41.5) (end 264.566998 41.5) (width 0.25) (layer F.Cu) (net 88))
  (segment (start 264.566998 41.5) (end 264.616998 41.45) (width 0.25) (layer F.Cu) (net 88))
  (segment (start 264.616998 41.45) (end 265.900762 41.45) (width 0.25) (layer F.Cu) (net 88))
  (segment (start 265.900762 41.45) (end 266.82 41.45) (width 0.25) (layer F.Cu) (net 88))
  (segment (start 263.25 40) (end 264.61 40) (width 0.25) (layer F.Cu) (net 89))
  (segment (start 264.61 40) (end 265.04 40.43) (width 0.25) (layer F.Cu) (net 89))
  (segment (start 270 40.75) (end 267.563002 40.75) (width 0.25) (layer F.Cu) (net 89))
  (segment (start 267.563002 40.75) (end 267.243002 40.43) (width 0.25) (layer F.Cu) (net 89))
  (segment (start 267.243002 40.43) (end 265.959238 40.43) (width 0.25) (layer F.Cu) (net 89))
  (segment (start 265.959238 40.43) (end 265.04 40.43) (width 0.25) (layer F.Cu) (net 89))
  (segment (start 237.75 111) (end 238.049999 111.299999) (width 0.25) (layer F.Cu) (net 110))
  (segment (start 238.049999 111.299999) (end 242.600001 111.299999) (width 0.25) (layer F.Cu) (net 110))
  (segment (start 242.600001 111.299999) (end 242.65 111.25) (width 0.25) (layer F.Cu) (net 110))
  (segment (start 225.81 98) (end 225.81 98.25) (width 0.25) (layer B.Cu) (net 110))
  (segment (start 225.81 98.25) (end 226.81 99.25) (width 0.25) (layer B.Cu) (net 110))
  (segment (start 226.81 99.25) (end 227.640293 99.25) (width 0.25) (layer B.Cu) (net 110))
  (segment (start 227.640293 99.25) (end 230.69501 102.304717) (width 0.25) (layer B.Cu) (net 110))
  (segment (start 230.69501 102.304717) (end 230.69501 104.695032) (width 0.25) (layer B.Cu) (net 110))
  (segment (start 230.69501 104.695032) (end 236.999978 111) (width 0.25) (layer B.Cu) (net 110))
  (via (at 237.75 111) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 110))
  (segment (start 236.999978 111) (end 237.75 111) (width 0.25) (layer B.Cu) (net 110))
  (segment (start 228.35 98) (end 228.35 98.25) (width 0.25) (layer B.Cu) (net 128))
  (segment (start 228.35 98.25) (end 229.35 99.25) (width 0.25) (layer B.Cu) (net 128))
  (segment (start 229.35 99.25) (end 230.180293 99.25) (width 0.25) (layer B.Cu) (net 128))
  (segment (start 230.180293 99.25) (end 233.5 102.569707) (width 0.25) (layer B.Cu) (net 128))
  (segment (start 233.5 102.569707) (end 233.5 106.57502) (width 0.25) (layer B.Cu) (net 128))
  (segment (start 233.5 106.57502) (end 236.950001 110.025021) (width 0.25) (layer B.Cu) (net 128))
  (segment (start 236.950001 110.025021) (end 237.25 110.32502) (width 0.25) (layer B.Cu) (net 128))
  (segment (start 237.25 110.32502) (end 237.674264 110.32502) (width 0.25) (layer F.Cu) (net 128))
  (segment (start 237.674264 110.32502) (end 237.749284 110.25) (width 0.25) (layer F.Cu) (net 128))
  (segment (start 237.749284 110.25) (end 241.75 110.25) (width 0.25) (layer F.Cu) (net 128))
  (segment (start 241.75 110.25) (end 242.65 110.25) (width 0.25) (layer F.Cu) (net 128))
  (via (at 237.25 110.32502) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 128))
  (segment (start 237.25 110.25) (end 237.25 110.32502) (width 0.25) (layer B.Cu) (net 128))
  (segment (start 230.89 98) (end 230.89 99.25) (width 0.25) (layer F.Cu) (net 129))
  (segment (start 231.08499 99.44499) (end 231.08499 103.695283) (width 0.25) (layer F.Cu) (net 129))
  (segment (start 231.08499 103.695283) (end 237.089717 109.70001) (width 0.25) (layer F.Cu) (net 129))
  (segment (start 237.089717 109.70001) (end 242.60001 109.70001) (width 0.25) (layer F.Cu) (net 129))
  (segment (start 230.89 99.25) (end 231.08499 99.44499) (width 0.25) (layer F.Cu) (net 129))
  (segment (start 242.60001 109.70001) (end 242.65 109.75) (width 0.25) (layer F.Cu) (net 129))
  (segment (start 233.43 98) (end 233.43 103.500293) (width 0.25) (layer F.Cu) (net 130))
  (segment (start 238.679707 108.75) (end 241.75 108.75) (width 0.25) (layer F.Cu) (net 130))
  (segment (start 233.43 103.500293) (end 238.679707 108.75) (width 0.25) (layer F.Cu) (net 130))
  (segment (start 241.75 108.75) (end 242.65 108.75) (width 0.25) (layer F.Cu) (net 130))
  (segment (start 235.97 98) (end 235.97 103.500293) (width 0.25) (layer F.Cu) (net 131))
  (segment (start 235.97 103.500293) (end 240.219707 107.75) (width 0.25) (layer F.Cu) (net 131))
  (segment (start 240.219707 107.75) (end 241.75 107.75) (width 0.25) (layer F.Cu) (net 131))
  (segment (start 241.75 107.75) (end 242.65 107.75) (width 0.25) (layer F.Cu) (net 131))
  (segment (start 241.75 109.25) (end 242.65 109.25) (width 0.25) (layer F.Cu) (net 132))
  (segment (start 238.543297 109.25) (end 241.75 109.25) (width 0.25) (layer F.Cu) (net 132))
  (segment (start 232.16 103) (end 232.293297 103) (width 0.25) (layer F.Cu) (net 132))
  (segment (start 232.293297 103) (end 238.543297 109.25) (width 0.25) (layer F.Cu) (net 132))
  (segment (start 234.7 103) (end 234.7 103.25) (width 0.25) (layer F.Cu) (net 133))
  (segment (start 234.7 103.25) (end 239.7 108.25) (width 0.25) (layer F.Cu) (net 133))
  (segment (start 239.7 108.25) (end 241.75 108.25) (width 0.25) (layer F.Cu) (net 133))
  (segment (start 241.75 108.25) (end 242.65 108.25) (width 0.25) (layer F.Cu) (net 133))
  (segment (start 256.294 42.095) (end 258.96778 42.095) (width 0.25) (layer F.Cu) (net 142))
  (segment (start 258.96778 42.095) (end 260.12278 43.25) (width 0.25) (layer F.Cu) (net 142))
  (segment (start 260.12278 43.25) (end 260.5 43.25) (width 0.25) (layer F.Cu) (net 142))
  (segment (start 256.294 36.595) (end 256.7258 36.595) (width 0.25) (layer F.Cu) (net 142))
  (segment (start 256.7258 36.595) (end 258.585799 38.454999) (width 0.25) (layer F.Cu) (net 142))
  (segment (start 258.585799 38.454999) (end 260.204999 38.454999) (width 0.25) (layer F.Cu) (net 142))
  (segment (start 261.25 39.5) (end 261.25 40) (width 0.25) (layer F.Cu) (net 142))
  (segment (start 260.204999 38.454999) (end 261.25 39.5) (width 0.25) (layer F.Cu) (net 142))
  (segment (start 256.294 47.595) (end 257.2806 47.595) (width 0.25) (layer F.Cu) (net 142))
  (segment (start 257.2806 47.595) (end 258.3756 46.5) (width 0.25) (layer F.Cu) (net 142))
  (segment (start 258.3756 46.5) (end 260.55 46.5) (width 0.25) (layer F.Cu) (net 142))
  (segment (start 260.55 46.5) (end 261.25 46.5) (width 0.25) (layer F.Cu) (net 142))
  (segment (start 242.27 57.25) (end 242.345 57.325) (width 0.25) (layer F.Cu) (net 175))

  (zone (net 16) (net_name VPP) (layer B.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads yes (clearance 1))
    (min_thickness 1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 218 101.5) (xy 221 101.5) (xy 222 102.5) (xy 222 104) (xy 224 106)
        (xy 224 112.5) (xy 232 120.5) (xy 233.75 122.25) (xy 233.75 123.75) (xy 232 125.5)
        (xy 212 125.5) (xy 204.5 125.5) (xy 193 114) (xy 192.5 114) (xy 192 113.5)
        (xy 192 112) (xy 193 111) (xy 195 111) (xy 204 120) (xy 207 120)
        (xy 215 112) (xy 215 106) (xy 217 104) (xy 217 102.5)
      )
    )
    (filled_polygon
      (pts
        (xy 221.5 102.707106) (xy 221.5 104) (xy 221.53806 104.191342) (xy 221.646447 104.353553) (xy 223.5 106.207106)
        (xy 223.5 112.5) (xy 223.53806 112.691342) (xy 223.646447 112.853553) (xy 233.25 122.457106) (xy 233.25 123.542894)
        (xy 231.792894 125) (xy 204.707106 125) (xy 193.353553 113.646447) (xy 193.191342 113.53806) (xy 193 113.5)
        (xy 192.707106 113.5) (xy 192.5 113.292894) (xy 192.5 112.207106) (xy 193.207106 111.5) (xy 194.792894 111.5)
        (xy 203.646447 120.353553) (xy 203.808658 120.46194) (xy 204 120.5) (xy 207 120.5) (xy 207.191342 120.46194)
        (xy 207.353553 120.353553) (xy 215.353553 112.353553) (xy 215.46194 112.191342) (xy 215.5 112) (xy 215.5 106.207106)
        (xy 217.353553 104.353553) (xy 217.46194 104.191342) (xy 217.5 104) (xy 217.5 102.707106) (xy 218.207106 102)
        (xy 220.792894 102)
      )
    )
  )
  (zone (net 16) (net_name VPP) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads yes (clearance 1))
    (min_thickness 1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 232 120.5) (xy 233.75 122.25) (xy 233.75 123.75) (xy 232 125.5) (xy 212 125.5)
        (xy 204.5 125.5) (xy 193 114) (xy 192.5 114) (xy 192 113.5) (xy 192 112)
        (xy 193 111) (xy 195 111) (xy 204.5 120.5)
      )
    )
    (filled_polygon
      (pts
        (xy 204.146447 120.853553) (xy 204.308658 120.96194) (xy 204.5 121) (xy 231.792894 121) (xy 233.25 122.457106)
        (xy 233.25 123.542894) (xy 231.792894 125) (xy 204.707106 125) (xy 193.353553 113.646447) (xy 193.191342 113.53806)
        (xy 193 113.5) (xy 192.707106 113.5) (xy 192.5 113.292894) (xy 192.5 112.207106) (xy 193.207106 111.5)
        (xy 194.792894 111.5)
      )
    )
  )
  (zone (net 4) (net_name GNDPWR) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 192 107) (xy 193 106) (xy 197.5 106) (xy 205 113.5) (xy 217.25 113.5)
        (xy 217.75 113) (xy 217.75 112) (xy 219.75 112) (xy 232.75 112) (xy 234.75 114)
        (xy 239.5 114) (xy 240.75 115.25) (xy 240.75 116.75) (xy 239 118.5) (xy 205 118.5)
        (xy 195.5 109) (xy 193 109) (xy 192 108)
      )
    )
    (filled_polygon
      (pts
        (xy 204.646447 113.853553) (xy 204.808658 113.96194) (xy 205 114) (xy 217.25 114) (xy 217.441342 113.96194)
        (xy 217.603553 113.853553) (xy 218.103553 113.353553) (xy 218.21194 113.191342) (xy 218.25 113) (xy 218.25 112.5)
        (xy 232.542894 112.5) (xy 234.396447 114.353553) (xy 234.558658 114.46194) (xy 234.75 114.5) (xy 239.292894 114.5)
        (xy 240.25 115.457106) (xy 240.25 116.542894) (xy 238.792894 118) (xy 205.207106 118) (xy 195.853553 108.646447)
        (xy 195.691342 108.53806) (xy 195.5 108.5) (xy 193.207106 108.5) (xy 192.5 107.792894) (xy 192.5 107.207106)
        (xy 193.207106 106.5) (xy 197.292894 106.5)
      )
    )
  )
  (zone (net 4) (net_name GNDPWR) (layer B.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193 109) (xy 192 108) (xy 192 107) (xy 193 106) (xy 197.5 106)
        (xy 206.5 115) (xy 206.5 116.5) (xy 205.5 117.5) (xy 204 117.5) (xy 195.5 109)
      )
    )
    (filled_polygon
      (pts
        (xy 206 115.207106) (xy 206 116.292894) (xy 205.292894 117) (xy 204.207106 117) (xy 195.853553 108.646447)
        (xy 195.691342 108.53806) (xy 195.5 108.5) (xy 193.207106 108.5) (xy 192.5 107.792894) (xy 192.5 107.207106)
        (xy 193.207106 106.5) (xy 197.292894 106.5)
      )
    )
  )
  (zone (net 33) (net_name /hv/back-emf/W) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193 99) (xy 192 100) (xy 192 101) (xy 193 102) (xy 200 102)
        (xy 202 100) (xy 206 100) (xy 207 99) (xy 207 97.5) (xy 206.5 97)
        (xy 200.5 97) (xy 198.5 99)
      )
    )
    (filled_polygon
      (pts
        (xy 206.5 97.707106) (xy 206.5 98.792894) (xy 205.792894 99.5) (xy 202 99.5) (xy 201.808658 99.53806)
        (xy 201.646447 99.646447) (xy 199.792894 101.5) (xy 193.207106 101.5) (xy 192.5 100.792894) (xy 192.5 100.207106)
        (xy 193.207106 99.5) (xy 198.5 99.5) (xy 198.691342 99.46194) (xy 198.853553 99.353553) (xy 200.707106 97.5)
        (xy 206.292894 97.5)
      )
    )
  )
  (zone (net 35) (net_name /hv/back-emf/V) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193 97) (xy 197.5 97) (xy 199 95.5) (xy 207.5 95.5) (xy 208.5 96.5)
        (xy 208.5 100) (xy 211 100) (xy 212 99) (xy 212 97.5) (xy 212 96)
        (xy 209 93) (xy 197.5 93) (xy 196.5 94) (xy 193 94) (xy 192 95)
        (xy 192 96)
      )
    )
    (filled_polygon
      (pts
        (xy 211.5 96.207106) (xy 211.5 98.792894) (xy 210.792894 99.5) (xy 209 99.5) (xy 209 96.5)
        (xy 208.96194 96.308658) (xy 208.853553 96.146447) (xy 207.853553 95.146447) (xy 207.691342 95.03806) (xy 207.5 95)
        (xy 199 95) (xy 198.808658 95.03806) (xy 198.646447 95.146447) (xy 197.292894 96.5) (xy 193.207106 96.5)
        (xy 192.5 95.792894) (xy 192.5 95.207106) (xy 193.207106 94.5) (xy 196.5 94.5) (xy 196.691342 94.46194)
        (xy 196.853553 94.353553) (xy 197.707106 93.5) (xy 208.792894 93.5)
      )
    )
  )
  (zone (net 37) (net_name /hv/back-emf/U) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193 92) (xy 195.5 92) (xy 196 91.5) (xy 210 91.5) (xy 213.5 95)
        (xy 213.5 100) (xy 216 100) (xy 217 99) (xy 217 94.25) (xy 211.75 89)
        (xy 196 89) (xy 193 89) (xy 192 90) (xy 192 91) (xy 192 91)
      )
    )
    (filled_polygon
      (pts
        (xy 216.5 94.457106) (xy 216.5 98.792894) (xy 215.792894 99.5) (xy 214 99.5) (xy 214 95)
        (xy 213.96194 94.808658) (xy 213.853553 94.646447) (xy 210.353553 91.146447) (xy 210.191342 91.03806) (xy 210 91)
        (xy 196 91) (xy 195.808658 91.03806) (xy 195.646447 91.146447) (xy 195.292894 91.5) (xy 193.207106 91.5)
        (xy 192.5 90.792894) (xy 192.5 90.207106) (xy 193.207106 89.5) (xy 211.542894 89.5)
      )
    )
  )
  (zone (net 33) (net_name /hv/back-emf/W) (layer B.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193 102) (xy 192 101) (xy 192 100) (xy 193 99) (xy 198.5 99)
        (xy 200.5 97) (xy 206.5 97) (xy 207 97.5) (xy 207 99) (xy 206 100)
        (xy 202 100) (xy 200 102)
      )
    )
    (filled_polygon
      (pts
        (xy 206.5 97.707106) (xy 206.5 98.792894) (xy 205.792894 99.5) (xy 202 99.5) (xy 201.808658 99.53806)
        (xy 201.646447 99.646447) (xy 199.792894 101.5) (xy 193.207106 101.5) (xy 192.5 100.792894) (xy 192.5 100.207106)
        (xy 193.207106 99.5) (xy 198.5 99.5) (xy 198.691342 99.46194) (xy 198.853553 99.353553) (xy 200.707106 97.5)
        (xy 206.292894 97.5)
      )
    )
  )
  (zone (net 35) (net_name /hv/back-emf/V) (layer B.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193 97) (xy 192 96) (xy 192 95) (xy 193 94) (xy 196.5 94)
        (xy 197.5 93) (xy 209 93) (xy 212 96) (xy 212 98.5) (xy 211 99.5)
        (xy 210 99.5) (xy 209 98.5) (xy 209 97) (xy 207.5 95.5) (xy 199 95.5)
        (xy 197.5 97)
      )
    )
    (filled_polygon
      (pts
        (xy 211.5 96.207106) (xy 211.5 98.292894) (xy 210.792894 99) (xy 210.207106 99) (xy 209.5 98.292894)
        (xy 209.5 97) (xy 209.46194 96.808658) (xy 209.353553 96.646447) (xy 207.853553 95.146447) (xy 207.691342 95.03806)
        (xy 207.5 95) (xy 199 95) (xy 198.808658 95.03806) (xy 198.646447 95.146447) (xy 197.292894 96.5)
        (xy 193.207106 96.5) (xy 192.5 95.792894) (xy 192.5 95.207106) (xy 193.207106 94.5) (xy 196.5 94.5)
        (xy 196.691342 94.46194) (xy 196.853553 94.353553) (xy 197.707106 93.5) (xy 208.792894 93.5)
      )
    )
  )
  (zone (net 37) (net_name /hv/back-emf/U) (layer B.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193 92) (xy 192 91) (xy 192 90) (xy 193 89) (xy 196 89)
        (xy 211.75 89) (xy 217 94.25) (xy 217 98.5) (xy 216 99.5) (xy 215 99.5)
        (xy 214 98.5) (xy 214 95.5) (xy 210 91.5) (xy 196 91.5) (xy 195.5 92)
      )
    )
    (filled_polygon
      (pts
        (xy 216.5 94.457106) (xy 216.5 98.292894) (xy 215.792894 99) (xy 215.207106 99) (xy 214.5 98.292894)
        (xy 214.5 95.5) (xy 214.46194 95.308658) (xy 214.353553 95.146447) (xy 210.353553 91.146447) (xy 210.191342 91.03806)
        (xy 210 91) (xy 196 91) (xy 195.808658 91.03806) (xy 195.646447 91.146447) (xy 195.292894 91.5)
        (xy 193.207106 91.5) (xy 192.5 90.792894) (xy 192.5 90.207106) (xy 193.207106 89.5) (xy 211.542894 89.5)
      )
    )
  )
  (zone (net 16) (net_name VPP) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads yes (clearance 1))
    (min_thickness 1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 219.75 104.75) (xy 221 103.5) (xy 221 102.5) (xy 220 101.5) (xy 219 101.5)
        (xy 217.75 102.75) (xy 217.75 107.5) (xy 217.75 108.5) (xy 219.75 108.5)
      )
    )
    (filled_polygon
      (pts
        (xy 220.5 102.707106) (xy 220.5 103.292894) (xy 219.396447 104.396447) (xy 219.28806 104.558658) (xy 219.25 104.75)
        (xy 219.25 108) (xy 218.25 108) (xy 218.25 102.957106) (xy 219.207106 102) (xy 219.792894 102)
      )
    )
  )
  (zone (net 75) (net_name /hv/driver/CUH) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 225.5 104.25) (xy 224.75 105) (xy 224.75 107) (xy 221.25 107) (xy 221.25 105.75)
        (xy 223.5 103.5) (xy 223.5 102.25) (xy 224 101.75) (xy 225 101.75) (xy 225.5 102.25)
      )
    )
    (filled_polygon
      (pts
        (xy 225 102.457106) (xy 225 104.042894) (xy 224.396447 104.646447) (xy 224.28806 104.808658) (xy 224.25 105)
        (xy 224.25 106.5) (xy 221.75 106.5) (xy 221.75 105.957106) (xy 223.853553 103.853553) (xy 223.96194 103.691342)
        (xy 224 103.5) (xy 224 102.457106) (xy 224.207106 102.25) (xy 224.792894 102.25)
      )
    )
  )
  (zone (net 92) (net_name /hv/driver/CVH) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 226 102.25) (xy 226.5 101.75) (xy 227.5 101.75) (xy 228 102.25) (xy 228 104.5)
        (xy 228.75 105.25) (xy 228.75 107) (xy 225.25 107) (xy 225.25 105.25) (xy 226 104.5)
      )
    )
    (filled_polygon
      (pts
        (xy 227.5 102.457106) (xy 227.5 104.5) (xy 227.53806 104.691342) (xy 227.646447 104.853553) (xy 228.25 105.457106)
        (xy 228.25 106.5) (xy 225.75 106.5) (xy 225.75 105.457106) (xy 226.353553 104.853553) (xy 226.46194 104.691342)
        (xy 226.5 104.5) (xy 226.5 102.457106) (xy 226.707106 102.25) (xy 227.292894 102.25)
      )
    )
  )
  (zone (net 93) (net_name /hv/driver/CWH) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 228.5 102.25) (xy 229 101.75) (xy 230 101.75) (xy 230.5 102.25) (xy 230.5 103.75)
        (xy 232.75 106) (xy 232.75 107) (xy 229.25 107) (xy 229.25 105) (xy 228.5 104.25)
      )
    )
    (filled_polygon
      (pts
        (xy 230 102.457106) (xy 230 103.75) (xy 230.03806 103.941342) (xy 230.146447 104.103553) (xy 232.25 106.207106)
        (xy 232.25 106.5) (xy 229.75 106.5) (xy 229.75 105) (xy 229.71194 104.808658) (xy 229.603553 104.646447)
        (xy 229 104.042894) (xy 229 102.457106) (xy 229.207106 102.25) (xy 229.792894 102.25)
      )
    )
  )
)
