(module C_1808 (layer F.Cu) (tedit 5775A534)
  (descr "Capacitor SMD 1808, reflow soldering, AVX (see smccp.pdf)")
  (tags "capacitor 1808")
  (attr smd)
  (fp_text reference REF** (at 0 -2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value C_1808 (at 0 2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.1 -1.25) (end 3.1 -1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.1 1.25) (end 3.1 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.1 -1.25) (end -3.1 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.1 -1.25) (end 3.1 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.8 -1.2) (end -1.8 -1.2) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.8 1.2) (end 1.8 1.2) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -2.3 0) (size 1 2) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 2.3 0) (size 1 2) (layers F.Cu F.Paste F.Mask))
  (model Capacitors_SMD.3dshapes/C_1812.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
