(module TO_SOT_Packages_SMD:TO-263-2 (layer F.Cu) (tedit 5A0240F7)
  (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
  (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
  (attr smd)
  (fp_text reference Q6 (at 0 -6.65) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Q_NMOS_GDS (at 0 6.65) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 8.32 -5.65) (end -8.32 -5.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start 8.32 5.65) (end 8.32 -5.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8.32 5.65) (end 8.32 5.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8.32 -5.65) (end -8.32 5.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.95 3.39) (end -4.05 3.39) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.95 5.2) (end -2.95 3.39) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.45 5.2) (end -2.95 5.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.95 -3.39) (end -8.075 -3.39) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.95 -5.2) (end -2.95 -3.39) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.45 -5.2) (end -2.95 -5.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.45 3.04) (end -2.75 3.04) (layer F.Fab) (width 0.1))
  (fp_line (start -7.45 2.04) (end -7.45 3.04) (layer F.Fab) (width 0.1))
  (fp_line (start -2.75 2.04) (end -7.45 2.04) (layer F.Fab) (width 0.1))
  (fp_line (start -7.45 -2.04) (end -2.75 -2.04) (layer F.Fab) (width 0.1))
  (fp_line (start -7.45 -3.04) (end -7.45 -2.04) (layer F.Fab) (width 0.1))
  (fp_line (start -2.75 -3.04) (end -7.45 -3.04) (layer F.Fab) (width 0.1))
  (fp_line (start -1.75 -5) (end 6.5 -5) (layer F.Fab) (width 0.1))
  (fp_line (start -2.75 -4) (end -1.75 -5) (layer F.Fab) (width 0.1))
  (fp_line (start -2.75 5) (end -2.75 -4) (layer F.Fab) (width 0.1))
  (fp_line (start 6.5 5) (end -2.75 5) (layer F.Fab) (width 0.1))
  (fp_line (start 6.5 -5) (end 6.5 5) (layer F.Fab) (width 0.1))
  (fp_line (start 7.5 5) (end 6.5 5) (layer F.Fab) (width 0.1))
  (fp_line (start 7.5 -5) (end 7.5 5) (layer F.Fab) (width 0.1))
  (fp_line (start 6.5 -5) (end 7.5 -5) (layer F.Fab) (width 0.1))
  (pad 2 smd rect (at 3.375 0) (size 9.4 10.8) (layers F.Cu F.Mask))
  (pad 3 smd rect (at -5.775 2.54) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -5.775 -2.54) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-263-2.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
