load adc
load reslimit
load rev
load fb_switch
load vel
load vel
load vel
load pid
load fault
load hv
load sim
load io
load iit
link conf
hv0.rt_prio = 0.9
adc0.rt_prio = 1
reslimit0.rt_prio = 3
rev0.rt_prio = 4
fb_switch0.rt_prio = 5
vel0.rt_prio = 6
vel1.rt_prio = 6
vel2.rt_prio = 6
io0.rt_prio = 7
io0.frt_prio = 3
pid0.rt_prio = 8
fault0.rt_prio = 10
iit0.rt_prio = 13
sim0.rt_prio = 13
term0.rt_prio = 16
rev0.rev = conf0.cmd_rev
fb_switch0.mot_rev = conf0.mot_fb_rev
fb_switch0.com_rev = conf0.com_fb_rev
fb_switch0.joint_rev = conf0.joint_fb_rev
reslimit0.res = conf0.mot_fb_res
vel1.j = conf0.j
vel2.j = conf0.j
pid0.j_mot = conf0.j
pid0.j_load = conf0.j_load
pid0.j_lpf = conf0.j_lpf
pid0.pos_p = conf0.pos_p
pid0.vel_p = conf0.vel_p
pid0.vel_i = conf0.vel_i
pid0.vel_g = conf0.vel_g
pid0.acc_g = conf0.acc_g
pid0.g = conf0.g
pid0.max_usr_vel = conf0.max_vel
pid0.max_usr_acc = conf0.max_acc
pid0.max_usr_torque = conf0.max_force
fault0.max_sat = conf0.max_sat
fault0.max_pos_error = conf0.max_pos_error
fault0.max_vel_error = conf0.max_vel_error
fault0.max_dc_cur = conf0.max_dc_cur
fault0.max_ac_cur = conf0.max_ac_cur
fault0.max_dc_volt = conf0.max_dc_volt
fault0.high_dc_volt = conf0.high_dc_volt
fault0.min_dc_volt = conf0.min_dc_volt
fault0.max_hv_temp = conf0.max_hv_temp
fault0.max_mot_temp = conf0.max_mot_temp
fault0.high_hv_temp = conf0.high_hv_temp
fault0.high_mot_temp = conf0.high_mot_temp
fault0.fan_hv_temp = conf0.fan_hv_temp
fault0.fan_mot_temp = conf0.fan_mot_temp
fault0.ac_cur = hv0.abs_cur
hv0.rev = conf0.out_rev
hv0.r = conf0.r
hv0.l = conf0.l
hv0.psi = conf0.psi
hv0.cur_p = conf0.cur_p
hv0.cur_i = conf0.cur_i
hv0.cur_ff = conf0.cur_ff
hv0.cur_ind = conf0.cur_ind
hv0.max_cur = conf0.max_ac_cur
reslimit0.pos_in = rev0.out
fb_switch0.cmd_pos = reslimit0.pos_out
fb_switch0.polecount = conf0.polecount
fb_switch0.en = fault0.en_fb
fb_switch0.mot_polecount = conf0.mot_fb_polecount
fb_switch0.joint_polecount = conf0.joint_fb_polecount
fb_switch0.com_polecount = conf0.com_fb_polecount
fb_switch0.mot_offset = conf0.mot_fb_offset
fb_switch0.joint_offset = conf0.joint_fb_offset
fb_switch0.com_offset = conf0.com_fb_offset
fb_switch0.phase_time = conf0.phase_time
fb_switch0.phase_cur = conf0.phase_cur
vel0.pos_in = rev0.out
vel0.en = fault0.en_fb
vel1.pos_in = fb_switch0.vel_fb
vel1.en = fault0.en_fb
vel1.torque = pid0.torque_cmd
vel2.pos_in = fb_switch0.com_fb
vel2.en = fault0.en_fb
vel2.torque = pid0.torque_cmd
pid0.enable = fault0.en_pid
pid0.pos_ext_cmd = reslimit0.pos_out
pid0.vel_ext_cmd = vel0.vel
pid0.pos_fb = fb_switch0.pos_fb
pid0.vel_fb = vel1.vel
rev0.in_d = vel0.vel
fault0.pos_error = pid0.pos_error
fault0.vel_error = pid0.vel_error
fault0.sat = pid0.saturated
fault0.dc_volt = hv0.dc_volt
fault0.hv_temp = hv0.hv_temp
fault0.dc_cur = hv0.dc_cur
fault0.hv_error = hv0.fault
fault0.fb_ready = fb_switch0.state
hv0.en = fault0.en_out
hv0.pos = vel2.pos_out
hv0.vel = vel2.vel
hv0.scale = fault0.scale
io0.fan = fault0.hv_fan
io0.fault = fault0.fault
io0.state = fault0.state
pe0.udc = hv0.dc_volt
pe0.idc = 0
pe0.ud = 0
pe0.uq = 0
pe0.id = hv0.id_fb
pe0.iq = hv0.iq_fb
pe0.torque = pid0.torque_cor_cmd
pe0.vel = vel1.vel
pe0.r = conf0.r
pe0.j = conf0.j
pe0.cap = 0.00054
iit0.max_temp = conf0.max_mot_temp
iit0.high_temp = conf0.high_mot_temp
iit0.max_cur = conf0.max_ac_cur
fault0.mot_temp = iit0.temp
iit0.cur = hv0.abs_cur
