load uvw
uvw0.rt_prio = 3
uvw0.u = io0.fb0a
uvw0.v = io0.fb0b
uvw0.w = io0.fb0z

uvw0.amp = adc0.amp0

fb_switch0.com_pos = uvw0.pos
fb_switch0.com_abs_pos = uvw0.pos
fb_switch0.com_state = uvw0.state
fb_switch0.com_polecount = conf0.com_fb_polecount
conf0.com_fb_polecount = conf0.polecount
fault0.com_fb_error = uvw0.error