(module RJ45 (layer F.Cu) (tedit 596502CB)
  (descr "mod. jack, ethernet, 8P8C, RJ45 connector, 2 leds, shielded")
  (tags "RJHSE538X 8P8C RJ45 ethernet jack")
  (fp_text reference REF** (at 3.49 -6.92) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value RJ45 (at 3.94 9.21) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 11.87 7.62) (end -4.76 7.62) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.76 -8.19) (end -4.76 -0.32) (layer F.SilkS) (width 0.12))
  (fp_line (start 11.87 -8.19) (end 11.87 -0.32) (layer F.SilkS) (width 0.12))
  (fp_line (start 11.87 -8.19) (end -4.76 -8.19) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.76 7.62) (end -4.76 2.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 11.87 7.62) (end 11.87 2.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.9 -8.45) (end -5.8 -8.45) (layer F.CrtYd) (width 0.05))
  (fp_line (start 12.9 7.9) (end 12.9 -8.45) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.8 7.9) (end 12.9 7.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.8 -8.45) (end -5.8 7.9) (layer F.CrtYd) (width 0.05))
  (pad 9 thru_hole circle (at -4.57 0.89) (size 2 2) (drill 1.57) (layers *.Cu *.Mask))
  (pad "" thru_hole circle (at 9.91 -2.54) (size 3.3 3.3) (drill 3.3) (layers *.Cu *.Mask))
  (pad "" thru_hole circle (at -2.79 -2.54) (size 3.3 3.3) (drill 3.3) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 6.1 0) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 2.03 0) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 4.06 0) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 1.02 1.78) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 3.05 1.78) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 5.08 1.78) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 7.11 1.78) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 11.68 0.89) (size 2 2) (drill 1.57) (layers *.Cu *.Mask))
  (model Connectors.3dshapes/RJHSE538X.wrl
    (at (xyz 0.14 0.06 0.12))
    (scale (xyz 0.4 0.4 0.4))
    (rotate (xyz -90 0 180))
  )
)
