(module C_1808 (layer F.Cu) (tedit 5AC5647C)
  (descr "Capacitor SMD 1808, reflow soldering, AVX (see smccp.pdf)")
  (tags "capacitor 1808")
  (attr smd)
  (fp_text reference C38 (at -4.936 0.05) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.2)))
  )
  (fp_text value 150n (at 0 2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.5 -1) (end 1.5 1) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.5 -1) (end -1.5 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.3 -1) (end -2.3 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.3 1) (end 2.3 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.3 1) (end 2.3 1) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.3 -1) (end -2.3 1) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.1 -1.2) (end 3.1 -1.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.1 1.2) (end 3.1 1.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.1 -1.2) (end -3.1 1.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.1 -1.2) (end 3.1 1.2) (layer F.CrtYd) (width 0.05))
  (pad 2 smd roundrect (at 2 0) (size 1.5 2) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25)
    (solder_mask_margin 0.1) (zone_connect 2))
  (pad 1 smd roundrect (at -2 0) (size 1.5 2) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25)
    (solder_mask_margin 0.1) (zone_connect 2))
  (model ${KIPRJMOD}/../lib/stmbl.pretty/cap_1808.wrl
    (at (xyz 0 0 0))
    (scale (xyz 393.7 393.7 393.7))
    (rotate (xyz 0 0 0))
  )
)
