(module stmbl:SOLDER_JUMPER_3_NC (layer F.Cu) (tedit 5B28FC99)
  (attr virtual)
  (fp_text reference JP5 (at -0.114 1.29) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.2)))
  )
  (fp_text value JUMPER3_NC (at 0 -2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0 0) (end 1.5 0) (layer F.Mask) (width 0.45))
  (fp_line (start -1.5 0) (end 0 0) (layer F.Cu) (width 0.25))
  (fp_line (start -1.5 0) (end 0 0) (layer F.Mask) (width 0.45))
  (fp_line (start 0 0) (end 0.55 0) (layer F.Cu) (width 0.25))
  (fp_line (start 1.5 0) (end 0.95 0) (layer F.Cu) (width 0.25))
  (pad 1 smd roundrect (at -1.5 0) (size 1 1.5) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at 0 0) (size 1 1.5) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at 1.5 0) (size 1 1.5) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
)
