(module R_2512_BIG (layer F.Cu) (tedit 580D3ED4)
  (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
  (tags "resistor 2512")
  (attr smd)
  (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value R_2512_BIG (at 0 2.6) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.25 1.8) (end 1.25 -1.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.25 -1.8) (end -1.25 1.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.25 -1.8) (end -3.25 -1.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.25 1.8) (end 3.25 -1.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.25 1.8) (end 3.25 1.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.25 -1.8) (end -3.25 1.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.8 -1.8) (end 3.8 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.8 1.8) (end 3.8 1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.8 -1.8) (end -3.8 1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.8 -1.8) (end 3.8 1.8) (layer F.CrtYd) (width 0.05))
  (pad 1 smd rect (at -2.5 0) (size 2.7 3.5) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1))
  (pad 2 smd rect (at 2.5 0) (size 2.7 3.5) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1))
  (model Resistors_SMD.3dshapes/R_2512.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
