(module CONN_1x04_2.54 (layer F.Cu) (tedit 593CA5FE)
  (descr "Through hole pin header")
  (tags "pin header")
  (fp_text reference P3 (at 0 -5.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value CONN_01X04 (at 0 5.75) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.5 -5.25) (end 1.5 -5.25) (layer F.CrtYd) (width 0.15))
  (fp_line (start 1.5 -5.25) (end 1.5 5.25) (layer F.CrtYd) (width 0.15))
  (fp_line (start 1.5 5.25) (end -1.5 5.25) (layer F.CrtYd) (width 0.15))
  (fp_line (start -1.5 5.25) (end -1.5 -5.25) (layer F.CrtYd) (width 0.15))
  (fp_line (start -1.5 -5.25) (end 1.5 -5.25) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.5 -5.25) (end 1.5 -2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.5 -2.5) (end -1.5 -2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.5 -2.5) (end -1.5 -5.25) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole roundrect (at 0 -3.81) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS)(roundrect_rratio 0.25))
  (pad 2 thru_hole roundrect (at 0 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS)(roundrect_rratio 0.25))
  (pad 3 thru_hole roundrect (at 0 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS)(roundrect_rratio 0.25))
  (pad 4 thru_hole roundrect (at 0 3.81) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS)(roundrect_rratio 0.25))
  (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
    (at (xyz 0 -0.15 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
