(module stmbl:akl182-6 (layer F.Cu) (tedit 5B2A1F15)
  (fp_text reference P5 (at 5.572 -6.608) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (fp_text value CONN_01X06 (at 6 9.8) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.55 8) (end 20.05 8) (layer F.SilkS) (width 0.15))
  (fp_line (start 20.05 -1.2) (end 20.05 8) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.55 -1.2) (end 20.05 -1.2) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.55 8) (end -2.55 -1.2) (layer F.SilkS) (width 0.15))
  (pad 6 smd roundrect (at 17.5 0) (size 2.5 2.5) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at 14 0) (size 2.5 2.5) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at 10.5 0) (size 2.5 2.5) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 1 smd roundrect (at 0 0) (size 2.5 2.5) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at 3.5 0) (size 2.5 2.5) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at 7 0) (size 2.5 2.5) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.2) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 3.5 0) (size 1.5 1.5) (drill 1.2) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 7 0) (size 1.5 1.5) (drill 1.2) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 10.5 0) (size 1.5 1.5) (drill 1.2) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 14 0) (size 1.5 1.5) (drill 1.2) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 17.5 0) (size 1.5 1.5) (drill 1.2) (layers *.Cu *.Mask))
  (model ${KIPRJMOD}/../lib/../lib/stmbl.pretty/akl182_6.wrl
    (offset (xyz 20.04999969887921 3.199999951940823 0))
    (scale (xyz 0.394 0.394 0.394))
    (rotate (xyz 0 0 180))
  )
)
