(module Crystal_SMD_0503_4Pads (layer F.Cu) (tedit 5AC566BD)
  (descr "Crystal, Quarz, SMD, 0603, 4 Pads,")
  (tags "Crystal, Quarz, SMD, 0603, 4 Pads,")
  (attr smd)
  (fp_text reference Y2 (at 0.146 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.2)))
  )
  (fp_text value 8M (at 0 4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2 -3) (end -2 -1.25) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.75 -3) (end -2 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.5 2.5) (end -1.5 -2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.5 2.5) (end -1.5 2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.5 -2.5) (end 1.5 2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.5 -2.5) (end 1.5 -2.5) (layer F.SilkS) (width 0.15))
  (pad 3 smd roundrect (at 1.25 -2 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 2 smd roundrect (at 1.25 2 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -1.25 2 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 1 smd roundrect (at -1.25 -2 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (model ${KIPRJMOD}/../lib/stmbl.pretty/GeyerElectronics_KX9A.wrl
    (at (xyz 0 0 0))
    (scale (xyz 393.7 393.7 393.7))
    (rotate (xyz -90 0 90))
  )
)
