(module Pin_Header_Straight_2x05_dual (layer F.Cu) (tedit 5944A8EB)
  (descr "Through hole pin header")
  (tags "pin header")
  (fp_text reference J1 (at 0 -5.1) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value CONN_02X05 (at 0 -3.1) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.54 -6.35) (end 2.54 -6.35) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.54 -6.35) (end 2.54 6.35) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.54 6.35) (end -2.54 6.35) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.54 6.35) (end -2.54 -6.35) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 -6.35) (end 0 -3.81) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 -3.81) (end -2.54 -3.81) (layer F.SilkS) (width 0.15))
  (pad 1 smd roundrect (at -1.27 -5.08) (size 1.75 1.75) (layers F.Cu F.Mask)(roundrect_rratio 0.1))
  (pad 2 smd roundrect (at 1.27 -5.08) (size 1.75 1.75) (layers F.Cu F.Mask)(roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -1.27 -2.54) (size 1.75 1.75) (layers F.Cu F.Mask)(roundrect_rratio 0.25))
  (pad 4 smd roundrect (at 1.27 -2.54) (size 1.75 1.75) (layers F.Cu F.Mask)(roundrect_rratio 0.25))
  (pad 5 smd roundrect (at -1.27 0) (size 1.75 1.75) (layers F.Cu F.Mask)(roundrect_rratio 0.25))
  (pad 6 smd roundrect (at 1.27 0) (size 1.75 1.75) (layers F.Cu F.Mask)(roundrect_rratio 0.25))
  (pad 7 smd roundrect (at -1.27 2.54) (size 1.75 1.75) (layers F.Cu F.Mask)(roundrect_rratio 0.25))
  (pad 8 smd roundrect (at 1.27 2.54) (size 1.75 1.75) (layers F.Cu F.Mask)(roundrect_rratio 0.25))
  (pad 9 smd roundrect (at -1.27 5.08) (size 1.75 1.75) (layers F.Cu F.Mask)(roundrect_rratio 0.25))
  (pad 10 smd roundrect (at 1.27 5.08) (size 1.75 1.75) (layers F.Cu F.Mask)(roundrect_rratio 0.25))
  (pad 1 thru_hole circle (at -1.27 -5.08) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (pad 4 smd roundrect (at 1.27 -2.54) (size 1.75 1.75) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 8 smd roundrect (at 1.27 2.54) (size 1.75 1.75) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 2 smd roundrect (at 1.27 -5.08) (size 1.75 1.75) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 6 smd roundrect (at 1.27 0) (size 1.75 1.75) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 10 smd roundrect (at 1.27 5.08) (size 1.75 1.75) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -1.27 -2.54) (size 1.75 1.75) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 7 smd roundrect (at -1.27 2.54) (size 1.75 1.75) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 5 smd roundrect (at -1.27 0) (size 1.75 1.75) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 9 smd roundrect (at -1.27 5.08) (size 1.75 1.75) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 1 smd roundrect (at -1.27 -5.08) (size 1.75 1.75) (layers B.Cu B.Mask)(roundrect_rratio 0.1))
  (pad 2 thru_hole circle (at 1.27 -5.08) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -1.27 -2.54) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 1.27 -2.54) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at -1.27 0) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 1.27 0) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at -1.27 2.54) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 1.27 2.54) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at -1.27 5.08) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 1.27 5.08) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (model Pin_Headers.3dshapes/Pin_Header_Straight_2x05.wrl
    (at (xyz 0.05 -0.2 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
