(module R_1206 (layer F.Cu) (tedit 5AC5649A)
  (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
  (tags "resistor 1206")
  (attr smd)
  (fp_text reference R27 (at 0 -1.7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.2)))
  )
  (fp_text value 249k (at 0 1.8) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.1 -0.8) (end 1.1 0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.1 -0.8) (end -1.1 0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.6 -0.8) (end -1.6 -0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.6 0.8) (end 1.6 -0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.6 0.8) (end 1.6 0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.6 -0.8) (end -1.6 0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.3 -1) (end 2.3 -1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.3 1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.3 -1) (end -2.3 1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.3 -1) (end 2.3 1) (layer F.CrtYd) (width 0.05))
  (pad 2 smd roundrect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 1 smd roundrect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (model Resistors_SMD.3dshapes/R_1206.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
