(export (version D)
  (design
    (source /Users/rene/dev/stmbl/hw/kicad/11ua/11ua.sch)
    (date "2017 May 31, Wednesday 02:02:43")
    (tool "Eeschema (2017-04-22 revision b385413)-master")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source 11ua.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value RJ45)
      (footprint Connect:RJ45_8)
      (libsource (lib conn) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E009D))
    (comp (ref J2)
      (value RJ45)
      (footprint Connect:RJ45_8)
      (libsource (lib conn) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E00E5))
    (comp (ref U1)
      (value LM393)
      (footprint stmbl:SOIC-8-N)
      (libsource (lib linear) (part LM393))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E0206))
    (comp (ref R4)
      (value 100k)
      (footprint stmbl:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E0847))
    (comp (ref R3)
      (value 100k)
      (footprint stmbl:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E08D0))
    (comp (ref C4)
      (value 27p)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E0942))
    (comp (ref C3)
      (value 27p)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E0986))
    (comp (ref R1)
      (value 100k)
      (footprint stmbl:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E0C0B))
    (comp (ref C1)
      (value 27p)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E0C46))
    (comp (ref R2)
      (value 100k)
      (footprint stmbl:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E0DC4))
    (comp (ref C2)
      (value 27p)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E0E05))
    (comp (ref R5)
      (value 120)
      (footprint stmbl:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E1018))
    (comp (ref R6)
      (value 120)
      (footprint stmbl:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E1061))
    (comp (ref C5)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E10E2))
    (comp (ref R7)
      (value 120)
      (footprint stmbl:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E1BC6))
    (comp (ref R8)
      (value 120)
      (footprint stmbl:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E1BCC))
    (comp (ref C6)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E1BDE)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib linear) (part LM2903)
      (aliases
        (alias LM293)
        (alias LM393)
        (alias LM193))
      (description "Dual Voltage Comparator")
      (docs ns/lm193.pdf)
      (footprints
        (fp SOIC*Pitch1.27mm*)
        (fp DIP*W7.62mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM2903))
      (pins
        (pin (num 1) (name ~) (type openCol))
        (pin (num 2) (name _) (type input))
        (pin (num 3) (name +) (type input))
        (pin (num 4) (name V-) (type power_in))
        (pin (num 5) (name +) (type input))
        (pin (num 6) (name _) (type input))
        (pin (num 7) (name ~) (type openCol))
        (pin (num 8) (name V+) (type power_in))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part RJ45)
      (description "RJ45 connector with shield")
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name SHIELD) (type passive)))))
  (libraries
    (library (logical device)
      (uri "/Library/Application Support/kicad/library/device.lib"))
    (library (logical conn)
      (uri "/Library/Application Support/kicad/library/conn.lib"))
    (library (logical linear)
      (uri "/Library/Application Support/kicad/library/linear.lib")))
  (nets
    (net (code 1) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4)))
    (net (code 2) (name "Net-(J1-Pad5)")
      (node (ref J1) (pin 5)))
    (net (code 3) (name "Net-(J2-Pad4)")
      (node (ref J2) (pin 4)))
    (net (code 4) (name "Net-(J2-Pad5)")
      (node (ref J2) (pin 5)))
    (net (code 5) (name "Net-(C2-Pad1)")
      (node (ref C6) (pin 2))
      (node (ref C2) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref J2) (pin 6))
      (node (ref R8) (pin 2))
      (node (ref R7) (pin 1)))
    (net (code 6) (name GND)
      (node (ref U1) (pin 4))
      (node (ref J2) (pin 8))
      (node (ref C5) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref J1) (pin 8))
      (node (ref R8) (pin 1)))
    (net (code 7) (name +5V)
      (node (ref J2) (pin 7))
      (node (ref J1) (pin 7))
      (node (ref R5) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref U1) (pin 8)))
    (net (code 8) (name "Net-(C3-Pad1)")
      (node (ref C3) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref J2) (pin 3))
      (node (ref U1) (pin 7)))
    (net (code 9) (name "Net-(C3-Pad2)")
      (node (ref C3) (pin 2))
      (node (ref J1) (pin 3))
      (node (ref R4) (pin 2))
      (node (ref U1) (pin 6)))
    (net (code 10) (name "Net-(C4-Pad1)")
      (node (ref U1) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref C4) (pin 1)))
    (net (code 11) (name "Net-(C4-Pad2)")
      (node (ref J1) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref C4) (pin 2)))
    (net (code 12) (name "Net-(C1-Pad2)")
      (node (ref J1) (pin 2))
      (node (ref U1) (pin 3))
      (node (ref R1) (pin 2))
      (node (ref C1) (pin 2)))
    (net (code 13) (name "Net-(C2-Pad2)")
      (node (ref J1) (pin 6))
      (node (ref U1) (pin 5))
      (node (ref C2) (pin 2))
      (node (ref R2) (pin 2)))
    (net (code 14) (name "Net-(C1-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref R6) (pin 2))
      (node (ref R1) (pin 1))
      (node (ref C5) (pin 2))
      (node (ref J2) (pin 2)))
    (net (code 15) (name GNDA)
      (node (ref J2) (pin 9))
      (node (ref J1) (pin 9)))))