(export (version D)
  (design
    (source trollerv2.sch)
    (date "Mi 08 Nov 2017 00:27:26 CET")
    (tool "Eeschema (2017-10-23 revision 788972554)-makepkg")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source trollerv2.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref Q1)
      (value Q_NMOS_GDS)
      (footprint TO_SOT_Packages_SMD:TO-263-2)
      (libsource (lib device) (part Q_NMOS_GDS))
      (sheetpath (names /) (tstamps /))
      (tstamp 59317448))
    (comp (ref Q2)
      (value Q_NMOS_GDS)
      (footprint TO_SOT_Packages_SMD:TO-263-2)
      (libsource (lib device) (part Q_NMOS_GDS))
      (sheetpath (names /) (tstamps /))
      (tstamp 59317498))
    (comp (ref C4)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59529438))
    (comp (ref C5)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59529498))
    (comp (ref C6)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 595294C2))
    (comp (ref C7)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 595294F4))
    (comp (ref C8)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952959E))
    (comp (ref C9)
      (value CP)
      (footprint stmbl:C_Radial_D26_L45_P10)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952961F))
    (comp (ref C10)
      (value CP)
      (footprint stmbl:C_Radial_D26_L45_P10)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952964F))
    (comp (ref R3)
      (value R)
      (footprint Resistors_SMD:R_2010)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59529A6D))
    (comp (ref U1)
      (value IRS2186)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib ir) (part IRS2186))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952A770))
    (comp (ref R2)
      (value R)
      (footprint Resistors_SMD:R_1206)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952AD53))
    (comp (ref R1)
      (value R)
      (footprint Resistors_SMD:R_1206)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952ADEF))
    (comp (ref D1)
      (value D)
      (footprint Diodes_SMD:D_SMA)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952AEC1))
    (comp (ref C1)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952B09B))
    (comp (ref Q3)
      (value Q_NMOS_GDS)
      (footprint TO_SOT_Packages_SMD:TO-263-2)
      (libsource (lib device) (part Q_NMOS_GDS))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952B45C))
    (comp (ref Q4)
      (value Q_NMOS_GDS)
      (footprint TO_SOT_Packages_SMD:TO-263-2)
      (libsource (lib device) (part Q_NMOS_GDS))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952B462))
    (comp (ref R6)
      (value R)
      (footprint Resistors_SMD:R_2010)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952B47A))
    (comp (ref U2)
      (value IRS2186)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib ir) (part IRS2186))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952B481))
    (comp (ref R5)
      (value R)
      (footprint Resistors_SMD:R_1206)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952B48E))
    (comp (ref R4)
      (value R)
      (footprint Resistors_SMD:R_1206)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952B497))
    (comp (ref D2)
      (value D)
      (footprint Diodes_SMD:D_SMA)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952B4A2))
    (comp (ref C2)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952B4AB))
    (comp (ref Q5)
      (value Q_NMOS_GDS)
      (footprint TO_SOT_Packages_SMD:TO-263-2)
      (libsource (lib device) (part Q_NMOS_GDS))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952B9EF))
    (comp (ref Q6)
      (value Q_NMOS_GDS)
      (footprint TO_SOT_Packages_SMD:TO-263-2)
      (libsource (lib device) (part Q_NMOS_GDS))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952B9F5))
    (comp (ref R9)
      (value R)
      (footprint Resistors_SMD:R_2010)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952BA0D))
    (comp (ref U3)
      (value IRS2186)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib ir) (part IRS2186))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952BA14))
    (comp (ref R8)
      (value R)
      (footprint Resistors_SMD:R_1206)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952BA21))
    (comp (ref R7)
      (value R)
      (footprint Resistors_SMD:R_1206)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952BA2A))
    (comp (ref D3)
      (value D)
      (footprint Diodes_SMD:D_SMA)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952BA35))
    (comp (ref C3)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952BA3E))
    (comp (ref J1)
      (value CONN_01X03)
      (footprint stmbl:RM5.08_1x3)
      (libsource (lib trollerv2-cache) (part CONN_01X03))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952BA81))
    (comp (ref J2)
      (value Conn_01x02)
      (footprint stmbl:RM5.08_1x2)
      (libsource (lib conn) (part Conn_01x02))
      (sheetpath (names /) (tstamps /))
      (tstamp 59FB34B0)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib trollerv2-cache) (part CONN_01X03)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X03))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib device) (part CP)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part Conn_01x02)
      (description "Generic connector, single row, 01x02")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib device) (part D)
      (description Diode)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib ir) (part IRS2186)
      (description "High and Low Side Gate Driver,  600V operation, 4A output current")
      (docs http://www.irf.com/product-info/datasheets/data/irs2186pbf.pdf)
      (footprints
        (fp SOIC*3.9x4.9mm*Pitch1.27mm*)
        (fp DIP*W7.62mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) IRS2186))
      (pins
        (pin (num 1) (name HIN) (type input))
        (pin (num 2) (name LIN) (type input))
        (pin (num 3) (name COM) (type power_in))
        (pin (num 4) (name LO) (type output))
        (pin (num 5) (name VCC) (type power_in))
        (pin (num 6) (name VS) (type passive))
        (pin (num 7) (name HO) (type output))
        (pin (num 8) (name VB) (type passive))))
    (libpart (lib device) (part Q_NMOS_GDS)
      (description "Transistor N-MOSFET with substrate diode (general)")
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NMOS_GDS))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name D) (type passive))
        (pin (num 3) (name S) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical ir)
      (uri /usr/share/kicad/library/ir.lib))
    (library (logical trollerv2-cache)
      (uri trollerv2-cache.lib)))
  (nets
    (net (code 1) (name "Net-(Q6-Pad3)")
      (node (ref R9) (pin 1))
      (node (ref Q6) (pin 3)))
    (net (code 2) (name "Net-(D2-Pad2)")
      (node (ref D2) (pin 2))
      (node (ref U2) (pin 5)))
    (net (code 3) (name "Net-(C2-Pad2)")
      (node (ref C2) (pin 2)))
    (net (code 4) (name "Net-(C2-Pad1)")
      (node (ref D2) (pin 1))
      (node (ref U2) (pin 8))
      (node (ref C2) (pin 1)))
    (net (code 5) (name HT)
      (node (ref J2) (pin 2))
      (node (ref C4) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref Q3) (pin 2))
      (node (ref Q1) (pin 2))
      (node (ref C9) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref Q5) (pin 2)))
    (net (code 6) (name GND)
      (node (ref R3) (pin 2))
      (node (ref U2) (pin 3))
      (node (ref C5) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref U3) (pin 3))
      (node (ref J2) (pin 1))
      (node (ref R9) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref U1) (pin 3))
      (node (ref C7) (pin 2))
      (node (ref C6) (pin 2)))
    (net (code 7) (name "Net-(Q4-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref Q4) (pin 1)))
    (net (code 8) (name "Net-(U2-Pad1)")
      (node (ref U2) (pin 1)))
    (net (code 9) (name "Net-(U2-Pad2)")
      (node (ref U2) (pin 2)))
    (net (code 10) (name "Net-(R5-Pad2)")
      (node (ref U2) (pin 4))
      (node (ref R5) (pin 2)))
    (net (code 11) (name "Net-(Q3-Pad1)")
      (node (ref Q3) (pin 1))
      (node (ref R4) (pin 1)))
    (net (code 12) (name "Net-(R4-Pad2)")
      (node (ref U2) (pin 7))
      (node (ref R4) (pin 2)))
    (net (code 13) (name "Net-(D3-Pad2)")
      (node (ref U3) (pin 5))
      (node (ref D3) (pin 2)))
    (net (code 14) (name "Net-(C3-Pad2)")
      (node (ref C3) (pin 2)))
    (net (code 15) (name U1)
      (node (ref U1) (pin 6))
      (node (ref Q1) (pin 3))
      (node (ref Q2) (pin 2))
      (node (ref J1) (pin 1)))
    (net (code 16) (name V1)
      (node (ref J1) (pin 2))
      (node (ref Q3) (pin 3))
      (node (ref Q4) (pin 2))
      (node (ref U2) (pin 6)))
    (net (code 17) (name "Net-(U3-Pad1)")
      (node (ref U3) (pin 1)))
    (net (code 18) (name "Net-(U3-Pad2)")
      (node (ref U3) (pin 2)))
    (net (code 19) (name "Net-(R8-Pad2)")
      (node (ref U3) (pin 4))
      (node (ref R8) (pin 2)))
    (net (code 20) (name W1)
      (node (ref Q5) (pin 3))
      (node (ref Q6) (pin 2))
      (node (ref J1) (pin 3))
      (node (ref U3) (pin 6)))
    (net (code 21) (name "Net-(Q6-Pad1)")
      (node (ref Q6) (pin 1))
      (node (ref R8) (pin 1)))
    (net (code 22) (name "Net-(Q5-Pad1)")
      (node (ref Q5) (pin 1))
      (node (ref R7) (pin 1)))
    (net (code 23) (name "Net-(R7-Pad2)")
      (node (ref U3) (pin 7))
      (node (ref R7) (pin 2)))
    (net (code 24) (name "Net-(C3-Pad1)")
      (node (ref C3) (pin 1))
      (node (ref U3) (pin 8))
      (node (ref D3) (pin 1)))
    (net (code 25) (name "Net-(Q2-Pad3)")
      (node (ref R3) (pin 1))
      (node (ref Q2) (pin 3)))
    (net (code 26) (name "Net-(Q4-Pad3)")
      (node (ref Q4) (pin 3))
      (node (ref R6) (pin 1)))
    (net (code 27) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref U1) (pin 5)))
    (net (code 28) (name "Net-(C1-Pad2)")
      (node (ref C1) (pin 2)))
    (net (code 29) (name "Net-(C1-Pad1)")
      (node (ref D1) (pin 1))
      (node (ref U1) (pin 8))
      (node (ref C1) (pin 1)))
    (net (code 30) (name "Net-(Q2-Pad1)")
      (node (ref Q2) (pin 1))
      (node (ref R2) (pin 1)))
    (net (code 31) (name "Net-(U1-Pad1)")
      (node (ref U1) (pin 1)))
    (net (code 32) (name "Net-(U1-Pad2)")
      (node (ref U1) (pin 2)))
    (net (code 33) (name "Net-(R2-Pad2)")
      (node (ref R2) (pin 2))
      (node (ref U1) (pin 4)))
    (net (code 34) (name "Net-(Q1-Pad1)")
      (node (ref Q1) (pin 1))
      (node (ref R1) (pin 1)))
    (net (code 35) (name "Net-(R1-Pad2)")
      (node (ref R1) (pin 2))
      (node (ref U1) (pin 7)))))
