(export (version D)
  (design
    (source rj45_breakout.sch)
    (date "Mi 16 Mär 2016 15:00:40 CET")
    (tool "Eeschema (2016-02-29 BZR 6601, Git bd80063)-product")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source rj45_breakout.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value RJ45)
      (footprint rj45_vertical_mhrjj88nfvs:RJ45_8)
      (libsource (lib conn) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E95EDF))
    (comp (ref P1)
      (value CONN_4)
      (footprint Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_4pol)
      (libsource (lib conn) (part CONN_4))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E95F7A))
    (comp (ref P2)
      (value CONN_5)
      (footprint Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_5pol)
      (libsource (lib conn) (part CONN_5))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E95FCC)))
  (libparts
    (libpart (lib conn) (part CONN_4)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_4))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib conn) (part CONN_5)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_5))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))))
    (libpart (lib conn) (part RJ45)
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name SHIELD) (type passive)))))
  (libraries
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib)))
  (nets
    (net (code 1) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1))
      (node (ref P1) (pin 4)))
    (net (code 2) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2))
      (node (ref P1) (pin 3)))
    (net (code 3) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3))
      (node (ref P1) (pin 2)))
    (net (code 4) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4))
      (node (ref P1) (pin 1)))
    (net (code 5) (name "Net-(J1-Pad5)")
      (node (ref J1) (pin 5))
      (node (ref P2) (pin 5)))
    (net (code 6) (name "Net-(J1-Pad6)")
      (node (ref J1) (pin 6))
      (node (ref P2) (pin 4)))
    (net (code 7) (name "Net-(J1-Pad7)")
      (node (ref J1) (pin 7))
      (node (ref P2) (pin 3)))
    (net (code 8) (name "Net-(J1-Pad8)")
      (node (ref J1) (pin 8))
      (node (ref P2) (pin 2)))
    (net (code 9) (name "Net-(J1-Pad9)")
      (node (ref J1) (pin 9))
      (node (ref P2) (pin 1)))))
