(export (version D)
  (design
    (source db25_bob.sch)
    (date "Di 01 Dez 2015 00:33:59 CET")
    (tool "Eeschema (2015-11-22 BZR 6327)-product")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source db25_bob.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /Encoder/) (tstamps /563A2AF8/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source encoder.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value DB25)
      (footprint Connect:DB25FD)
      (libsource (lib conn) (part DB25))
      (sheetpath (names /) (tstamps /))
      (tstamp 56392616))
    (comp (ref U8)
      (value ADuM1201WT)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib interface) (part ADuM1201WT))
      (sheetpath (names /) (tstamps /))
      (tstamp 5639453C))
    (comp (ref U7)
      (value ADuM1201WT)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib interface) (part ADuM1201WT))
      (sheetpath (names /) (tstamps /))
      (tstamp 563945E9))
    (comp (ref U6)
      (value ADuM1201WT)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib interface) (part ADuM1201WT))
      (sheetpath (names /) (tstamps /))
      (tstamp 56394653))
    (comp (ref C4)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5639F65A))
    (comp (ref C6)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5639F77D))
    (comp (ref C8)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5639F825))
    (comp (ref C10)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5639F869))
    (comp (ref C12)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5639F8AE))
    (comp (ref C14)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5639F8FA))
    (comp (ref C16)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5639F949))
    (comp (ref C2)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5639F997))
    (comp (ref C3)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5639FDE2))
    (comp (ref C5)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5639FDE8))
    (comp (ref C7)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5639FDEE))
    (comp (ref C9)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5639FDF4))
    (comp (ref C11)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5639FDFA))
    (comp (ref C13)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5639FE00))
    (comp (ref C15)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5639FE06))
    (comp (ref C1)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5639FE0C))
    (comp (ref U1)
      (value ADuM1201WT)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib interface) (part ADuM1201WT))
      (sheetpath (names /) (tstamps /))
      (tstamp 563A36D0))
    (comp (ref U5)
      (value ADuM1201WT)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib interface) (part ADuM1201WT))
      (sheetpath (names /) (tstamps /))
      (tstamp 563A36D6))
    (comp (ref U4)
      (value ADuM1201WT)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib interface) (part ADuM1201WT))
      (sheetpath (names /) (tstamps /))
      (tstamp 563A36DC))
    (comp (ref U3)
      (value ADuM1201WT)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib interface) (part ADuM1201WT))
      (sheetpath (names /) (tstamps /))
      (tstamp 563A384E))
    (comp (ref U2)
      (value ADuM1201WT)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib interface) (part ADuM1201WT))
      (sheetpath (names /) (tstamps /))
      (tstamp 563A3854))
    (comp (ref D1)
      (value LED)
      (footprint LEDs:LED-0805)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 563A5274))
    (comp (ref R1)
      (value R)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 563A5311))
    (comp (ref D2)
      (value LED)
      (footprint LEDs:LED-0805)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 563A53E1))
    (comp (ref R2)
      (value R)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 563A53E7))
    (comp (ref D3)
      (value LED)
      (footprint LEDs:LED-0805)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 563A59FE))
    (comp (ref R3)
      (value R)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 563A5A04))
    (comp (ref P2)
      (value DIL8)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib conn) (part DIL8))
      (sheetpath (names /) (tstamps /))
      (tstamp 563A8871))
    (comp (ref P4)
      (value DIL8)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib conn) (part DIL8))
      (sheetpath (names /) (tstamps /))
      (tstamp 563AA0A9))
    (comp (ref P5)
      (value DIL8)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib conn) (part DIL8))
      (sheetpath (names /) (tstamps /))
      (tstamp 563AA173))
    (comp (ref P6)
      (value DIL8)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib conn) (part DIL8))
      (sheetpath (names /) (tstamps /))
      (tstamp 563AA4D3))
    (comp (ref P1)
      (value DIL8)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib conn) (part DIL8))
      (sheetpath (names /) (tstamps /))
      (tstamp 563AA72F))
    (comp (ref P3)
      (value DIL6)
      (footprint Housings_SOT-23_SOT-143_TSOT-6:SC-70-6)
      (libsource (lib conn) (part DIL6))
      (sheetpath (names /) (tstamps /))
      (tstamp 563AD013))
    (comp (ref R9)
      (value R)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 563AE572))
    (comp (ref R10)
      (value R)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 563AE64F))
    (comp (ref R11)
      (value R)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 563AE711))
    (comp (ref R6)
      (value R)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 563AFB1C))
    (comp (ref R7)
      (value R)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 563AFC20))
    (comp (ref C23)
      (value C)
      (footprint Capacitors_SMD:C_0805)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 563AFCDF))
    (comp (ref R8)
      (value R)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 563B02F7))
    (comp (ref R12)
      (value R)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 563B02FD))
    (comp (ref C24)
      (value C)
      (footprint Capacitors_SMD:C_0805)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 563B0303))
    (comp (ref R4)
      (value R)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 563B05DE))
    (comp (ref R5)
      (value R)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 563B05E4))
    (comp (ref C22)
      (value C)
      (footprint Capacitors_SMD:C_0805)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 563B05EA))
    (comp (ref J7)
      (value RJ45)
      (footprint Connect:RJ45_8)
      (libsource (lib conn) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 563FE95B))
    (comp (ref J10)
      (value RJ45)
      (footprint Connect:RJ45_8)
      (libsource (lib conn) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 563FEA93))
    (comp (ref J8)
      (value RJ45)
      (footprint Connect:RJ45_8)
      (libsource (lib conn) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 563FEB85))
    (comp (ref J9)
      (value RJ45)
      (footprint Connect:RJ45_8)
      (libsource (lib conn) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 5640523C))
    (comp (ref P10)
      (value CONN_2)
      (footprint Sockets_WAGO734:WAGO_734_2pin_Straight_RuggedPads)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 5640E11C))
    (comp (ref C17)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5640F251))
    (comp (ref Q1)
      (value FET_N)
      (footprint Transistors_SMD:sc70)
      (libsource (lib device) (part FET_N))
      (sheetpath (names /) (tstamps /))
      (tstamp 5641787F))
    (comp (ref Q2)
      (value FET_N)
      (footprint Transistors_SMD:sc70)
      (libsource (lib device) (part FET_N))
      (sheetpath (names /) (tstamps /))
      (tstamp 564179AE))
    (comp (ref Q3)
      (value FET_N)
      (footprint Transistors_SMD:sc70)
      (libsource (lib device) (part FET_N))
      (sheetpath (names /) (tstamps /))
      (tstamp 56417AD1))
    (comp (ref P11)
      (value CONN_6)
      (footprint Sockets_WAGO734:WAGO_734_6pin_Straight_RuggedPads)
      (libsource (lib conn) (part CONN_6))
      (sheetpath (names /) (tstamps /))
      (tstamp 564210DC))
    (comp (ref P13)
      (value CONN_6)
      (footprint Sockets_WAGO734:WAGO_734_6pin_Straight_RuggedPads)
      (libsource (lib conn) (part CONN_6))
      (sheetpath (names /) (tstamps /))
      (tstamp 5642124C))
    (comp (ref P15)
      (value CONN_4)
      (footprint custom_footprints:SIP7)
      (libsource (lib conn) (part CONN_4))
      (sheetpath (names /) (tstamps /))
      (tstamp 565150F1))
    (comp (ref J11)
      (value RJ45)
      (footprint Connect:RJ45_8)
      (libsource (lib conn) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 563FEC84))
    (comp (ref D4)
      (value DIODE)
      (footprint Diodes_SMD:MiniMELF_Standard)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /) (tstamps /))
      (tstamp 565D8D3E))
    (comp (ref D5)
      (value DIODE)
      (footprint Diodes_SMD:MiniMELF_Standard)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /) (tstamps /))
      (tstamp 565D8EC8))
    (comp (ref D6)
      (value DIODE)
      (footprint Diodes_SMD:MiniMELF_Standard)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /) (tstamps /))
      (tstamp 565D8FAE))
    (comp (ref J2)
      (value DB25)
      (footprint Connect:DB25FD)
      (libsource (lib conn) (part DB25))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563A2DB1))
    (comp (ref U11)
      (value ADuM1200CR)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib interface) (part ADuM1200CR))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D3E41))
    (comp (ref U10)
      (value ADuM1200CR)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib interface) (part ADuM1200CR))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D3E9D))
    (comp (ref U9)
      (value ADuM1200CR)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib interface) (part ADuM1200CR))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D3EDA))
    (comp (ref U12)
      (value ADuM1200CR)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib interface) (part ADuM1200CR))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D3F0E))
    (comp (ref C25)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D611F))
    (comp (ref C27)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D61F8))
    (comp (ref C29)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D6229))
    (comp (ref C31)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D625D))
    (comp (ref C33)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D6294))
    (comp (ref C35)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D62CE))
    (comp (ref C36)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D630B))
    (comp (ref C34)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D635D))
    (comp (ref C32)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D63A0))
    (comp (ref C30)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D63E6))
    (comp (ref C28)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D642F))
    (comp (ref C26)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D647B))
    (comp (ref J3)
      (value RJ45)
      (footprint Connect:RJ45_8)
      (libsource (lib conn) (part RJ45))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D7321))
    (comp (ref J4)
      (value RJ45)
      (footprint Connect:RJ45_8)
      (libsource (lib conn) (part RJ45))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D7420))
    (comp (ref J6)
      (value RJ45)
      (footprint Connect:RJ45_8)
      (libsource (lib conn) (part RJ45))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D74A3))
    (comp (ref J5)
      (value RJ45)
      (footprint Connect:RJ45_8)
      (libsource (lib conn) (part RJ45))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D751D))
    (comp (ref P9)
      (value DIL16)
      (footprint Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm)
      (libsource (lib conn) (part DIL16))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D7EC4))
    (comp (ref P8)
      (value DIL16)
      (footprint Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm)
      (libsource (lib conn) (part DIL16))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D7F7B))
    (comp (ref P7)
      (value DIL16)
      (footprint Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm)
      (libsource (lib conn) (part DIL16))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D8003))
    (comp (ref U13)
      (value ADuM1200CR)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib interface) (part ADuM1200CR))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D867A))
    (comp (ref U14)
      (value ADuM1200CR)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib interface) (part ADuM1200CR))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563D87C6))
    (comp (ref C37)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563E5ABD))
    (comp (ref C39)
      (value C)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part C))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 563E5D4D))
    (comp (ref P12)
      (value CONN_7)
      (footprint Socket_Strips:Socket_Strip_Straight_1x07)
      (libsource (lib conn) (part CONN_7))
      (sheetpath (names /Encoder/) (tstamps /563A2AF8/))
      (tstamp 565BA284)))
  (libparts
    (libpart (lib interface) (part ADUM1200AR)
      (aliases
        (alias ADuM1200BR)
        (alias ADuM1200CR)
        (alias ADuM1200WS)
        (alias ADuM1200WT)
        (alias ADuM1200WU))
      (description "ADuM1200AR, Dual-Channel Digital Isolator, 1Mbps 150ns, SO8")
      (docs http://www.analog.com/static/imported-files/data_sheets/ADuM1200_1201.pdf)
      (footprints
        (fp SO*))
      (fields
        (field (name Reference) U)
        (field (name Value) ADUM1200AR)
        (field (name Footprint) SO8))
      (pins
        (pin (num 1) (name VDD1) (type power_in))
        (pin (num 2) (name VIA) (type input))
        (pin (num 3) (name VIB) (type input))
        (pin (num 4) (name GND1) (type power_in))
        (pin (num 5) (name GND2) (type power_in))
        (pin (num 6) (name VOB) (type output))
        (pin (num 7) (name VOA) (type output))
        (pin (num 8) (name VDD2) (type power_in))))
    (libpart (lib interface) (part ADuM1201AR)
      (aliases
        (alias ADuM1201BR)
        (alias ADuM1201CR)
        (alias ADuM1201WS)
        (alias ADuM1201WT)
        (alias ADuM1201WU))
      (description "ADuM1201AR, Dual-Channel Digital Isolator, 1Mbps 150ns, SO8")
      (docs http://www.analog.com/static/imported-files/data_sheets/ADuM1200_1201.pdf)
      (footprints
        (fp SO*))
      (fields
        (field (name Reference) U)
        (field (name Value) ADuM1201AR)
        (field (name Footprint) SO8))
      (pins
        (pin (num 1) (name VDD1) (type power_in))
        (pin (num 2) (name VOA) (type output))
        (pin (num 3) (name VIB) (type input))
        (pin (num 4) (name GND1) (type power_in))
        (pin (num 5) (name GND2) (type power_in))
        (pin (num 6) (name VOB) (type output))
        (pin (num 7) (name VIA) (type input))
        (pin (num 8) (name VDD2) (type power_in))))
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib conn) (part CONN_4)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_4))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib conn) (part CONN_6)
      (description "ymbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_6))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))))
    (libpart (lib conn) (part CONN_7)
      (description "Symbole general pour connexions")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_7))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))))
    (libpart (lib conn) (part DB25)
      (footprints
        (fp DB25*))
      (fields
        (field (name Reference) J)
        (field (name Value) DB25))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))
        (pin (num 9) (name 9) (type passive))
        (pin (num 10) (name 10) (type passive))
        (pin (num 11) (name 11) (type passive))
        (pin (num 12) (name 12) (type passive))
        (pin (num 13) (name 13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name P25) (type passive))))
    (libpart (lib conn) (part DIL16)
      (fields
        (field (name Reference) P)
        (field (name Value) DIL16))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))
        (pin (num 9) (name 9) (type passive))
        (pin (num 10) (name 10) (type passive))
        (pin (num 11) (name 11) (type passive))
        (pin (num 12) (name 12) (type passive))
        (pin (num 13) (name 13) (type passive))
        (pin (num 14) (name 14) (type passive))
        (pin (num 15) (name 15) (type passive))
        (pin (num 16) (name 16) (type passive))))
    (libpart (lib conn) (part DIL6)
      (fields
        (field (name Reference) P)
        (field (name Value) DIL6))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib conn) (part DIL8)
      (fields
        (field (name Reference) P)
        (field (name Value) DIL8))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))))
    (libpart (lib device) (part DIODE)
      (description "Diode simple")
      (footprints
        (fp D?)
        (fp S*))
      (fields
        (field (name Reference) D)
        (field (name Value) DIODE))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part FET_N)
      (fields
        (field (name Reference) Q)
        (field (name Value) FET_N))
      (pins
        (pin (num D) (name D) (type passive))
        (pin (num G) (name G) (type input))
        (pin (num S) (name S) (type passive))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part RJ45)
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name SHIELD) (type passive)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical interface)
      (uri /usr/share/kicad/library/interface.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib)))
  (nets
    (net (code 1) (name IO1)
      (node (ref U6) (pin 2))
      (node (ref J1) (pin 5)))
    (net (code 2) (name IO2)
      (node (ref U7) (pin 3))
      (node (ref J1) (pin 6)))
    (net (code 3) (name IO3)
      (node (ref J1) (pin 7))
      (node (ref U7) (pin 2)))
    (net (code 4) (name IO4)
      (node (ref J1) (pin 8))
      (node (ref U8) (pin 3)))
    (net (code 5) (name IO5)
      (node (ref J1) (pin 9))
      (node (ref U8) (pin 2)))
    (net (code 6) (name IO0)
      (node (ref U6) (pin 3))
      (node (ref J1) (pin 17)))
    (net (code 7) (name IO16)
      (node (ref J1) (pin 1))
      (node (ref R3) (pin 1)))
    (net (code 8) (name IO10)
      (node (ref J1) (pin 14))
      (node (ref U1) (pin 3)))
    (net (code 9) (name IO11)
      (node (ref U1) (pin 2))
      (node (ref J1) (pin 2)))
    (net (code 10) (name IO8)
      (node (ref U5) (pin 3))
      (node (ref J1) (pin 12)))
    (net (code 11) (name IO9)
      (node (ref J1) (pin 13))
      (node (ref U5) (pin 2)))
    (net (code 12) (name IO6)
      (node (ref J1) (pin 10))
      (node (ref U4) (pin 3)))
    (net (code 13) (name IO7)
      (node (ref U4) (pin 2))
      (node (ref J1) (pin 11)))
    (net (code 14) (name IO14)
      (node (ref U3) (pin 3))
      (node (ref J1) (pin 16)))
    (net (code 15) (name IO15)
      (node (ref J1) (pin 4))
      (node (ref U3) (pin 2)))
    (net (code 16) (name IO12)
      (node (ref J1) (pin 15))
      (node (ref U2) (pin 3)))
    (net (code 17) (name IO13)
      (node (ref J1) (pin 3))
      (node (ref U2) (pin 2)))
    (net (code 18) (name OUT1)
      (node (ref Q2) (pin G))
      (node (ref U2) (pin 7)))
    (net (code 19) (name OUT2)
      (node (ref Q3) (pin G))
      (node (ref U3) (pin 7)))
    (net (code 20) (name OUT2FET)
      (node (ref P13) (pin 5))
      (node (ref Q3) (pin D))
      (node (ref D6) (pin 2)))
    (net (code 21) (name OUT1FET)
      (node (ref P13) (pin 3))
      (node (ref D5) (pin 2))
      (node (ref Q2) (pin D)))
    (net (code 22) (name IN0)
      (node (ref P11) (pin 1))
      (node (ref R9) (pin 1)))
    (net (code 23) (name IN1)
      (node (ref R10) (pin 1))
      (node (ref P11) (pin 3)))
    (net (code 24) (name IN2)
      (node (ref P11) (pin 5))
      (node (ref R11) (pin 1)))
    (net (code 25) (name +24V)
      (node (ref P13) (pin 4))
      (node (ref P13) (pin 6))
      (node (ref P15) (pin 1))
      (node (ref C17) (pin 1))
      (node (ref P13) (pin 2))
      (node (ref P10) (pin 2)))
    (net (code 26) (name OUT0FET)
      (node (ref Q1) (pin D))
      (node (ref D4) (pin 2))
      (node (ref P13) (pin 1)))
    (net (code 27) (name OUT0)
      (node (ref U1) (pin 7))
      (node (ref Q1) (pin G)))
    (net (code 28) (name 5V1)
      (node (ref U7) (pin 8))
      (node (ref P2) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref J10) (pin 7)))
    (net (code 29) (name 5V4)
      (node (ref U5) (pin 8))
      (node (ref P6) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref J9) (pin 7)))
    (net (code 30) (name 5V3)
      (node (ref U4) (pin 8))
      (node (ref C3) (pin 1))
      (node (ref P5) (pin 1))
      (node (ref J11) (pin 7)))
    (net (code 31) (name 5V2)
      (node (ref J8) (pin 7))
      (node (ref U8) (pin 8))
      (node (ref P4) (pin 1))
      (node (ref C5) (pin 1)))
    (net (code 32) (name 5V0)
      (node (ref C15) (pin 1))
      (node (ref P1) (pin 1))
      (node (ref U6) (pin 8))
      (node (ref J7) (pin 7)))
    (net (code 33) (name +5VA)
      (node (ref C39) (pin 1))
      (node (ref C37) (pin 1))
      (node (ref J3) (pin 7))
      (node (ref P9) (pin 4))
      (node (ref P7) (pin 4))
      (node (ref R7) (pin 1))
      (node (ref J4) (pin 7))
      (node (ref U3) (pin 8))
      (node (ref P8) (pin 16))
      (node (ref U1) (pin 8))
      (node (ref R1) (pin 1))
      (node (ref P9) (pin 16))
      (node (ref C32) (pin 1))
      (node (ref C26) (pin 1))
      (node (ref C30) (pin 1))
      (node (ref C28) (pin 1))
      (node (ref P8) (pin 4))
      (node (ref C13) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref C34) (pin 1))
      (node (ref P3) (pin 5))
      (node (ref U9) (pin 1))
      (node (ref P15) (pin 4))
      (node (ref R12) (pin 1))
      (node (ref U11) (pin 1))
      (node (ref U12) (pin 1))
      (node (ref U13) (pin 1))
      (node (ref P7) (pin 16))
      (node (ref U10) (pin 1))
      (node (ref U14) (pin 1))
      (node (ref J5) (pin 7))
      (node (ref U2) (pin 8))
      (node (ref R5) (pin 1))
      (node (ref J6) (pin 7))
      (node (ref C36) (pin 1)))
    (net (code 34) (name 3TX+)
      (node (ref P5) (pin 5))
      (node (ref J11) (pin 1)))
    (net (code 35) (name 3TX-)
      (node (ref J11) (pin 2))
      (node (ref P5) (pin 6)))
    (net (code 36) (name "Net-(J11-Pad3)")
      (node (ref J11) (pin 3)))
    (net (code 37) (name 3RX-)
      (node (ref J11) (pin 4))
      (node (ref P5) (pin 7)))
    (net (code 38) (name 3RX+)
      (node (ref P5) (pin 8))
      (node (ref J11) (pin 5)))
    (net (code 39) (name "Net-(J11-Pad6)")
      (node (ref J11) (pin 6)))
    (net (code 40) (name 4TX+)
      (node (ref P6) (pin 5))
      (node (ref J9) (pin 1)))
    (net (code 41) (name 4TX-)
      (node (ref J9) (pin 2))
      (node (ref P6) (pin 6)))
    (net (code 42) (name 4RX-)
      (node (ref J9) (pin 4))
      (node (ref P6) (pin 7)))
    (net (code 43) (name 4RX+)
      (node (ref J9) (pin 5))
      (node (ref P6) (pin 8)))
    (net (code 44) (name GND0)
      (node (ref U6) (pin 5))
      (node (ref P1) (pin 4))
      (node (ref J7) (pin 8))
      (node (ref J7) (pin 9))
      (node (ref C15) (pin 2)))
    (net (code 45) (name GND1)
      (node (ref C7) (pin 2))
      (node (ref P2) (pin 4))
      (node (ref J10) (pin 8))
      (node (ref J10) (pin 9))
      (node (ref U7) (pin 5)))
    (net (code 46) (name GND2)
      (node (ref U8) (pin 5))
      (node (ref J8) (pin 8))
      (node (ref P4) (pin 4))
      (node (ref J8) (pin 9))
      (node (ref C5) (pin 2)))
    (net (code 47) (name GND3)
      (node (ref U4) (pin 5))
      (node (ref P5) (pin 4))
      (node (ref J11) (pin 9))
      (node (ref J11) (pin 8))
      (node (ref C3) (pin 2)))
    (net (code 48) (name GND4)
      (node (ref J9) (pin 9))
      (node (ref C1) (pin 2))
      (node (ref U5) (pin 5))
      (node (ref P6) (pin 4))
      (node (ref J9) (pin 8)))
    (net (code 49) (name 0RX)
      (node (ref U6) (pin 7))
      (node (ref P1) (pin 2)))
    (net (code 50) (name 2TX)
      (node (ref P4) (pin 3))
      (node (ref U8) (pin 6)))
    (net (code 51) (name 2RX)
      (node (ref U8) (pin 7))
      (node (ref P4) (pin 2)))
    (net (code 52) (name 1TX)
      (node (ref U7) (pin 6))
      (node (ref P2) (pin 3)))
    (net (code 53) (name 1RX)
      (node (ref U7) (pin 7))
      (node (ref P2) (pin 2)))
    (net (code 54) (name 0TX)
      (node (ref U6) (pin 6))
      (node (ref P1) (pin 3)))
    (net (code 55) (name 4TX)
      (node (ref U5) (pin 6))
      (node (ref P6) (pin 3)))
    (net (code 56) (name 4RX)
      (node (ref U5) (pin 7))
      (node (ref P6) (pin 2)))
    (net (code 57) (name 3TX)
      (node (ref U4) (pin 6))
      (node (ref P5) (pin 3)))
    (net (code 58) (name 3RX)
      (node (ref P5) (pin 2))
      (node (ref U4) (pin 7)))
    (net (code 59) (name 0RX+)
      (node (ref J7) (pin 5))
      (node (ref P1) (pin 8)))
    (net (code 60) (name IN1R)
      (node (ref P3) (pin 3))
      (node (ref R10) (pin 2))
      (node (ref R6) (pin 1)))
    (net (code 61) (name IN2R)
      (node (ref R11) (pin 2))
      (node (ref R8) (pin 1))
      (node (ref P3) (pin 4)))
    (net (code 62) (name 0TX+)
      (node (ref J7) (pin 1))
      (node (ref P1) (pin 5)))
    (net (code 63) (name 0TX-)
      (node (ref J7) (pin 2))
      (node (ref P1) (pin 6)))
    (net (code 64) (name 0RX-)
      (node (ref J7) (pin 4))
      (node (ref P1) (pin 7)))
    (net (code 65) (name 1TX+)
      (node (ref J10) (pin 1))
      (node (ref P2) (pin 5)))
    (net (code 66) (name 1TX-)
      (node (ref P2) (pin 6))
      (node (ref J10) (pin 2)))
    (net (code 67) (name 1RX-)
      (node (ref J10) (pin 4))
      (node (ref P2) (pin 7)))
    (net (code 68) (name 1RX+)
      (node (ref P2) (pin 8))
      (node (ref J10) (pin 5)))
    (net (code 69) (name 2TX+)
      (node (ref J8) (pin 1))
      (node (ref P4) (pin 5)))
    (net (code 70) (name 2TX-)
      (node (ref J8) (pin 2))
      (node (ref P4) (pin 6)))
    (net (code 71) (name 2RX-)
      (node (ref P4) (pin 7))
      (node (ref J8) (pin 4)))
    (net (code 72) (name 2RX+)
      (node (ref P4) (pin 8))
      (node (ref J8) (pin 5)))
    (net (code 73) (name IN0R)
      (node (ref R4) (pin 1))
      (node (ref R9) (pin 2))
      (node (ref P3) (pin 1)))
    (net (code 74) (name GND)
      (node (ref D2) (pin 2))
      (node (ref D3) (pin 2))
      (node (ref U5) (pin 4))
      (node (ref U1) (pin 4))
      (node (ref U4) (pin 4))
      (node (ref J2) (pin 20))
      (node (ref J2) (pin 21))
      (node (ref U12) (pin 5))
      (node (ref C29) (pin 2))
      (node (ref C35) (pin 2))
      (node (ref C33) (pin 2))
      (node (ref C31) (pin 2))
      (node (ref C27) (pin 2))
      (node (ref C25) (pin 2))
      (node (ref U3) (pin 4))
      (node (ref J2) (pin 18))
      (node (ref J2) (pin 19))
      (node (ref C10) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref U7) (pin 4))
      (node (ref U6) (pin 4))
      (node (ref C12) (pin 2))
      (node (ref U9) (pin 5))
      (node (ref P12) (pin 7))
      (node (ref U13) (pin 5))
      (node (ref U14) (pin 5))
      (node (ref U10) (pin 5))
      (node (ref U2) (pin 4))
      (node (ref U11) (pin 5))
      (node (ref U8) (pin 4))
      (node (ref J1) (pin 20))
      (node (ref J1) (pin 21))
      (node (ref J1) (pin 18))
      (node (ref J1) (pin 19))
      (node (ref C8) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C6) (pin 2)))
    (net (code 75) (name EN-)
      (node (ref J5) (pin 8))
      (node (ref U13) (pin 4))
      (node (ref P8) (pin 8))
      (node (ref P9) (pin 12))
      (node (ref P9) (pin 8))
      (node (ref P7) (pin 12))
      (node (ref P7) (pin 8))
      (node (ref P8) (pin 12))
      (node (ref J4) (pin 9))
      (node (ref J4) (pin 8))
      (node (ref J3) (pin 9))
      (node (ref J3) (pin 8))
      (node (ref J5) (pin 9))
      (node (ref J6) (pin 9))
      (node (ref J6) (pin 8))
      (node (ref U9) (pin 4))
      (node (ref U10) (pin 4))
      (node (ref U11) (pin 4))
      (node (ref U12) (pin 4))
      (node (ref C36) (pin 2))
      (node (ref U14) (pin 4))
      (node (ref C26) (pin 2))
      (node (ref C28) (pin 2))
      (node (ref C30) (pin 2))
      (node (ref C32) (pin 2))
      (node (ref C34) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref P10) (pin 1))
      (node (ref P3) (pin 2))
      (node (ref C23) (pin 2))
      (node (ref U2) (pin 5))
      (node (ref U3) (pin 5))
      (node (ref P11) (pin 6))
      (node (ref P11) (pin 4))
      (node (ref P11) (pin 2))
      (node (ref Q3) (pin S))
      (node (ref Q2) (pin S))
      (node (ref C22) (pin 2))
      (node (ref C24) (pin 2))
      (node (ref D6) (pin 1))
      (node (ref P15) (pin 3))
      (node (ref P15) (pin 2))
      (node (ref D4) (pin 1))
      (node (ref Q1) (pin S))
      (node (ref C17) (pin 2))
      (node (ref D5) (pin 1))
      (node (ref U1) (pin 5))
      (node (ref C37) (pin 2))
      (node (ref C39) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref C9) (pin 2)))
    (net (code 76) (name +5V)
      (node (ref C33) (pin 1))
      (node (ref U3) (pin 1))
      (node (ref U6) (pin 1))
      (node (ref J2) (pin 23))
      (node (ref C31) (pin 1))
      (node (ref C29) (pin 1))
      (node (ref J2) (pin 24))
      (node (ref C27) (pin 1))
      (node (ref C25) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref U4) (pin 1))
      (node (ref J1) (pin 25))
      (node (ref J1) (pin 24))
      (node (ref C8) (pin 1))
      (node (ref J1) (pin 23))
      (node (ref J1) (pin 22))
      (node (ref U5) (pin 1))
      (node (ref U8) (pin 1))
      (node (ref J2) (pin 25))
      (node (ref U2) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref U7) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C16) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref C35) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref U14) (pin 8))
      (node (ref U13) (pin 8))
      (node (ref U10) (pin 8))
      (node (ref U11) (pin 8))
      (node (ref U9) (pin 8))
      (node (ref U12) (pin 8))
      (node (ref R2) (pin 1))
      (node (ref J2) (pin 22))
      (node (ref P12) (pin 1)))
    (net (code 77) (name IN2P)
      (node (ref R8) (pin 2))
      (node (ref C24) (pin 1))
      (node (ref U3) (pin 6))
      (node (ref R12) (pin 2)))
    (net (code 78) (name IN0P)
      (node (ref U1) (pin 6))
      (node (ref R4) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref C22) (pin 1)))
    (net (code 79) (name "Net-(J7-Pad3)")
      (node (ref J7) (pin 3)))
    (net (code 80) (name IN1P)
      (node (ref U2) (pin 6))
      (node (ref R6) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref C23) (pin 1)))
    (net (code 81) (name "Net-(J9-Pad3)")
      (node (ref J9) (pin 3)))
    (net (code 82) (name "Net-(J9-Pad6)")
      (node (ref J9) (pin 6)))
    (net (code 83) (name "Net-(J7-Pad6)")
      (node (ref J7) (pin 6)))
    (net (code 84) (name "Net-(J10-Pad3)")
      (node (ref J10) (pin 3)))
    (net (code 85) (name "Net-(J10-Pad6)")
      (node (ref J10) (pin 6)))
    (net (code 86) (name "Net-(D1-Pad1)")
      (node (ref R1) (pin 2))
      (node (ref D1) (pin 1)))
    (net (code 87) (name "Net-(J8-Pad3)")
      (node (ref J8) (pin 3)))
    (net (code 88) (name "Net-(J8-Pad6)")
      (node (ref J8) (pin 6)))
    (net (code 89) (name "Net-(D2-Pad1)")
      (node (ref D2) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 90) (name "Net-(D3-Pad1)")
      (node (ref D3) (pin 1))
      (node (ref R3) (pin 2)))
    (net (code 91) (name "Net-(P3-Pad6)")
      (node (ref P3) (pin 6)))
    (net (code 92) (name ENC2B)
      (node (ref U12) (pin 3))
      (node (ref P8) (pin 3)))
    (net (code 93) (name ENC1B)
      (node (ref P8) (pin 11))
      (node (ref U11) (pin 2)))
    (net (code 94) (name ENC2Z)
      (node (ref P8) (pin 5))
      (node (ref U12) (pin 2)))
    (net (code 95) (name ENC1A)
      (node (ref U11) (pin 3))
      (node (ref P8) (pin 13)))
    (net (code 96) (name ENC0B)
      (node (ref P7) (pin 13))
      (node (ref U9) (pin 3)))
    (net (code 97) (name ENC0A)
      (node (ref P7) (pin 11))
      (node (ref U9) (pin 2)))
    (net (code 98) (name ENC1Z)
      (node (ref P7) (pin 5))
      (node (ref U10) (pin 2)))
    (net (code 99) (name ENC0Z)
      (node (ref P7) (pin 3))
      (node (ref U10) (pin 3)))
    (net (code 100) (name ENC2B+)
      (node (ref J5) (pin 3))
      (node (ref P8) (pin 2)))
    (net (code 101) (name ENC1A+)
      (node (ref J4) (pin 1))
      (node (ref P8) (pin 14)))
    (net (code 102) (name ENC1A-)
      (node (ref J4) (pin 2))
      (node (ref P8) (pin 15)))
    (net (code 103) (name ENC1B-)
      (node (ref P8) (pin 9))
      (node (ref J4) (pin 6)))
    (net (code 104) (name ENC1B+)
      (node (ref P8) (pin 10))
      (node (ref J4) (pin 3)))
    (net (code 105) (name ENC1Z-)
      (node (ref J4) (pin 4))
      (node (ref P7) (pin 7)))
    (net (code 106) (name ENC1Z+)
      (node (ref J4) (pin 5))
      (node (ref P7) (pin 6)))
    (net (code 107) (name ENC2A+)
      (node (ref J5) (pin 1))
      (node (ref P9) (pin 14)))
    (net (code 108) (name ENC2A-)
      (node (ref J5) (pin 2))
      (node (ref P9) (pin 15)))
    (net (code 109) (name ENC2B-)
      (node (ref P8) (pin 1))
      (node (ref J5) (pin 6)))
    (net (code 110) (name ENC0Z+)
      (node (ref P7) (pin 2))
      (node (ref J3) (pin 5)))
    (net (code 111) (name ENC2Z-)
      (node (ref P8) (pin 7))
      (node (ref J5) (pin 4)))
    (net (code 112) (name ENC2Z+)
      (node (ref J5) (pin 5))
      (node (ref P8) (pin 6)))
    (net (code 113) (name ENC3A+)
      (node (ref P9) (pin 6))
      (node (ref J6) (pin 1)))
    (net (code 114) (name ENC3A-)
      (node (ref J6) (pin 2))
      (node (ref P9) (pin 7)))
    (net (code 115) (name ENC3B+)
      (node (ref J6) (pin 3))
      (node (ref P9) (pin 10)))
    (net (code 116) (name ENC3B-)
      (node (ref P9) (pin 9))
      (node (ref J6) (pin 6)))
    (net (code 117) (name ENC3Z-)
      (node (ref J6) (pin 4))
      (node (ref P9) (pin 1)))
    (net (code 118) (name ENC3Z+)
      (node (ref P9) (pin 2))
      (node (ref J6) (pin 5)))
    (net (code 119) (name ENC0A-)
      (node (ref J3) (pin 2))
      (node (ref P7) (pin 9)))
    (net (code 120) (name ENC0A+)
      (node (ref J3) (pin 1))
      (node (ref P7) (pin 10)))
    (net (code 121) (name ENC0B-)
      (node (ref J3) (pin 6))
      (node (ref P7) (pin 15)))
    (net (code 122) (name ENC0B+)
      (node (ref J3) (pin 3))
      (node (ref P7) (pin 14)))
    (net (code 123) (name ENC0Z-)
      (node (ref P7) (pin 1))
      (node (ref J3) (pin 4)))
    (net (code 124) (name ENC2AO)
      (node (ref U13) (pin 6))
      (node (ref J2) (pin 5)))
    (net (code 125) (name ENC0AO)
      (node (ref J2) (pin 12))
      (node (ref U9) (pin 7)))
    (net (code 126) (name ENC0BO)
      (node (ref U9) (pin 6))
      (node (ref J2) (pin 13)))
    (net (code 127) (name ENC0ZO)
      (node (ref U10) (pin 6))
      (node (ref J2) (pin 11)))
    (net (code 128) (name ENC1AO)
      (node (ref J2) (pin 9))
      (node (ref U11) (pin 6)))
    (net (code 129) (name ENC1BO)
      (node (ref U11) (pin 7))
      (node (ref J2) (pin 8)))
    (net (code 130) (name ENC1ZO)
      (node (ref J2) (pin 10))
      (node (ref U10) (pin 7)))
    (net (code 131) (name ENC2BO)
      (node (ref U12) (pin 6))
      (node (ref J2) (pin 7)))
    (net (code 132) (name ENC2ZO)
      (node (ref J2) (pin 6))
      (node (ref U12) (pin 7)))
    (net (code 133) (name ENC3AO)
      (node (ref J2) (pin 16))
      (node (ref U14) (pin 7)))
    (net (code 134) (name ENC3BO)
      (node (ref J2) (pin 17))
      (node (ref U13) (pin 7)))
    (net (code 135) (name ENC3ZO)
      (node (ref U14) (pin 6))
      (node (ref J2) (pin 4)))
    (net (code 136) (name "Net-(J2-Pad1)")
      (node (ref P12) (pin 2))
      (node (ref J2) (pin 1)))
    (net (code 137) (name "Net-(J2-Pad14)")
      (node (ref J2) (pin 14))
      (node (ref P12) (pin 3)))
    (net (code 138) (name "Net-(J2-Pad2)")
      (node (ref J2) (pin 2))
      (node (ref P12) (pin 4)))
    (net (code 139) (name "Net-(J2-Pad15)")
      (node (ref J2) (pin 15))
      (node (ref P12) (pin 5)))
    (net (code 140) (name "Net-(J2-Pad3)")
      (node (ref J2) (pin 3))
      (node (ref P12) (pin 6)))
    (net (code 141) (name ENC3B)
      (node (ref P9) (pin 11))
      (node (ref U13) (pin 2)))
    (net (code 142) (name ENC2A)
      (node (ref P9) (pin 13))
      (node (ref U13) (pin 3)))
    (net (code 143) (name ENC3A)
      (node (ref U14) (pin 2))
      (node (ref P9) (pin 5)))
    (net (code 144) (name ENC3Z)
      (node (ref U14) (pin 3))
      (node (ref P9) (pin 3)))))
