(export (version D)
  (design
    (source /Users/rene/dev/stmbl/hw/kicad/powerstep/powerstep.sch)
    (date "2017 October 28, Saturday 17:31:59")
    (tool "Eeschema (2017-07-31 revision 816307e)-master")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source powerstep.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /stepper/) (tstamps /59F49F2C/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source stepper.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /stepper2/) (tstamps /59F4C6C6/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source stepper.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value POWERSTEP01)
      (footprint stmbl:VFQFPNPSTEP)
      (libsource (lib stmbl) (part POWERSTEP01))
      (sheetpath (names /stepper/) (tstamps /59F49F2C/))
      (tstamp 59F49F89))
    (comp (ref R1)
      (value R)
      (footprint stmbl:R_2512)
      (libsource (lib device) (part R))
      (sheetpath (names /stepper/) (tstamps /59F49F2C/))
      (tstamp 59F4A079))
    (comp (ref R2)
      (value R)
      (footprint stmbl:R_2512)
      (libsource (lib device) (part R))
      (sheetpath (names /stepper/) (tstamps /59F49F2C/))
      (tstamp 59F4A11F))
    (comp (ref D1)
      (value D)
      (footprint stmbl:SMA_Standard)
      (libsource (lib device) (part D))
      (sheetpath (names /stepper/) (tstamps /59F49F2C/))
      (tstamp 59F4A23F))
    (comp (ref D2)
      (value D)
      (footprint stmbl:SMA_Standard)
      (libsource (lib device) (part D))
      (sheetpath (names /stepper/) (tstamps /59F49F2C/))
      (tstamp 59F4A2D7))
    (comp (ref C4)
      (value C)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /stepper/) (tstamps /59F49F2C/))
      (tstamp 59F4A42C))
    (comp (ref C3)
      (value C)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /stepper/) (tstamps /59F49F2C/))
      (tstamp 59F4A539))
    (comp (ref C5)
      (value C)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /stepper/) (tstamps /59F49F2C/))
      (tstamp 59F4A5C9))
    (comp (ref R4)
      (value R)
      (footprint stmbl:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /stepper/) (tstamps /59F49F2C/))
      (tstamp 59F4A831))
    (comp (ref R3)
      (value R)
      (footprint stmbl:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /stepper/) (tstamps /59F49F2C/))
      (tstamp 59F4A876))
    (comp (ref J1)
      (value CONN_01X04)
      (footprint stmbl:CONN_1x04_2.54)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /stepper/) (tstamps /59F49F2C/))
      (tstamp 59F4B2B2))
    (comp (ref C6)
      (value C)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /stepper/) (tstamps /59F49F2C/))
      (tstamp 59F4B6B3))
    (comp (ref C2)
      (value C)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /stepper/) (tstamps /59F49F2C/))
      (tstamp 59F4BB09))
    (comp (ref C1)
      (value C)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /stepper/) (tstamps /59F49F2C/))
      (tstamp 59F4BB44))
    (comp (ref U2)
      (value POWERSTEP01)
      (footprint stmbl:VFQFPNPSTEP)
      (libsource (lib stmbl) (part POWERSTEP01))
      (sheetpath (names /stepper2/) (tstamps /59F4C6C6/))
      (tstamp 59F49F89))
    (comp (ref R5)
      (value R)
      (footprint stmbl:R_2512)
      (libsource (lib device) (part R))
      (sheetpath (names /stepper2/) (tstamps /59F4C6C6/))
      (tstamp 59F4A079))
    (comp (ref R6)
      (value R)
      (footprint stmbl:R_2512)
      (libsource (lib device) (part R))
      (sheetpath (names /stepper2/) (tstamps /59F4C6C6/))
      (tstamp 59F4A11F))
    (comp (ref D3)
      (value D)
      (footprint stmbl:SMA_Standard)
      (libsource (lib device) (part D))
      (sheetpath (names /stepper2/) (tstamps /59F4C6C6/))
      (tstamp 59F4A23F))
    (comp (ref D4)
      (value D)
      (footprint stmbl:SMA_Standard)
      (libsource (lib device) (part D))
      (sheetpath (names /stepper2/) (tstamps /59F4C6C6/))
      (tstamp 59F4A2D7))
    (comp (ref C10)
      (value C)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /stepper2/) (tstamps /59F4C6C6/))
      (tstamp 59F4A42C))
    (comp (ref C9)
      (value C)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /stepper2/) (tstamps /59F4C6C6/))
      (tstamp 59F4A539))
    (comp (ref C11)
      (value C)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /stepper2/) (tstamps /59F4C6C6/))
      (tstamp 59F4A5C9))
    (comp (ref R8)
      (value R)
      (footprint stmbl:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /stepper2/) (tstamps /59F4C6C6/))
      (tstamp 59F4A831))
    (comp (ref R7)
      (value R)
      (footprint stmbl:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /stepper2/) (tstamps /59F4C6C6/))
      (tstamp 59F4A876))
    (comp (ref J2)
      (value CONN_01X04)
      (footprint stmbl:CONN_1x04_2.54)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /stepper2/) (tstamps /59F4C6C6/))
      (tstamp 59F4B2B2))
    (comp (ref C12)
      (value C)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /stepper2/) (tstamps /59F4C6C6/))
      (tstamp 59F4B6B3))
    (comp (ref C8)
      (value C)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /stepper2/) (tstamps /59F4C6C6/))
      (tstamp 59F4BB09))
    (comp (ref C7)
      (value C)
      (footprint stmbl:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /stepper2/) (tstamps /59F4C6C6/))
      (tstamp 59F4BB44)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X04)
      (description "Connector, single row, 01x04, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib device) (part D)
      (description Diode)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib stmbl) (part POWERSTEP01)
      (fields
        (field (name Reference) U)
        (field (name Value) POWERSTEP01))
      (pins
        (pin (num 1) (name VS) (type input))
        (pin (num 7) (name OUTB2) (type input))
        (pin (num 8) (name GND) (type input))
        (pin (num 9) (name SENSEB_S) (type input))
        (pin (num 10) (name ~CS) (type input))
        (pin (num 11) (name CK) (type input))
        (pin (num 12) (name SDI) (type input))
        (pin (num 13) (name VDDIO) (type input))
        (pin (num 14) (name SDO) (type input))
        (pin (num 15) (name ~BUSY) (type input))
        (pin (num 16) (name ~FLAG) (type input))
        (pin (num 17) (name STCK) (type input))
        (pin (num 18) (name SW) (type input))
        (pin (num 19) (name ~STBY/RESET) (type input))
        (pin (num 20) (name SENSEA_S) (type input))
        (pin (num 22) (name OUTA2) (type input))
        (pin (num 34) (name SENSEA_P) (type input))
        (pin (num 38) (name OUTA1) (type input))
        (pin (num 54) (name ADCIN) (type input))
        (pin (num 56) (name VBOOT) (type input))
        (pin (num 57) (name CP) (type input))
        (pin (num 58) (name VCC) (type input))
        (pin (num 60) (name VCCREG) (type input))
        (pin (num 61) (name VSREG) (type input))
        (pin (num 62) (name VREG) (type input))
        (pin (num 63) (name OSCIN) (type input))
        (pin (num 64) (name OSCOUT) (type input))
        (pin (num 65) (name OUTB1) (type input))
        (pin (num 77) (name SENSEB_P) (type input))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical device)
      (uri "/Library/Application Support/kicad/library/device.lib"))
    (library (logical conn)
      (uri "/Library/Application Support/kicad/library/conn.lib"))
    (library (logical stmbl)
      (uri /Users/rene/dev/stmbl/hw/kicad/lib/stmbl.lib)))
  (nets
    (net (code 1) (name /stepper/~CS)
      (node (ref U1) (pin 10))
      (node (ref U2) (pin 10)))
    (net (code 2) (name /stepper/CK)
      (node (ref U2) (pin 11))
      (node (ref U1) (pin 11)))
    (net (code 3) (name /stepper2/SDI)
      (node (ref U2) (pin 12))
      (node (ref U1) (pin 14)))
    (net (code 4) (name /stepper/SDI)
      (node (ref U1) (pin 12)))
    (net (code 5) (name /stepper/~STBY)
      (node (ref U2) (pin 19))
      (node (ref U1) (pin 19)))
    (net (code 6) (name /stepper2/SDO)
      (node (ref U2) (pin 14)))
    (net (code 7) (name "Net-(R1-Pad1)")
      (node (ref U1) (pin 20))
      (node (ref R1) (pin 1))
      (node (ref U1) (pin 34)))
    (net (code 8) (name "Net-(C3-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref R3) (pin 1))
      (node (ref C6) (pin 2))
      (node (ref U1) (pin 1))
      (node (ref U1) (pin 61)))
    (net (code 9) (name "Net-(C1-Pad2)")
      (node (ref U1) (pin 62))
      (node (ref U1) (pin 13))
      (node (ref C1) (pin 2)))
    (net (code 10) (name "Net-(U1-Pad63)")
      (node (ref U1) (pin 63)))
    (net (code 11) (name "Net-(R3-Pad2)")
      (node (ref U1) (pin 54))
      (node (ref R4) (pin 1))
      (node (ref R3) (pin 2)))
    (net (code 12) (name "Net-(U1-Pad64)")
      (node (ref U1) (pin 64)))
    (net (code 13) (name "Net-(U1-Pad15)")
      (node (ref U1) (pin 15)))
    (net (code 14) (name "Net-(U1-Pad16)")
      (node (ref U1) (pin 16)))
    (net (code 15) (name "Net-(U1-Pad17)")
      (node (ref U1) (pin 17)))
    (net (code 16) (name "Net-(U1-Pad18)")
      (node (ref U1) (pin 18)))
    (net (code 17) (name "Net-(J1-Pad1)")
      (node (ref U1) (pin 38))
      (node (ref J1) (pin 1)))
    (net (code 18) (name GND)
      (node (ref R8) (pin 2))
      (node (ref C12) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref R4) (pin 2))
      (node (ref C5) (pin 1))
      (node (ref U1) (pin 8))
      (node (ref C1) (pin 1))
      (node (ref R6) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref C2) (pin 1))
      (node (ref R2) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref U2) (pin 8)))
    (net (code 19) (name "Net-(C3-Pad1)")
      (node (ref D2) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref U1) (pin 56)))
    (net (code 20) (name "Net-(C4-Pad2)")
      (node (ref U1) (pin 57))
      (node (ref C4) (pin 2)))
    (net (code 21) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2))
      (node (ref U1) (pin 22)))
    (net (code 22) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3))
      (node (ref U1) (pin 65)))
    (net (code 23) (name "Net-(J1-Pad4)")
      (node (ref U1) (pin 7))
      (node (ref J1) (pin 4)))
    (net (code 24) (name "Net-(C4-Pad1)")
      (node (ref D1) (pin 1))
      (node (ref D2) (pin 2))
      (node (ref C4) (pin 1)))
    (net (code 25) (name "Net-(R2-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref U1) (pin 9))
      (node (ref U1) (pin 77)))
    (net (code 26) (name "Net-(C2-Pad2)")
      (node (ref C2) (pin 2))
      (node (ref U1) (pin 60))
      (node (ref U1) (pin 58)))
    (net (code 27) (name "Net-(R5-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref U2) (pin 20))
      (node (ref U2) (pin 34)))
    (net (code 28) (name "Net-(C11-Pad2)")
      (node (ref U2) (pin 61))
      (node (ref R7) (pin 1))
      (node (ref U2) (pin 1))
      (node (ref C11) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref D3) (pin 2)))
    (net (code 29) (name "Net-(C7-Pad2)")
      (node (ref C7) (pin 2))
      (node (ref U2) (pin 13))
      (node (ref U2) (pin 62)))
    (net (code 30) (name "Net-(U2-Pad63)")
      (node (ref U2) (pin 63)))
    (net (code 31) (name "Net-(R7-Pad2)")
      (node (ref U2) (pin 54))
      (node (ref R7) (pin 2))
      (node (ref R8) (pin 1)))
    (net (code 32) (name "Net-(U2-Pad64)")
      (node (ref U2) (pin 64)))
    (net (code 33) (name "Net-(U2-Pad15)")
      (node (ref U2) (pin 15)))
    (net (code 34) (name "Net-(U2-Pad16)")
      (node (ref U2) (pin 16)))
    (net (code 35) (name "Net-(U2-Pad17)")
      (node (ref U2) (pin 17)))
    (net (code 36) (name "Net-(U2-Pad18)")
      (node (ref U2) (pin 18)))
    (net (code 37) (name "Net-(J2-Pad1)")
      (node (ref U2) (pin 38))
      (node (ref J2) (pin 1)))
    (net (code 38) (name "Net-(C9-Pad1)")
      (node (ref U2) (pin 56))
      (node (ref C9) (pin 1))
      (node (ref D4) (pin 1)))
    (net (code 39) (name "Net-(C10-Pad2)")
      (node (ref U2) (pin 57))
      (node (ref C10) (pin 2)))
    (net (code 40) (name "Net-(J2-Pad2)")
      (node (ref J2) (pin 2))
      (node (ref U2) (pin 22)))
    (net (code 41) (name "Net-(J2-Pad3)")
      (node (ref J2) (pin 3))
      (node (ref U2) (pin 65)))
    (net (code 42) (name "Net-(J2-Pad4)")
      (node (ref U2) (pin 7))
      (node (ref J2) (pin 4)))
    (net (code 43) (name "Net-(C10-Pad1)")
      (node (ref D3) (pin 1))
      (node (ref D4) (pin 2))
      (node (ref C10) (pin 1)))
    (net (code 44) (name "Net-(R6-Pad1)")
      (node (ref U2) (pin 9))
      (node (ref U2) (pin 77))
      (node (ref R6) (pin 1)))
    (net (code 45) (name "Net-(C8-Pad2)")
      (node (ref U2) (pin 58))
      (node (ref C8) (pin 2))
      (node (ref U2) (pin 60)))))