(export (version D)
  (design
    (source /home/stefan/Dokumente/Development/Basteln/stmbl/hw/kicad/11ua/11ua.sch)
    (date "Fri 22 Feb 2019 03:25:37 PM CET")
    (tool "Eeschema (5.1.0-rc1-120-gc4fe6785a)")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "11µA to differential adapter with index")
        (company)
        (rev B)
        (date)
        (source 11ua.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value RJ45)
      (footprint Connect:RJ45_8)
      (libsource (lib 11ua-rescue) (part RJ45) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E009D))
    (comp (ref J2)
      (value RJ45)
      (footprint Connect:RJ45_8)
      (libsource (lib 11ua-rescue) (part RJ45) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E00E5))
    (comp (ref R4)
      (value 100k)
      (footprint stmbl:R_0603)
      (libsource (lib 11ua-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E0847))
    (comp (ref R3)
      (value 100k)
      (footprint stmbl:R_0603)
      (libsource (lib 11ua-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E08D0))
    (comp (ref C4)
      (value 27p)
      (footprint stmbl:C_0603)
      (libsource (lib 11ua-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E0942))
    (comp (ref C3)
      (value 27p)
      (footprint stmbl:C_0603)
      (libsource (lib 11ua-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E0986))
    (comp (ref R1)
      (value 100k)
      (footprint stmbl:R_0603)
      (libsource (lib 11ua-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E0C0B))
    (comp (ref C1)
      (value 27p)
      (footprint stmbl:C_0603)
      (libsource (lib 11ua-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E0C46))
    (comp (ref R2)
      (value 100k)
      (footprint stmbl:R_0603)
      (libsource (lib 11ua-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E0DC4))
    (comp (ref C2)
      (value 27p)
      (footprint stmbl:C_0603)
      (libsource (lib 11ua-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E0E05))
    (comp (ref R5)
      (value 120)
      (footprint stmbl:R_0603)
      (libsource (lib 11ua-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E1018))
    (comp (ref R6)
      (value 120)
      (footprint stmbl:R_0603)
      (libsource (lib 11ua-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E1061))
    (comp (ref C5)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib 11ua-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E10E2))
    (comp (ref R7)
      (value 120)
      (footprint stmbl:R_0603)
      (libsource (lib 11ua-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E1BC6))
    (comp (ref R8)
      (value 120)
      (footprint stmbl:R_0603)
      (libsource (lib 11ua-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E1BCC))
    (comp (ref C6)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib 11ua-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E1BDE))
    (comp (ref R10)
      (value 100k)
      (footprint stmbl:R_0603)
      (libsource (lib 11ua-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C724DB4))
    (comp (ref C7)
      (value 27p)
      (footprint stmbl:C_0603)
      (libsource (lib 11ua-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C724DBA))
    (comp (ref R9)
      (value 100k)
      (footprint stmbl:R_0603)
      (libsource (lib 11ua-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C724DC0))
    (comp (ref C8)
      (value 27p)
      (footprint stmbl:C_0603)
      (libsource (lib 11ua-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C724DC6))
    (comp (ref R11)
      (value 120)
      (footprint stmbl:R_0603)
      (libsource (lib 11ua-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C731BAD))
    (comp (ref R12)
      (value 120)
      (footprint stmbl:R_0603)
      (libsource (lib 11ua-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C731BB3))
    (comp (ref C9)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib 11ua-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C731BC5))
    (comp (ref J4)
      (value CONN_01X04)
      (footprint stmbl:RM3.81_1x4_UP)
      (libsource (lib stmbl) (part CONN_01X04) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C702B75))
    (comp (ref J3)
      (value CONN_01X04)
      (footprint stmbl:RM3.81_1x4_UP)
      (libsource (lib stmbl) (part CONN_01X04) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C702C41))
    (comp (ref U1)
      (value LM339)
      (footprint Package_SO:SOIC-14_3.9x8.7mm_P1.27mm)
      (datasheet http://www.ti.com/lit/ds/symlink/lm339.pdf)
      (libsource (lib Comparator) (part LM339) (description "Quad Differential Comparators, DIP-14/SOIC-14/SSOP-14"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C70CB52))
    (comp (ref C10)
      (value C)
      (footprint stmbl:C_0603)
      (libsource (lib 11ua-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C74F384))
    (comp (ref C11)
      (value C)
      (footprint stmbl:C_0603)
      (libsource (lib 11ua-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C74FF0F))
    (comp (ref C12)
      (value C)
      (footprint stmbl:C_0603)
      (libsource (lib 11ua-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7501E4))
    (comp (ref C13)
      (value CP)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-2012-15_AVX-P)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C750A44))
    (comp (ref C14)
      (value CP)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-2012-15_AVX-P)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C750E54)))
  (libparts
    (libpart (lib 11ua-rescue) (part C)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib 11ua-rescue) (part R)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib 11ua-rescue) (part RJ45)
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name SHIELD) (type passive))))
    (libpart (lib Comparator) (part LM2901)
      (aliases
        (alias LM339)
        (alias LMV339))
      (description "Quad Differential Comparators, DIP-14/SOIC-14/SSOP-14")
      (docs http://www.ti.com/lit/ds/symlink/lm339.pdf)
      (footprints
        (fp SOIC*3.9x8.7mm*P1.27mm*)
        (fp DIP*W7.62mm*)
        (fp TSSOP*4.4x5mm*P0.65mm*)
        (fp SSOP*5.3x6.2mm*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM2901))
      (pins
        (pin (num 1) (name ~) (type openCol))
        (pin (num 2) (name ~) (type openCol))
        (pin (num 3) (name V+) (type power_in))
        (pin (num 4) (name -) (type input))
        (pin (num 5) (name +) (type input))
        (pin (num 6) (name -) (type input))
        (pin (num 7) (name +) (type input))
        (pin (num 8) (name -) (type input))
        (pin (num 9) (name +) (type input))
        (pin (num 10) (name -) (type input))
        (pin (num 11) (name +) (type input))
        (pin (num 12) (name V-) (type power_in))
        (pin (num 13) (name ~) (type openCol))
        (pin (num 14) (name ~) (type openCol))))
    (libpart (lib Device) (part CP)
      (description "Polarised capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib stmbl) (part CONN_01X04)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive)))))
  (libraries
    (library (logical 11ua-rescue)
      (uri /home/stefan/Dokumente/Development/Basteln/stmbl/hw/kicad/11ua/11ua-rescue.lib))
    (library (logical Comparator)
      (uri /usr/share/kicad/library/Comparator.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical stmbl)
      (uri /home/stefan/Dokumente/Development/Basteln/stmbl-kicad-lib/stmbl.lib)))
  (nets
    (net (code 1) (name "Net-(C8-Pad1)")
      (node (ref R9) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref J2) (pin 4))
      (node (ref R11) (pin 1))
      (node (ref R12) (pin 2))
      (node (ref C9) (pin 2)))
    (net (code 2) (name +5V)
      (node (ref C11) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref R7) (pin 2))
      (node (ref C14) (pin 1))
      (node (ref J1) (pin 7))
      (node (ref J2) (pin 7))
      (node (ref R5) (pin 2))
      (node (ref U1) (pin 3))
      (node (ref C10) (pin 1))
      (node (ref R11) (pin 2))
      (node (ref J4) (pin 3)))
    (net (code 3) (name GND)
      (node (ref U1) (pin 8))
      (node (ref U1) (pin 12))
      (node (ref U1) (pin 9))
      (node (ref C5) (pin 1))
      (node (ref J4) (pin 4))
      (node (ref R8) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref R12) (pin 1))
      (node (ref J1) (pin 8))
      (node (ref J2) (pin 8))
      (node (ref R6) (pin 1))
      (node (ref C10) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref C14) (pin 2)))
    (net (code 4) (name "Net-(C8-Pad2)")
      (node (ref C8) (pin 2))
      (node (ref J3) (pin 4))
      (node (ref R9) (pin 2))
      (node (ref U1) (pin 7))
      (node (ref J1) (pin 4)))
    (net (code 5) (name "Net-(C7-Pad1)")
      (node (ref C7) (pin 1))
      (node (ref J2) (pin 5))
      (node (ref R10) (pin 1))
      (node (ref U1) (pin 1)))
    (net (code 6) (name "Net-(C7-Pad2)")
      (node (ref J1) (pin 5))
      (node (ref R10) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref J4) (pin 1))
      (node (ref U1) (pin 6)))
    (net (code 7) (name "Net-(U1-Pad14)")
      (node (ref U1) (pin 14)))
    (net (code 8) (name "Net-(C3-Pad2)")
      (node (ref U1) (pin 4))
      (node (ref R4) (pin 2))
      (node (ref J3) (pin 3))
      (node (ref J1) (pin 3))
      (node (ref C3) (pin 2)))
    (net (code 9) (name "Net-(C4-Pad2)")
      (node (ref R3) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref U1) (pin 10))
      (node (ref J3) (pin 1))
      (node (ref J1) (pin 1)))
    (net (code 10) (name "Net-(C1-Pad1)")
      (node (ref R1) (pin 1))
      (node (ref J2) (pin 2))
      (node (ref R5) (pin 1))
      (node (ref R6) (pin 2))
      (node (ref C1) (pin 1))
      (node (ref C5) (pin 2)))
    (net (code 11) (name "Net-(C3-Pad1)")
      (node (ref U1) (pin 2))
      (node (ref J2) (pin 3))
      (node (ref R4) (pin 1))
      (node (ref C3) (pin 1)))
    (net (code 12) (name "Net-(C4-Pad1)")
      (node (ref C4) (pin 1))
      (node (ref U1) (pin 13))
      (node (ref R3) (pin 1))
      (node (ref J2) (pin 1)))
    (net (code 13) (name "Net-(C2-Pad2)")
      (node (ref J1) (pin 6))
      (node (ref C2) (pin 2))
      (node (ref U1) (pin 5))
      (node (ref J4) (pin 2))
      (node (ref R2) (pin 2)))
    (net (code 14) (name "Net-(C1-Pad2)")
      (node (ref C1) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref U1) (pin 11))
      (node (ref J1) (pin 2))
      (node (ref J3) (pin 2)))
    (net (code 15) (name GNDA)
      (node (ref J1) (pin 9))
      (node (ref J2) (pin 9)))
    (net (code 16) (name "Net-(C2-Pad1)")
      (node (ref R8) (pin 2))
      (node (ref R7) (pin 1))
      (node (ref J2) (pin 6))
      (node (ref C6) (pin 2))
      (node (ref C2) (pin 1))
      (node (ref R2) (pin 1)))))