(export (version D)
  (design
    (source /Users/crinq/Documents/sandbox/stmbl/hw/kicad/stmsp/stmsp.sch)
    (date "2017 July 27, Thursday 14:53:52")
    (tool "Eeschema (2017-04-07 revision 70c961f)-master")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source stmsp.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /drv/) (tstamps /5918AB0C/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source drv.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /supply/) (tstamps /5918AB94/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source supply.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /sensor/) (tstamps /5918AD6D/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source sensor.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /cmd/) (tstamps /5918ADEA/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source cmd.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 6) (name /f3/) (tstamps /5915CECC/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source f303.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 7) (name /in0/) (tstamps /594079D4/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source in.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 8) (name /out0/) (tstamps /5940CCE8/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source out.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 9) (name /in1/) (tstamps /5940FC3C/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source in.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 10) (name /out1/) (tstamps /59418122/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source out.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref P5)
      (value CONN_01X06)
      (footprint stmbl:Pin_Header_Straight_1x06)
      (libsource (lib stmbl) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 593F9343))
    (comp (ref J1)
      (value CONN_02X05)
      (footprint stmbl:Pin_Header_Straight_2x05)
      (libsource (lib conn) (part CONN_02X05))
      (sheetpath (names /) (tstamps /))
      (tstamp 5943C634))
    (comp (ref P2)
      (value CONN_01X04)
      (footprint stmbl:Pin_Header_Straight_1x04)
      (libsource (lib stmbl) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 594404FD))
    (comp (ref C15)
      (value 220n)
      (footprint stmbl:C_0805)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5918DE6E))
    (comp (ref C14)
      (value 220n)
      (footprint stmbl:C_0805)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5918DE99))
    (comp (ref C12)
      (value 220n)
      (footprint stmbl:C_0805)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5918DEB2))
    (comp (ref R12)
      (value 0.02)
      (footprint stmbl:R_0805)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5918E2CF))
    (comp (ref R8)
      (value 0.02)
      (footprint stmbl:R_0805)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5918E363))
    (comp (ref R19)
      (value 10k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5918F0F4))
    (comp (ref R20)
      (value 1k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5918F156))
    (comp (ref C18)
      (value 18p)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5918F1B7))
    (comp (ref R18)
      (value 10k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5918FC7B))
    (comp (ref R23)
      (value 10k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5918FEA4))
    (comp (ref R24)
      (value 1k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5918FEAA))
    (comp (ref C19)
      (value 18p)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5918FEB0))
    (comp (ref R22)
      (value 10k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5918FECC))
    (comp (ref R16)
      (value 10k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 591903B9))
    (comp (ref R17)
      (value 1k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 591903C0))
    (comp (ref C16)
      (value 18p)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 591903C7))
    (comp (ref R15)
      (value 10k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 591903E4))
    (comp (ref R14)
      (value 10k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5919412F))
    (comp (ref R13)
      (value 10k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5919419E))
    (comp (ref R7)
      (value 1k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 59194A21))
    (comp (ref R6)
      (value 1k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 59194A90))
    (comp (ref P3)
      (value CONN_01X04)
      (footprint stmbl:Pin_Header_Straight_1x04_dual)
      (libsource (lib stmbl) (part CONN_01X04))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 59197AB1))
    (comp (ref C20)
      (value 220n)
      (footprint stmbl:C_0805)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 591994D2))
    (comp (ref P4)
      (value CONN_01X02)
      (footprint stmbl:akl182-2)
      (libsource (lib stmbl) (part CONN_01X02))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 59239420))
    (comp (ref U2)
      (value L6206Q)
      (footprint stmbl:VFQFPN48)
      (libsource (lib stmbl) (part L6206Q))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5923F2B9))
    (comp (ref R51)
      (value 120)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5924BE0E))
    (comp (ref R50)
      (value 120)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5924C018))
    (comp (ref R49)
      (value 120)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5924C06E))
    (comp (ref R46)
      (value 3.9k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5924C587))
    (comp (ref R47)
      (value 3.9k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5924C73F))
    (comp (ref R48)
      (value 3.9k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5924C78E))
    (comp (ref C6)
      (value 18p)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5924D3B2))
    (comp (ref C34)
      (value 18p)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5924D426))
    (comp (ref C35)
      (value 18p)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 5924D478))
    (comp (ref TH1)
      (value 4.7k)
      (footprint stmbl:R_0603)
      (libsource (lib device) (part Thermistor_NTC))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 59271C6A))
    (comp (ref C30)
      (value 10n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 593B1682))
    (comp (ref R56)
      (value 100)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 593B170F))
    (comp (ref D10)
      (value 1N4148)
      (footprint stmbl:SOD-123)
      (libsource (lib stmbl) (part D))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 593B19D3))
    (comp (ref C5)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 593B1B2E))
    (comp (ref D11)
      (value 1N4148)
      (footprint stmbl:SOD-123)
      (libsource (lib stmbl) (part D))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 593B1BE8))
    (comp (ref R55)
      (value 1k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 593B4A59))
    (comp (ref C33)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 59455941))
    (comp (ref C26)
      (value 22u)
      (footprint stmbl:c_elec_5x5.3)
      (libsource (lib stmbl) (part CP))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 59457B45))
    (comp (ref P6)
      (value CONN_01X02)
      (footprint stmbl:akl183-2)
      (libsource (lib stmbl) (part CONN_01X02))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 593C4D39))
    (comp (ref C39)
      (value 1n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 593CC856))
    (comp (ref C38)
      (value 1n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /drv/) (tstamps /5918AB0C/))
      (tstamp 593CC99F))
    (comp (ref U5)
      (value MCP16331)
      (footprint stmbl:SOT-23-6)
      (libsource (lib stmbl) (part MCP16331))
      (sheetpath (names /supply/) (tstamps /5918AB94/))
      (tstamp 5918AC00))
    (comp (ref L3)
      (value "22µ 650mA")
      (footprint stmbl:SMD_INDUCTOR_32x25)
      (libsource (lib stmbl) (part INDUCTOR))
      (sheetpath (names /supply/) (tstamps /5918AB94/))
      (tstamp 5918C529))
    (comp (ref C23)
      (value 2.2u)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /supply/) (tstamps /5918AB94/))
      (tstamp 5918DD3D))
    (comp (ref C25)
      (value 2.2u)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /supply/) (tstamps /5918AB94/))
      (tstamp 5918DD80))
    (comp (ref C24)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /supply/) (tstamps /5918AB94/))
      (tstamp 5918DDD5))
    (comp (ref C22)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /supply/) (tstamps /5918AB94/))
      (tstamp 5918DE05))
    (comp (ref D1)
      (value ss110)
      (footprint stmbl:SMA_Standard)
      (libsource (lib stmbl) (part D))
      (sheetpath (names /supply/) (tstamps /5918AB94/))
      (tstamp 59234466))
    (comp (ref R25)
      (value 51k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /supply/) (tstamps /5918AB94/))
      (tstamp 59234687))
    (comp (ref R26)
      (value 10k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /supply/) (tstamps /5918AB94/))
      (tstamp 592346BA))
    (comp (ref D2)
      (value 1N4148)
      (footprint stmbl:SOD-123)
      (libsource (lib stmbl) (part D))
      (sheetpath (names /supply/) (tstamps /5918AB94/))
      (tstamp 5923480D))
    (comp (ref C21)
      (value 10u)
      (footprint stmbl:C_0805)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /supply/) (tstamps /5918AB94/))
      (tstamp 592353E2))
    (comp (ref C28)
      (value 10u)
      (footprint stmbl:C_0805)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /supply/) (tstamps /5918AB94/))
      (tstamp 5923540F))
    (comp (ref U6)
      (value MIC5504-3.3YM5)
      (footprint stmbl:SOT-23-5)
      (libsource (lib stmbl) (part MIC55))
      (sheetpath (names /supply/) (tstamps /5918AB94/))
      (tstamp 59444047))
    (comp (ref D12)
      (value Led_Small)
      (footprint stmbl:LED-0805-SIDE)
      (libsource (lib stmbl) (part Led_Small))
      (sheetpath (names /supply/) (tstamps /5918AB94/))
      (tstamp 5944CEE5))
    (comp (ref R1)
      (value 470)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /supply/) (tstamps /5918AB94/))
      (tstamp 5944CF59))
    (comp (ref C27)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /sensor/) (tstamps /5918AD6D/))
      (tstamp 5918C487))
    (comp (ref U7)
      (value TLE5012)
      (footprint stmbl:SOIC-8-N)
      (libsource (lib stmbl) (part TLE5012))
      (sheetpath (names /sensor/) (tstamps /5918AD6D/))
      (tstamp 5923BF54))
    (comp (ref JP2)
      (value JUMPER3_NC)
      (footprint stmbl:SOLDER_JUMPER_3_NC)
      (libsource (lib stmbl) (part JUMPER3_NC))
      (sheetpath (names /sensor/) (tstamps /5918AD6D/))
      (tstamp 5923C12B))
    (comp (ref U10)
      (value TLE5012)
      (footprint stmbl:SOIC-8-N)
      (libsource (lib stmbl) (part TLE5012))
      (sheetpath (names /sensor/) (tstamps /5918AD6D/))
      (tstamp 5945AC83))
    (comp (ref U8)
      (value SN65176B)
      (footprint stmbl:SOIC-8-N)
      (libsource (lib interface) (part SP3485EN))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 565DD0E7))
    (comp (ref R10)
      (value 1k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 565DD7F2))
    (comp (ref C13)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 565DD843))
    (comp (ref R9)
      (value 10k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 56F9D4F8))
    (comp (ref R11)
      (value 10k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 56F9D5CB))
    (comp (ref R21)
      (value 1k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 57758B35))
    (comp (ref L2)
      (value "220r 700mA")
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part INDUCTOR))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 57AD7F96))
    (comp (ref C17)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 57AD80BE))
    (comp (ref U9)
      (value SN65176B)
      (footprint stmbl:SOIC-8-N)
      (libsource (lib interface) (part SP3485EN))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 59233172))
    (comp (ref R28)
      (value 1k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 59233178))
    (comp (ref C29)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 5923317E))
    (comp (ref R27)
      (value 10k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 5923318C))
    (comp (ref R29)
      (value 10k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 59233192))
    (comp (ref R30)
      (value 1k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 59233357))
    (comp (ref R33)
      (value 1k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 59447745))
    (comp (ref R38)
      (value 1k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 59447977))
    (comp (ref R41)
      (value 1k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 59447BF9))
    (comp (ref R42)
      (value 1k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /cmd/) (tstamps /5918ADEA/))
      (tstamp 59447C01))
    (comp (ref C7)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 5663136E))
    (comp (ref C8)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 56631543))
    (comp (ref C9)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 5663155A))
    (comp (ref C10)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 56631574))
    (comp (ref Y1)
      (value 8M)
      (footprint stmbl:Crystal_SMD_0503_4Pads)
      (libsource (lib stmbl) (part Crystal))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 56631593))
    (comp (ref C2)
      (value 18p)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 56631605))
    (comp (ref C3)
      (value 18p)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 566316C7))
    (comp (ref C1)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 566317E6))
    (comp (ref C4)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 56631C3B))
    (comp (ref L1)
      (value "220r 700mA")
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part INDUCTOR))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 57B2E566))
    (comp (ref C11)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 57B2E6B6))
    (comp (ref P1)
      (value USB_OTG)
      (footprint stmbl:USB_Micro-B)
      (libsource (lib stmbl) (part USB_OTG))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 582597E3))
    (comp (ref R4)
      (value 22)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 5825AC16))
    (comp (ref R5)
      (value 22)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 5825B725))
    (comp (ref R3)
      (value 1.5k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 5825B8D4))
    (comp (ref R2)
      (value 1k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 582CAB11))
    (comp (ref U3)
      (value STM32F303CBTx)
      (footprint stmbl:LQFP-48_7x7mm_Pitch0.5mm)
      (libsource (lib stmbl) (part STM32F303CBTx))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 592409F6))
    (comp (ref D7)
      (value Led_Small)
      (footprint stmbl:LED-0805-SIDE)
      (libsource (lib stmbl) (part Led_Small))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 5924E0F3))
    (comp (ref D8)
      (value Led_Small)
      (footprint stmbl:LED-0805-SIDE)
      (libsource (lib stmbl) (part Led_Small))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 5924E137))
    (comp (ref D9)
      (value Led_Small)
      (footprint stmbl:LED-0805-SIDE)
      (libsource (lib stmbl) (part Led_Small))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 5924E175))
    (comp (ref R52)
      (value 470)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 5924E259))
    (comp (ref R53)
      (value 470)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 5924E4AD))
    (comp (ref R54)
      (value 470)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 5924E4EF))
    (comp (ref U1)
      (value USBLC6-4SC6)
      (footprint stmbl:SOT-23-6)
      (fields
        (field (name Description) "TRANSIENT VOLTAGE SUPPRESSOR"))
      (libsource (lib stmbl) (part USBLC6-4SC6))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 59258712))
    (comp (ref C36)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 5925871B))
    (comp (ref U4)
      (value USBLC6-4SC6)
      (footprint stmbl:SOT-23-6)
      (fields
        (field (name Description) "TRANSIENT VOLTAGE SUPPRESSOR"))
      (libsource (lib stmbl) (part USBLC6-4SC6))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 59258743))
    (comp (ref C37)
      (value 100n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 5925874C))
    (comp (ref T3)
      (value testpoint)
      (footprint stmbl:Measurement_Point_Round-SMD-Pad_Small)
      (libsource (lib stmbl) (part testpoint))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 5925B771))
    (comp (ref T2)
      (value testpoint)
      (footprint stmbl:Measurement_Point_Round-SMD-Pad_Small)
      (libsource (lib stmbl) (part testpoint))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 5925CEA4))
    (comp (ref T1)
      (value testpoint)
      (footprint stmbl:Measurement_Point_Round-SMD-Pad_Small)
      (libsource (lib stmbl) (part testpoint))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 5925D4E4))
    (comp (ref R43)
      (value 470)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /f3/) (tstamps /5915CECC/))
      (tstamp 59489CB0))
    (comp (ref R31)
      (value 10k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /in0/) (tstamps /594079D4/))
      (tstamp 59409106))
    (comp (ref R32)
      (value 1.5k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /in0/) (tstamps /594079D4/))
      (tstamp 5940910D))
    (comp (ref C31)
      (value 1n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /in0/) (tstamps /594079D4/))
      (tstamp 5940911B))
    (comp (ref R34)
      (value 1k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /out0/) (tstamps /5940CCE8/))
      (tstamp 5940D06F))
    (comp (ref R35)
      (value 120)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /out0/) (tstamps /5940CCE8/))
      (tstamp 5940D076))
    (comp (ref Q1)
      (value Q_NJFET_GSD)
      (footprint stmbl:SOT-23)
      (libsource (lib device) (part Q_NJFET_GSD))
      (sheetpath (names /out0/) (tstamps /5940CCE8/))
      (tstamp 5940D07D))
    (comp (ref D4)
      (value "200V 1A")
      (footprint stmbl:SOD-123)
      (libsource (lib stmbl) (part D))
      (sheetpath (names /out0/) (tstamps /5940CCE8/))
      (tstamp 5940D084))
    (comp (ref R36)
      (value 10k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /in1/) (tstamps /5940FC3C/))
      (tstamp 59409106))
    (comp (ref R37)
      (value 1.5k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /in1/) (tstamps /5940FC3C/))
      (tstamp 5940910D))
    (comp (ref C32)
      (value 1n)
      (footprint stmbl:C_0603)
      (libsource (lib stmbl) (part C))
      (sheetpath (names /in1/) (tstamps /5940FC3C/))
      (tstamp 5940911B))
    (comp (ref R39)
      (value 1k)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /out1/) (tstamps /59418122/))
      (tstamp 5940D06F))
    (comp (ref R40)
      (value 120)
      (footprint stmbl:R_0603)
      (libsource (lib stmbl) (part R))
      (sheetpath (names /out1/) (tstamps /59418122/))
      (tstamp 5940D076))
    (comp (ref Q2)
      (value Q_NJFET_GSD)
      (footprint stmbl:SOT-23)
      (libsource (lib device) (part Q_NJFET_GSD))
      (sheetpath (names /out1/) (tstamps /59418122/))
      (tstamp 5940D07D))
    (comp (ref D6)
      (value "200V 1A")
      (footprint stmbl:SOD-123)
      (libsource (lib stmbl) (part D))
      (sheetpath (names /out1/) (tstamps /59418122/))
      (tstamp 5940D084)))
  (libparts
    (libpart (lib stmbl) (part C)
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib stmbl) (part CONN_01X02)
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib stmbl) (part CONN_01X04)
      (footprints
        (fp Pin_Header_Straight_1X04)
        (fp Pin_Header_Angled_1X04)
        (fp Socket_Strip_Straight_1X04)
        (fp Socket_Strip_Angled_1X04))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib stmbl) (part CONN_01X06)
      (footprints
        (fp Pin_Header_Straight_1X06)
        (fp Pin_Header_Angled_1X06)
        (fp Socket_Strip_Straight_1X06)
        (fp Socket_Strip_Angled_1X06))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X06))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib conn) (part CONN_02X05)
      (description "Connector, double row, 02x05, pin header")
      (footprints
        (fp Pin_Header_Straight_2X*)
        (fp Pin_Header_Angled_2X*)
        (fp Socket_Strip_Straight_2X*)
        (fp Socket_Strip_Angled_2X*)
        (fp IDC_Header_Straight_*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_02X05))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))))
    (libpart (lib stmbl) (part CP)
      (footprints
        (fp CP*)
        (fp Elko*)
        (fp TantalC*)
        (fp C*elec)
        (fp c_elec*)
        (fp SMD*_Pol))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib stmbl) (part Crystal)
      (footprints
        (fp Crystal_*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib stmbl) (part D)
      (footprints
        (fp Diode_*)
        (fp D-Pak_TO252AA)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib stmbl) (part INDUCTOR)
      (fields
        (field (name Reference) L)
        (field (name Value) INDUCTOR))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib stmbl) (part JUMPER3_NC)
      (fields
        (field (name Reference) JP)
        (field (name Value) JUMPER3_NC))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib stmbl) (part L6206Q)
      (fields
        (field (name Reference) U)
        (field (name Value) L6206Q))
      (pins
        (pin (num 1) (name ~) (type NotConnected))
        (pin (num 2) (name OUT1A) (type output))
        (pin (num 3) (name OUT1A) (type output))
        (pin (num 4) (name ~) (type NotConnected))
        (pin (num 5) (name ~) (type NotConnected))
        (pin (num 6) (name GND) (type power_in))
        (pin (num 7) (name ~) (type NotConnected))
        (pin (num 8) (name ~) (type NotConnected))
        (pin (num 9) (name ~) (type NotConnected))
        (pin (num 10) (name OUT1B) (type output))
        (pin (num 11) (name OUT1B) (type output))
        (pin (num 12) (name ~) (type NotConnected))
        (pin (num 13) (name OCDB) (type power_in))
        (pin (num 14) (name ~) (type NotConnected))
        (pin (num 15) (name SENSEB) (type power_in))
        (pin (num 16) (name SENSEB) (type power_in))
        (pin (num 17) (name IN1B) (type output))
        (pin (num 18) (name IN2B) (type output))
        (pin (num 19) (name PROGCLB) (type power_in))
        (pin (num 20) (name ENB) (type output))
        (pin (num 21) (name VBOOT) (type power_in))
        (pin (num 22) (name OUT2B) (type output))
        (pin (num 23) (name OUT2B) (type output))
        (pin (num 24) (name ~) (type NotConnected))
        (pin (num 25) (name ~) (type NotConnected))
        (pin (num 26) (name VSB) (type power_in))
        (pin (num 27) (name VSB) (type power_in))
        (pin (num 28) (name ~) (type NotConnected))
        (pin (num 29) (name ~) (type NotConnected))
        (pin (num 30) (name ~) (type NotConnected))
        (pin (num 31) (name GND) (type power_in))
        (pin (num 32) (name ~) (type NotConnected))
        (pin (num 33) (name ~) (type NotConnected))
        (pin (num 34) (name VSA) (type power_in))
        (pin (num 35) (name VSA) (type power_in))
        (pin (num 36) (name ~) (type NotConnected))
        (pin (num 37) (name ~) (type NotConnected))
        (pin (num 38) (name OUT2A) (type output))
        (pin (num 39) (name OUT2A) (type output))
        (pin (num 40) (name VCP) (type power_in))
        (pin (num 41) (name ENA) (type output))
        (pin (num 42) (name PROGCLA) (type power_in))
        (pin (num 43) (name IN1A) (type output))
        (pin (num 44) (name IN2A) (type output))
        (pin (num 45) (name SENSEA) (type power_in))
        (pin (num 46) (name SENSEA) (type power_in))
        (pin (num 47) (name ~) (type NotConnected))
        (pin (num 48) (name OCDA) (type power_in))
        (pin (num 49) (name GND) (type power_in))))
    (libpart (lib stmbl) (part Led_Small)
      (footprints
        (fp CP*)
        (fp SM*))
      (fields
        (field (name Reference) D)
        (field (name Value) Led_Small))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib stmbl) (part MCP16331)
      (fields
        (field (name Reference) U)
        (field (name Value) MCP16331))
      (pins
        (pin (num 1) (name BOOST) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name FB) (type input))
        (pin (num 4) (name EN) (type input))
        (pin (num 5) (name VIN) (type power_in))
        (pin (num 6) (name SW) (type openEm))))
    (libpart (lib stmbl) (part MIC55)
      (description "300mA LDO")
      (footprints
        (fp SOT-23*))
      (fields
        (field (name Reference) U)
        (field (name Value) MIC55)
        (field (name Footprint) stmbl:SOT-23-5))
      (pins
        (pin (num 1) (name VIN) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name EN) (type input))
        (pin (num 5) (name VOUT) (type power_out))))
    (libpart (lib device) (part Q_NJFET_GSD)
      (description "Transistor N-JFET (general)")
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NJFET_GSD))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib stmbl) (part R)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib interface) (part SP3481CN)
      (aliases
        (alias MAX3072E)
        (alias MAX3075E)
        (alias MAX3078E)
        (alias SP3481EN)
        (alias SP3485CN)
        (alias SP3485EN))
      (description "3.3V Low Power Half-Duplex RS-485 Transceiver 10Mbps, SO8")
      (docs http://www.icbase.com/pdf/SPX/SPX00480106.pdf)
      (footprints
        (fp SOIC*3.9x4.9mm*Pitch1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) SP3481CN)
        (field (name Footprint) Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm))
      (pins
        (pin (num 1) (name RO) (type output))
        (pin (num 2) (name ~RE~) (type input))
        (pin (num 3) (name DE) (type input))
        (pin (num 4) (name DI) (type input))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name A) (type BiDi))
        (pin (num 7) (name B) (type BiDi))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib stmbl) (part STM32F303CBTx)
      (aliases
        (alias STM32F303CCTx))
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F303CBTx)
        (field (name Footprint) LQFP48))
      (pins
        (pin (num 1) (name VBAT) (type power_in))
        (pin (num 2) (name PC13) (type BiDi))
        (pin (num 3) (name PC14) (type BiDi))
        (pin (num 4) (name PC15) (type BiDi))
        (pin (num 5) (name PF0) (type input))
        (pin (num 6) (name PF1) (type input))
        (pin (num 7) (name NRST) (type input))
        (pin (num 8) (name VSSA) (type power_in))
        (pin (num 9) (name VDDA) (type power_in))
        (pin (num 10) (name PA0) (type BiDi))
        (pin (num 11) (name PA1) (type BiDi))
        (pin (num 12) (name PA2) (type BiDi))
        (pin (num 13) (name PA3) (type BiDi))
        (pin (num 14) (name PA4) (type BiDi))
        (pin (num 15) (name PA5) (type BiDi))
        (pin (num 16) (name PA6) (type BiDi))
        (pin (num 17) (name PA7) (type BiDi))
        (pin (num 18) (name PB0) (type BiDi))
        (pin (num 19) (name PB1) (type BiDi))
        (pin (num 20) (name PB2) (type BiDi))
        (pin (num 21) (name PB10) (type BiDi))
        (pin (num 22) (name PB11) (type BiDi))
        (pin (num 23) (name VSS) (type power_in))
        (pin (num 24) (name VDD) (type power_in))
        (pin (num 25) (name PB12) (type BiDi))
        (pin (num 26) (name PB13) (type BiDi))
        (pin (num 27) (name PB14) (type BiDi))
        (pin (num 28) (name PB15) (type BiDi))
        (pin (num 29) (name PA8) (type BiDi))
        (pin (num 30) (name PA9) (type BiDi))
        (pin (num 31) (name PA10) (type BiDi))
        (pin (num 32) (name PA11) (type BiDi))
        (pin (num 33) (name PA12) (type BiDi))
        (pin (num 34) (name PA13) (type BiDi))
        (pin (num 35) (name VSS) (type power_in))
        (pin (num 36) (name VDD) (type power_in))
        (pin (num 37) (name PA14) (type BiDi))
        (pin (num 38) (name PA15) (type BiDi))
        (pin (num 39) (name PB3) (type BiDi))
        (pin (num 40) (name PB4) (type BiDi))
        (pin (num 41) (name PB5) (type BiDi))
        (pin (num 42) (name PB6) (type BiDi))
        (pin (num 43) (name PB7) (type BiDi))
        (pin (num 44) (name BOOT0) (type input))
        (pin (num 45) (name PB8) (type BiDi))
        (pin (num 46) (name PB9) (type BiDi))
        (pin (num 47) (name VSS) (type power_in))
        (pin (num 48) (name VDD) (type power_in))))
    (libpart (lib stmbl) (part TLE5012)
      (fields
        (field (name Reference) U)
        (field (name Value) TLE5012))
      (pins
        (pin (num 1) (name CLK) (type input))
        (pin (num 2) (name SCK) (type input))
        (pin (num 3) (name CSQ) (type input))
        (pin (num 4) (name DATA) (type BiDi))
        (pin (num 5) (name IFA) (type output))
        (pin (num 6) (name VCC) (type power_in))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name IFB) (type output))))
    (libpart (lib device) (part Thermistor_NTC)
      (description "temperature dependent resistor, negative temperature coefficient (NTC)")
      (footprints
        (fp *NTC*)
        (fp *Thermistor*)
        (fp PIN?ARRAY*)
        (fp bornier*)
        (fp *Terminal?Block*))
      (fields
        (field (name Reference) TH)
        (field (name Value) Thermistor_NTC))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib stmbl) (part USBLC6-4SC6)
      (fields
        (field (name Reference) U)
        (field (name Value) USBLC6-4SC6)
        (field (name Description) "TRANSIENT VOLTAGE SUPPRESSOR"))
      (pins
        (pin (num 1) (name I/O1) (type unspc))
        (pin (num 2) (name GND) (type unspc))
        (pin (num 3) (name I/O2) (type unspc))
        (pin (num 4) (name I/O3) (type unspc))
        (pin (num 5) (name VBUS) (type unspc))
        (pin (num 6) (name I/O4) (type unspc))))
    (libpart (lib stmbl) (part USB_OTG)
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) P)
        (field (name Value) USB_OTG))
      (pins
        (pin (num 1) (name VCC) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name ID) (type power_in))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name shield) (type passive))))
    (libpart (lib stmbl) (part testpoint)
      (fields
        (field (name Reference) T)
        (field (name Value) testpoint))
      (pins
        (pin (num 1) (name ~) (type BiDi)))))
  (libraries
    (library (logical conn)
      (uri "/Library/Application Support/kicad/library/conn.lib"))
    (library (logical device)
      (uri "/Library/Application Support/kicad/library/device.lib"))
    (library (logical interface)
      (uri "/Library/Application Support/kicad/library/interface.lib"))
    (library (logical stmbl)
      (uri /Users/crinq/Documents/sandbox/stmbl/hw/kicad/lib/stmbl.lib)))
  (nets
    (net (code 1) (name /SHUNT_A)
      (node (ref R46) (pin 2))
      (node (ref R49) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref U3) (pin 18)))
    (net (code 2) (name /SHUNT_B)
      (node (ref C34) (pin 2))
      (node (ref R47) (pin 2))
      (node (ref R50) (pin 2))
      (node (ref U3) (pin 22)))
    (net (code 3) (name /SHUNT_LOW)
      (node (ref R48) (pin 2))
      (node (ref U3) (pin 17))
      (node (ref R51) (pin 2))
      (node (ref C35) (pin 2)))
    (net (code 4) (name /cmd/A0)
      (node (ref U9) (pin 6))
      (node (ref R28) (pin 1))
      (node (ref R38) (pin 2))
      (node (ref R27) (pin 2))
      (node (ref P5) (pin 4)))
    (net (code 5) (name /cmd/B0)
      (node (ref R28) (pin 2))
      (node (ref R29) (pin 1))
      (node (ref P5) (pin 5))
      (node (ref U9) (pin 7))
      (node (ref R33) (pin 2)))
    (net (code 6) (name /cmd/A1)
      (node (ref P5) (pin 2))
      (node (ref R42) (pin 2))
      (node (ref U8) (pin 6))
      (node (ref R9) (pin 2))
      (node (ref R10) (pin 1)))
    (net (code 7) (name /cmd/B1)
      (node (ref R41) (pin 2))
      (node (ref P5) (pin 3))
      (node (ref U8) (pin 7))
      (node (ref R10) (pin 2))
      (node (ref R11) (pin 1)))
    (net (code 8) (name /DCLINK)
      (node (ref C16) (pin 1))
      (node (ref U3) (pin 10))
      (node (ref R17) (pin 1))
      (node (ref R16) (pin 2)))
    (net (code 9) (name /BEMF_1A)
      (node (ref U3) (pin 13))
      (node (ref R23) (pin 2))
      (node (ref R24) (pin 1))
      (node (ref C19) (pin 1)))
    (net (code 10) (name /BEMF_2A)
      (node (ref U3) (pin 14))
      (node (ref C18) (pin 1))
      (node (ref R19) (pin 2))
      (node (ref R20) (pin 1)))
    (net (code 11) (name /TEMP)
      (node (ref R55) (pin 1))
      (node (ref U3) (pin 11))
      (node (ref TH1) (pin 1)))
    (net (code 12) (name /ENA)
      (node (ref R13) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref U3) (pin 28)))
    (net (code 13) (name /ENB)
      (node (ref R7) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref U3) (pin 31)))
    (net (code 14) (name /IN1A)
      (node (ref U3) (pin 29))
      (node (ref U2) (pin 43)))
    (net (code 15) (name /IN2A)
      (node (ref U3) (pin 26))
      (node (ref U2) (pin 44)))
    (net (code 16) (name /IN1B)
      (node (ref U3) (pin 30))
      (node (ref U2) (pin 17)))
    (net (code 17) (name /IN2B)
      (node (ref U3) (pin 27))
      (node (ref U2) (pin 18)))
    (net (code 18) (name /NRST)
      (node (ref U3) (pin 7))
      (node (ref U4) (pin 4))
      (node (ref C4) (pin 1))
      (node (ref P2) (pin 4)))
    (net (code 19) (name /SWDIO)
      (node (ref P2) (pin 3))
      (node (ref U4) (pin 3))
      (node (ref U3) (pin 34)))
    (net (code 20) (name /SWCLK)
      (node (ref U3) (pin 37))
      (node (ref P2) (pin 1))
      (node (ref U4) (pin 1)))
    (net (code 21) (name /SCK)
      (node (ref U3) (pin 39))
      (node (ref U7) (pin 2))
      (node (ref U10) (pin 2)))
    (net (code 22) (name /MOSI)
      (node (ref U10) (pin 4))
      (node (ref U7) (pin 4))
      (node (ref R43) (pin 2)))
    (net (code 23) (name /CSQ)
      (node (ref U10) (pin 3))
      (node (ref U7) (pin 3))
      (node (ref U3) (pin 38)))
    (net (code 24) (name /TX)
      (node (ref U3) (pin 42))
      (node (ref U9) (pin 1))
      (node (ref U9) (pin 4))
      (node (ref R38) (pin 1)))
    (net (code 25) (name /ENTX)
      (node (ref U3) (pin 45))
      (node (ref U9) (pin 3))
      (node (ref U9) (pin 2))
      (node (ref R33) (pin 1))
      (node (ref R30) (pin 1)))
    (net (code 26) (name /ENRX)
      (node (ref U3) (pin 40))
      (node (ref R21) (pin 1))
      (node (ref U8) (pin 2))
      (node (ref U8) (pin 3))
      (node (ref R41) (pin 1)))
    (net (code 27) (name /RX)
      (node (ref U3) (pin 43))
      (node (ref R42) (pin 1))
      (node (ref U8) (pin 4))
      (node (ref U8) (pin 1)))
    (net (code 28) (name /I0)
      (node (ref U1) (pin 1))
      (node (ref C31) (pin 1))
      (node (ref R32) (pin 1))
      (node (ref U3) (pin 12))
      (node (ref R31) (pin 2)))
    (net (code 29) (name /I1)
      (node (ref U1) (pin 3))
      (node (ref R36) (pin 2))
      (node (ref R37) (pin 1))
      (node (ref C32) (pin 1))
      (node (ref U3) (pin 15)))
    (net (code 30) (name /O0)
      (node (ref R35) (pin 1))
      (node (ref U3) (pin 21)))
    (net (code 31) (name /O1)
      (node (ref U3) (pin 46))
      (node (ref R40) (pin 1)))
    (net (code 32) (name /IN0)
      (node (ref R31) (pin 1))
      (node (ref J1) (pin 3)))
    (net (code 33) (name /IN1)
      (node (ref R36) (pin 1))
      (node (ref J1) (pin 4)))
    (net (code 34) (name GND)
      (node (ref R34) (pin 2))
      (node (ref Q1) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref R21) (pin 2))
      (node (ref R11) (pin 2))
      (node (ref C11) (pin 1))
      (node (ref C4) (pin 2))
      (node (ref P2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref C10) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref U8) (pin 5))
      (node (ref R37) (pin 2))
      (node (ref U10) (pin 7))
      (node (ref C32) (pin 2))
      (node (ref P1) (pin 5))
      (node (ref J1) (pin 6))
      (node (ref J1) (pin 5))
      (node (ref U10) (pin 1))
      (node (ref P1) (pin 6))
      (node (ref U7) (pin 7))
      (node (ref U7) (pin 1))
      (node (ref C27) (pin 2))
      (node (ref C26) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref U6) (pin 2))
      (node (ref P6) (pin 2))
      (node (ref C39) (pin 2))
      (node (ref C38) (pin 2))
      (node (ref C28) (pin 2))
      (node (ref C21) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref R12) (pin 1))
      (node (ref R8) (pin 2))
      (node (ref R20) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref U9) (pin 5))
      (node (ref R26) (pin 2))
      (node (ref R24) (pin 2))
      (node (ref C19) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref C22) (pin 2))
      (node (ref C25) (pin 2))
      (node (ref C23) (pin 2))
      (node (ref C29) (pin 2))
      (node (ref R17) (pin 2))
      (node (ref R39) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref U5) (pin 2))
      (node (ref Q2) (pin 2))
      (node (ref U3) (pin 8))
      (node (ref R29) (pin 2))
      (node (ref R7) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref P5) (pin 6))
      (node (ref U3) (pin 23))
      (node (ref C20) (pin 2))
      (node (ref P4) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref U3) (pin 44))
      (node (ref U2) (pin 4))
      (node (ref U2) (pin 5))
      (node (ref U2) (pin 6))
      (node (ref U2) (pin 7))
      (node (ref U2) (pin 8))
      (node (ref U2) (pin 9))
      (node (ref U2) (pin 30))
      (node (ref U2) (pin 31))
      (node (ref U2) (pin 12))
      (node (ref U3) (pin 35))
      (node (ref U2) (pin 32))
      (node (ref U2) (pin 42))
      (node (ref U2) (pin 33))
      (node (ref U2) (pin 14))
      (node (ref U2) (pin 24))
      (node (ref U2) (pin 25))
      (node (ref U2) (pin 36))
      (node (ref U3) (pin 47))
      (node (ref U2) (pin 37))
      (node (ref U2) (pin 47))
      (node (ref U2) (pin 28))
      (node (ref C31) (pin 2))
      (node (ref U2) (pin 19))
      (node (ref U2) (pin 29))
      (node (ref R32) (pin 2))
      (node (ref U2) (pin 49))
      (node (ref R51) (pin 1))
      (node (ref R30) (pin 2))
      (node (ref U1) (pin 2))
      (node (ref C36) (pin 2))
      (node (ref C6) (pin 1))
      (node (ref C34) (pin 1))
      (node (ref C35) (pin 1))
      (node (ref U4) (pin 2))
      (node (ref C37) (pin 2))
      (node (ref TH1) (pin 2)))
    (net (code 35) (name +5V)
      (node (ref L3) (pin 2))
      (node (ref JP2) (pin 1))
      (node (ref D12) (pin 2))
      (node (ref P5) (pin 1))
      (node (ref C21) (pin 1))
      (node (ref C28) (pin 1))
      (node (ref U6) (pin 3))
      (node (ref U6) (pin 1))
      (node (ref C23) (pin 1))
      (node (ref C17) (pin 1))
      (node (ref L2) (pin 2))
      (node (ref R25) (pin 1))
      (node (ref D2) (pin 2))
      (node (ref J1) (pin 1))
      (node (ref J1) (pin 2)))
    (net (code 36) (name /OUT0)
      (node (ref J1) (pin 7))
      (node (ref Q1) (pin 3))
      (node (ref D4) (pin 2)))
    (net (code 37) (name /OUT1)
      (node (ref J1) (pin 8))
      (node (ref Q2) (pin 3))
      (node (ref D6) (pin 2)))
    (net (code 38) (name VPP)
      (node (ref P4) (pin 1))
      (node (ref C20) (pin 1))
      (node (ref D4) (pin 1))
      (node (ref C26) (pin 1))
      (node (ref C15) (pin 1))
      (node (ref R15) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref P6) (pin 1))
      (node (ref U5) (pin 5))
      (node (ref U2) (pin 34))
      (node (ref C33) (pin 2))
      (node (ref U2) (pin 26))
      (node (ref C22) (pin 1))
      (node (ref U2) (pin 27))
      (node (ref J1) (pin 10))
      (node (ref J1) (pin 9))
      (node (ref U2) (pin 35))
      (node (ref C12) (pin 1))
      (node (ref D6) (pin 1))
      (node (ref D10) (pin 2))
      (node (ref C5) (pin 2)))
    (net (code 39) (name "Net-(R43-Pad1)")
      (node (ref R43) (pin 1))
      (node (ref U3) (pin 41)))
    (net (code 40) (name /f3/USB_EN)
      (node (ref U4) (pin 6))
      (node (ref R3) (pin 2))
      (node (ref U3) (pin 20)))
    (net (code 41) (name /f3/USB-)
      (node (ref U3) (pin 32))
      (node (ref R4) (pin 1))
      (node (ref U1) (pin 6)))
    (net (code 42) (name /f3/USB+)
      (node (ref R5) (pin 1))
      (node (ref U1) (pin 4))
      (node (ref U3) (pin 33)))
    (net (code 43) (name /f3/LED2)
      (node (ref R54) (pin 2))
      (node (ref U3) (pin 4)))
    (net (code 44) (name /f3/LED1)
      (node (ref R53) (pin 2))
      (node (ref U3) (pin 3)))
    (net (code 45) (name /f3/LED0)
      (node (ref U3) (pin 2))
      (node (ref R52) (pin 2)))
    (net (code 46) (name "Net-(T1-Pad1)")
      (node (ref U3) (pin 19))
      (node (ref T1) (pin 1)))
    (net (code 47) (name "Net-(T2-Pad1)")
      (node (ref U3) (pin 25))
      (node (ref T2) (pin 1)))
    (net (code 48) (name "Net-(T3-Pad1)")
      (node (ref T3) (pin 1))
      (node (ref U3) (pin 16)))
    (net (code 49) (name "Net-(D7-Pad1)")
      (node (ref R52) (pin 1))
      (node (ref D7) (pin 1)))
    (net (code 50) (name "Net-(D8-Pad1)")
      (node (ref R53) (pin 1))
      (node (ref D8) (pin 1)))
    (net (code 51) (name "Net-(D9-Pad1)")
      (node (ref D9) (pin 1))
      (node (ref R54) (pin 1)))
    (net (code 52) (name "Net-(P1-Pad4)")
      (node (ref P1) (pin 4)))
    (net (code 53) (name "Net-(P1-Pad1)")
      (node (ref P1) (pin 1)))
    (net (code 54) (name "Net-(R2-Pad1)")
      (node (ref U3) (pin 6))
      (node (ref R2) (pin 1)))
    (net (code 55) (name "Net-(P1-Pad3)")
      (node (ref R5) (pin 2))
      (node (ref P1) (pin 3))
      (node (ref R3) (pin 1)))
    (net (code 56) (name "Net-(P1-Pad2)")
      (node (ref R4) (pin 2))
      (node (ref P1) (pin 2)))
    (net (code 57) (name "Net-(C10-Pad2)")
      (node (ref L1) (pin 1))
      (node (ref C10) (pin 2))
      (node (ref U3) (pin 9)))
    (net (code 58) (name +3V3)
      (node (ref JP2) (pin 3))
      (node (ref D9) (pin 2))
      (node (ref D8) (pin 2))
      (node (ref D7) (pin 2))
      (node (ref R55) (pin 2))
      (node (ref U3) (pin 48))
      (node (ref U3) (pin 36))
      (node (ref U3) (pin 24))
      (node (ref U6) (pin 5))
      (node (ref U1) (pin 5))
      (node (ref C36) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref R48) (pin 1))
      (node (ref R47) (pin 1))
      (node (ref R46) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref L1) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref U4) (pin 5))
      (node (ref C37) (pin 1))
      (node (ref U3) (pin 1))
      (node (ref C25) (pin 1)))
    (net (code 59) (name "Net-(C3-Pad1)")
      (node (ref R2) (pin 2))
      (node (ref C3) (pin 1))
      (node (ref Y1) (pin 2)))
    (net (code 60) (name "Net-(C2-Pad1)")
      (node (ref C2) (pin 1))
      (node (ref Y1) (pin 1))
      (node (ref U3) (pin 5)))
    (net (code 61) (name "Net-(C30-Pad1)")
      (node (ref U2) (pin 40))
      (node (ref C30) (pin 1)))
    (net (code 62) (name "Net-(C30-Pad2)")
      (node (ref C30) (pin 2))
      (node (ref R56) (pin 2)))
    (net (code 63) (name "Net-(D10-Pad1)")
      (node (ref R56) (pin 1))
      (node (ref D10) (pin 1))
      (node (ref D11) (pin 2)))
    (net (code 64) (name "Net-(C33-Pad1)")
      (node (ref C33) (pin 1))
      (node (ref U2) (pin 21))
      (node (ref C5) (pin 1))
      (node (ref D11) (pin 1)))
    (net (code 65) (name "Net-(R12-Pad2)")
      (node (ref R50) (pin 1))
      (node (ref R12) (pin 2))
      (node (ref U2) (pin 16))
      (node (ref U2) (pin 15)))
    (net (code 66) (name "Net-(R49-Pad1)")
      (node (ref U2) (pin 45))
      (node (ref U2) (pin 46))
      (node (ref R49) (pin 1))
      (node (ref R8) (pin 1)))
    (net (code 67) (name "Net-(R18-Pad2)")
      (node (ref R19) (pin 1))
      (node (ref R18) (pin 2)))
    (net (code 68) (name "Net-(R22-Pad2)")
      (node (ref R22) (pin 2))
      (node (ref R23) (pin 1)))
    (net (code 69) (name "Net-(R15-Pad2)")
      (node (ref R16) (pin 1))
      (node (ref R15) (pin 2)))
    (net (code 70) (name "Net-(C39-Pad1)")
      (node (ref U2) (pin 13))
      (node (ref R14) (pin 1))
      (node (ref U2) (pin 20))
      (node (ref C39) (pin 1)))
    (net (code 71) (name "Net-(C38-Pad1)")
      (node (ref U2) (pin 41))
      (node (ref R13) (pin 1))
      (node (ref U2) (pin 48))
      (node (ref C38) (pin 1)))
    (net (code 72) (name "Net-(P3-Pad4)")
      (node (ref P3) (pin 4))
      (node (ref U2) (pin 22))
      (node (ref U2) (pin 23)))
    (net (code 73) (name "Net-(P3-Pad3)")
      (node (ref U2) (pin 10))
      (node (ref U2) (pin 11))
      (node (ref P3) (pin 3)))
    (net (code 74) (name "Net-(P3-Pad1)")
      (node (ref U2) (pin 38))
      (node (ref U2) (pin 39))
      (node (ref R22) (pin 1))
      (node (ref P3) (pin 1)))
    (net (code 75) (name "Net-(P3-Pad2)")
      (node (ref U2) (pin 2))
      (node (ref U2) (pin 3))
      (node (ref R18) (pin 1))
      (node (ref P3) (pin 2)))
    (net (code 76) (name "Net-(R25-Pad2)")
      (node (ref U5) (pin 3))
      (node (ref R25) (pin 2))
      (node (ref R26) (pin 1)))
    (net (code 77) (name "Net-(U5-Pad4)")
      (node (ref U5) (pin 4)))
    (net (code 78) (name "Net-(C24-Pad1)")
      (node (ref U5) (pin 1))
      (node (ref C24) (pin 1))
      (node (ref D2) (pin 1)))
    (net (code 79) (name "Net-(C24-Pad2)")
      (node (ref D1) (pin 1))
      (node (ref U5) (pin 6))
      (node (ref L3) (pin 1))
      (node (ref C24) (pin 2)))
    (net (code 80) (name "Net-(D12-Pad1)")
      (node (ref D12) (pin 1))
      (node (ref R1) (pin 1)))
    (net (code 81) (name "Net-(U7-Pad5)")
      (node (ref U7) (pin 5)))
    (net (code 82) (name "Net-(U7-Pad8)")
      (node (ref U7) (pin 8)))
    (net (code 83) (name "Net-(U10-Pad5)")
      (node (ref U10) (pin 5)))
    (net (code 84) (name "Net-(C27-Pad1)")
      (node (ref U10) (pin 6))
      (node (ref JP2) (pin 2))
      (node (ref C27) (pin 1))
      (node (ref U7) (pin 6)))
    (net (code 85) (name "Net-(U10-Pad8)")
      (node (ref U10) (pin 8)))
    (net (code 86) (name "Net-(C13-Pad1)")
      (node (ref U9) (pin 8))
      (node (ref C29) (pin 1))
      (node (ref L2) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref U8) (pin 8))
      (node (ref R27) (pin 1)))
    (net (code 87) (name "Net-(Q1-Pad1)")
      (node (ref Q1) (pin 1))
      (node (ref R35) (pin 2))
      (node (ref R34) (pin 1)))
    (net (code 88) (name "Net-(Q2-Pad1)")
      (node (ref Q2) (pin 1))
      (node (ref R40) (pin 2))
      (node (ref R39) (pin 1)))))