(export (version D)
  (design
    (source rectifier.sch)
    (date "Do 14 Jan 2016 18:16:13 CET")
    (tool "Eeschema (2016-01-09 BZR 6434, Git 5e36c48)-product")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source rectifier.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref D3)
      (value BRIDGE)
      (footprint bridge:dfb_bridge)
      (libsource (lib device) (part BRIDGE))
      (sheetpath (names /) (tstamps /))
      (tstamp 56262529))
    (comp (ref C1)
      (value CP1)
      (footprint Capacitors_ThroughHole:C_Radial_D35_L51_P10)
      (libsource (lib device) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 562625AE))
    (comp (ref P3)
      (value CONN_2)
      (footprint custom_footprints:WE313-2)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 56262678))
    (comp (ref P2)
      (value CONN_2)
      (footprint custom_footprints:WE313-2)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 562626ED))
    (comp (ref K1)
      (value CONN_3)
      (footprint custom_footprints:WE313-3)
      (libsource (lib conn) (part CONN_3))
      (sheetpath (names /) (tstamps /))
      (tstamp 562627B8))
    (comp (ref F1)
      (value FUSE)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_SemiClosed_Casing10x25mm)
      (libsource (lib device) (part FUSE))
      (sheetpath (names /) (tstamps /))
      (tstamp 5626282B))
    (comp (ref R2)
      (value R)
      (footprint Resistors_ThroughHole:Resistor_Vertical_RM7.5mm)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56262BA3))
    (comp (ref D2)
      (value DIODE)
      (footprint Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /) (tstamps /))
      (tstamp 56262D54))
    (comp (ref D1)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 56262E24))
    (comp (ref R1)
      (value R)
      (footprint Resistors_ThroughHole:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56263013))
    (comp (ref P1)
      (value CONN_2)
      (footprint custom_footprints:WE313-2)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 5626358D))
    (comp (ref P4)
      (value CONN_2)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 56266A2B))
    (comp (ref R3)
      (value R)
      (footprint Resistors_ThroughHole:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5626609F))
    (comp (ref P5)
      (value CONN_1)
      (footprint Wire_Pads:SolderWirePad_single_2-5mmDrill)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 56267627))
    (comp (ref RL2)
      (value FINDER-40.52)
      (footprint Relays_ThroughHole:Relay_DPDT_Schrack-RT2_RM5mm)
      (libsource (lib relays) (part FINDER-40.52))
      (sheetpath (names /) (tstamps /))
      (tstamp 56268E4F))
    (comp (ref RL1)
      (value FINDER-40.52)
      (footprint Relays_ThroughHole:Relay_DPDT_Schrack-RT2_RM5mm)
      (libsource (lib relays) (part FINDER-40.52))
      (sheetpath (names /) (tstamps /))
      (tstamp 562691A0)))
  (libparts
    (libpart (lib device) (part BRIDGE)
      (description "Pont de Diodes")
      (fields
        (field (name Reference) D)
        (field (name Value) BRIDGE))
      (pins
        (pin (num 1) (name -) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name +) (type input))
        (pin (num 4) (name ~) (type input))))
    (libpart (lib conn) (part CONN_1)
      (description "1 pin")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_1))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib conn) (part CONN_2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib conn) (part CONN_3)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) K)
        (field (name Value) CONN_3))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib device) (part CP1)
      (description "Condensateur polarise")
      (footprints
        (fp CP*)
        (fp SM*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part DIODE)
      (description "Diode simple")
      (footprints
        (fp D?)
        (fp S*))
      (fields
        (field (name Reference) D)
        (field (name Value) DIODE))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib relays) (part FINDER-40.52)
      (aliases
        (alias FINDER-41.52)
        (alias FINDER-44.52)
        (alias FINDER-44.62)
        (alias FINDER-30.22)
        (alias RSM822)
        (alias RM84))
      (description "FINDER 40.52, Dual Pole Relay, 5mm Pitch, 8A")
      (docs http://gfinder.findernet.com//assets/Series/5/S40EN.pdf)
      (fields
        (field (name Reference) RL)
        (field (name Value) FINDER-40.52))
      (pins
        (pin (num 11) (name ~) (type passive))
        (pin (num 12) (name ~) (type passive))
        (pin (num 14) (name ~) (type passive))
        (pin (num 21) (name ~) (type passive))
        (pin (num 22) (name ~) (type passive))
        (pin (num 24) (name ~) (type passive))
        (pin (num A1) (name ~) (type passive))
        (pin (num A2) (name ~) (type passive))))
    (libpart (lib device) (part FUSE)
      (fields
        (field (name Reference) F)
        (field (name Value) FUSE))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical relays)
      (uri /usr/share/kicad/library/relays.lib)))
  (nets
    (net (code 1) (name PE)
      (node (ref K1) (pin 1))
      (node (ref P5) (pin 1)))
    (net (code 2) (name DC+)
      (node (ref P3) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref D3) (pin 3))
      (node (ref R3) (pin 1)))
    (net (code 3) (name DC-)
      (node (ref C1) (pin 2))
      (node (ref D3) (pin 1))
      (node (ref R3) (pin 2))
      (node (ref P3) (pin 2)))
    (net (code 4) (name "Net-(P1-Pad1)")
      (node (ref P1) (pin 1))
      (node (ref P2) (pin 2)))
    (net (code 5) (name Neutral)
      (node (ref RL2) (pin 21))
      (node (ref K1) (pin 3))
      (node (ref RL1) (pin A2)))
    (net (code 6) (name "Net-(RL1-Pad22)")
      (node (ref RL1) (pin 22)))
    (net (code 7) (name "Net-(RL1-Pad12)")
      (node (ref RL1) (pin 12)))
    (net (code 8) (name "Net-(RL2-Pad22)")
      (node (ref RL2) (pin 22)))
    (net (code 9) (name "Net-(RL2-Pad12)")
      (node (ref RL2) (pin 12)))
    (net (code 10) (name "Net-(D1-Pad2)")
      (node (ref R1) (pin 1))
      (node (ref D1) (pin 2)))
    (net (code 11) (name "Net-(D2-Pad1)")
      (node (ref R1) (pin 2))
      (node (ref P4) (pin 2))
      (node (ref D2) (pin 1))
      (node (ref RL2) (pin A2))
      (node (ref P2) (pin 1)))
    (net (code 12) (name AC_switched)
      (node (ref R2) (pin 2))
      (node (ref RL1) (pin 24))
      (node (ref RL1) (pin 14))
      (node (ref RL2) (pin 14)))
    (net (code 13) (name AC_fused)
      (node (ref F1) (pin 2))
      (node (ref RL2) (pin 11)))
    (net (code 14) (name "Net-(F1-Pad1)")
      (node (ref F1) (pin 1))
      (node (ref K1) (pin 2)))
    (net (code 15) (name AC_ntc)
      (node (ref R2) (pin 1))
      (node (ref D3) (pin 4))
      (node (ref RL1) (pin A1))
      (node (ref RL1) (pin 21))
      (node (ref RL1) (pin 11)))
    (net (code 16) (name Neutral_Switched)
      (node (ref RL2) (pin 24))
      (node (ref D3) (pin 2)))
    (net (code 17) (name "Net-(D1-Pad1)")
      (node (ref RL2) (pin A1))
      (node (ref D1) (pin 1))
      (node (ref D2) (pin 2))
      (node (ref P4) (pin 1))
      (node (ref P1) (pin 2)))))
