(module stmbl:C_Radial_D26_L45_P10 (layer F.Cu) (tedit 5B2A2802)
  (descr "Radial Electrolytic Capacitor Diameter 26mm x Length 45mm, Pitch 10mm")
  (tags "Electrolytic Capacitor")
  (fp_text reference C22 (at 0 -14.3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.2)))
  )
  (fp_text value 270µ (at 0 14.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 0 0) (end 0 -13.3) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0 0) (end 0 -13.0375) (layer F.SilkS) (width 0.15))
  (fp_arc (start 0 0) (end 12.5 -4.25) (angle 37.55606373) (layer F.SilkS) (width 0.5))
  (pad 2 thru_hole circle (at 5 0) (size 3.3 3.3) (drill 2) (layers *.Cu *.Mask F.SilkS)
    (zone_connect 2))
  (pad 1 thru_hole roundrect (at -5 0) (size 3.3 3.3) (drill 2) (layers *.Cu *.Mask F.SilkS) (roundrect_rratio 0.25))
  (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D26.0mm_P10.00mm_SnapIn.step
    (offset (xyz -5 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
