#!/bin/sh

#
# Please make sure that the following things are OK:
#
#   1. You have installed the arm-elf-tools already.
#   2. Your uClinux distribution has been installed into the directory of '/opt/em85xx/'.
#

rm config.cache config.status -f
PREFIX=/home/hejia/work/crosscp/local
CC=arm-linux-gcc \
CFLAGS="-I/home/hejia/work/crosscp/crosstool/arm-linux/include -I${PREFIX}/include" \
CXXFLAGS="-I/home/hejia/work/crosscp/crosstool/arm-linux/include -I${PREFIX}/include" \
LDFLAGS="-L/home/hejia/work/crosscp/crosstool/arm-linux/lib -L${PREFIX}/lib" \
	./configure --prefix=${PREFIX} \
    --enable-procs \
    --build=i686-linux \
    --host=arm-linux \
    --target=arm-linux \
	--enable-customial
